

|  |  |  |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | **LCD Display Soft Key Definitions** |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | |  |  | | --- | --- | | **Soft Key** | **Definition** | | ABR | Activates Automatic Busy Redial after dialing a busy outside telephone number | | ACB | Activates Automatic Callback after reaching a busy station , CO line, or CO line group | | BUSY | (Busy Override) Sends a call-waiting tone to a busy station | | CONF | Initiates or completes a conference | | EXEC | (Executive Override) Breaks into the conversation of a busy called station | | EXIT | Exits you from a conference; remaining parties are connected | | JOIN | Joins all parties to a conference while on a conference call | | LINE | Adds a CO line to an existing call while in the Conference mode. The LCD prompts you to access a CO line after you press this key | | MESG | Sets a message waiting indication at a busy or unanswered station | | OVRD | Overrides options, busy mode, or overrides Do Not Disturb mode | | PGE | Enables you to enter a Page Group number (01-16) | | RING | Makes a called station ring when making a voice announce call to the station | | RLS | Disconnects a call and returns telephone to the idle state | | RTRN | Terminates a feature operation and to return to a previously displayed state | | SPLT | Enables you to break off from a conference call with another conference call member for a private conversation (split). You can use the Join key to reconnect both of you back into the conference. | | STA. | Adds a station to an existing call while in the conference mode.  The LCD prompts you to dial a station number after you press this key | | TALK | Makes a voice announcement to a called station that is ringing | | TRNS | Initiates or completes a Transfer while on an outside call.  Press once for an immediate or announced transfer, depending on system programming.  Pressing TRNS again completes the transfer. | |     **For additional help please call our office at 249-248-0000 (Michigan) or 239-561-0090 (Florida)** |