Audio Head instructions:

-With a screwdriver, unscrew the lid.

-Screw in the speakers to the amplifier board, positive is on the left and negative is on the right.

+ - + -

-Plug in the power.

-When turned on by the switch, you can either connect to the amplifier by 3.5 mm input or Bluetooth. If connected through Bluetooth look for the tag “Arshon speaker” on your device to find the amp.

-Turn the volume all the way up on the amplifier and control it through the connected device.

- Secure the box to the wall, table, or whatever structure you prefer.