1. GFCI protection is required for all branch circuits or the outlet supplying listed appliances rated 150V to ground and 60A or less?  
     
   Section 210.8(D)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. Outside emergency disconnects for feeders supplied to one-and two-family dwelling units are required to be installed?  
     
   Section 225.41

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. What is the distance from the pool wall that requires all receptacles to be GFCI protected?    
     
   Section 680.22

|  |
| --- |
|  |
| Only select one answer | **A)** | 20 Feet |
| Only select one answer | **B)** | 15 Feet |
| Only select one answer | **C)** | 10 Feet |
| Only select one answer | **D)** | 5 Feet |

1. The 2023 NEC code requires that upon installation of new electrical equipment "Commissioning" be performed before it is put into service.   
     
   Section 700.3(A)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. According to the 2023 NEC Article 90.2 (B) states that you must allow for future expansion when installing new electrical equipment.    
     
   Section 90.2(B)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. The width of the working space (must be kept clear) must be a minimum of 30" but in no case less than the with of the equipment.  
     
   Section 110.26(A)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. You can have two different voltages share the same conduit?   
     
   Section 200.6(D)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. Ground-Fault Circuit Interrupter (GFCI) opens the circuit when the ground-fault current is 6 mA and greater.

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. Any cord-and-plug-connected appliances in the kitchen such as the range receptacle, refrigerator receptacle, disposal receptacle, and microwave receptacles require to be GFCI protected?  
     
   Section 210.8(A)(6)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |

1. GFCI protection is required for all receptacles in a dwelling unit boathouse.  
     
   Section 210.8(A)(9)

|  |
| --- |
|  |
| Only select one answer | **A)** | True |
| Only select one answer | **B)** | False |