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[image: ]1. Clean the build surface  
Wipe your bed with warm water and soap to remove dust and oils. Dry completely.
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2. Saturate applicator 
Use the builtin 30mm or 50mm applicator by pressing down the applicator on the build surface until OMNILAYER adhesive begins to flow out making sure the applicator tip is saturated. 
0[image: ]3. Apply OMNILAYER 
Begin to spread a light thin layer across the print area. A little goes a long way. 
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4. Start your print normally  
The adhesive layer activates as the bed heats, creating strong adhesion for most filaments.
5. Easy part removal  
[image: ]Once the bed cools, parts release with minimal effort — no chiseling or scraping.

[image: ]6. Reapply as needed  
Most coatings last for 20-30 prints. Reapply when adhesion begins to fade.
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