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1. Cool and clean the nozzle   
Make sure the nozzle is cool, then remove any leftover filament or residue.

2. Shake and uncap  
Gently shake the OMNISHIELD applicator, then remove the cap.

03. Brush it on  
Use the microfiber brush tip to lightly coat the outside of the nozzle in thin, even strokes. Avoid the tip opening.

4. Let it dry    
The coating dries white. Give it a few minutes to set fully.

5. Print normally    
OMNISHIELD is rated for 0-320°C and works with all thermoplastics.

6. Reapply as needed    
Thin coats work best. Reapply when you notice filament starting to cling again.
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