**Required Tool List**

**for HRC, HRB, HRBA, HRR, HRP, HRU.**

* Air Hose (3/8, 50 ft. with type M fittings)
* Electrical Cord (50ft.)
* Flash Light
* Safety Glasses
* Leather Work Boots
* Dark Cutting Glasses
* Screwdriver Set (Phillips and Straight blade)
* ½” Drive Socket Set (Standard and Metric)
* 3/8” Drive Socket Set (Standard and Metric)
* ¼” Socket Set
* Combination hand wrenches (Standard and Metric)
* Allen Wrench Set (Standard and Metric)
* Ball Peen Hammer
* Small Sledge Hammer (3 lb)
* Welding Helmet (Auto Darkening)
* Welding Gloves (thin)
* Mechanics Gloves
* Welding Sleeve
* Plier Set
* Punch & Chisel Set
* Die Grinder
* Cut-Off Saw
* Combination Square
* Tape Measure
* High Crown Body Hammer
* Low Crown Body Hammer
* Heel Dolly
* General Propose Body Hammer
* Center Punch
* Scratch Awl or Scribe
* Air Blower
* Tin Snips (Left & Right) (Red & Green Handle)
* Vise Grips
* Drill Bit Set
* Scraper or putty knife
* Long Wet Sanding Board
* 3” or 5” Air Grinder / Sander
* 3M Paint Mask with replaceable filters
* Dual Action Orbital Sander
* Assortment of Durablock Sanding Blocks
* Paint Suit
* Air File (Pneumatic Long Board)
* DVOM Multi Meter
* 12 Volt Test Light
* Compression Gauge Set
* Vernier Calipers (Dial or Digital)
* 10” Shears for Upholstery
* Staple Remover
* Tucking Tools
* Tack Hammer
* Metal Ruler 36”
* 3/8’s Cordless Drill