Nudge Bar Installation Instructions

-Installation should take approximately 45 minutes.

1- Remove the plastic covers that are located directly in front of the recovery point locations in the front lower facia.

2- insert the nudge bar mounts/recovery points in a way that the large 3/4” holes are facing upward and outward.

3- Apply a lock washer and flat washer on the M10 bolts (black, grade 12.9). Use these bolts to mount the recovery point/nudge mounts to the frame of the GC. The holes in the frame are threaded, and can be accessed from underneath the vehicle or through the front access openings. Leave these bolts finger tight at this time.

4- Apply the nudge bar using the 3/4” bolts (yellow, grade 8). The nudge bar does not have a front or back, simply choose which side looks best to you. Leave these bolts finger tight at this time.

5- Now that everything is in place, you can shift the nudge a bit right or left to center it. Once centered to your liking, tighten the M10 bolts (black), then the 3/4” (yellow) bolts.

6- Lastly, apply the recovery shackles. Your nudge bar installation is now complete and ready for use! Enjoy!