Monkey Panel Installation Instructions

1. Remove factory grab handles using a star bit. You’ll need to pop off the hardware tab covers, and remove the 2 star bolts on each side. Save these bolts, as they will be reused. 
2. Insert the 4 pipe spacers into the headliner openings. Allow the headliner to retain the spacers, they do not need to be pushed all the way in at this time. 
3. locate the bent mount brackets. Use the above pics to determine mount orientation. Using the factory star bolts, put the handle D brackets on the bolts, and insert the bolts on to the mount brackets. 
4. Apply the mount brackets to the factory grab handle locations by inserting the bolts through the steel pipe spacers. Start the bolts, but do not tighten at this time
5. Locate the Monkey panel. Proper orientation is to have the slotted bent portion towards the front, and bent downward. This panel can be mounted on the top side or bottom side of the brackets, depending on personal preference. 
6. Align the mount holes in the Monkey panel with the slots in the mount brackets. Using the supplied hardware, insert the bolts through the bottom, apply a washer and acorn nut on top. Do not tighten at this time.
7. Tighten the 4 factory star bolts that mount the brackets and grab handle D brackets to the factory grab handle locations. Note- be sure to orientate your D brackets in a way that best suits your paracord handles (not supplied).
8.Using an Allen wrench and a 7/16” wrench, tighten down the supplied hardware that attaches the Monkey panel to the mount brackets.
9. Installation is now complete! You can now start to personalize your Monkey panel with anything you deem fit!