

|  |  |  |
| --- | --- | --- |
|  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |  |
| --- | --- | --- |
| **LCD Display Soft Key Definitions** |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |  |
| --- | --- |
| **Soft Key** | **Definition** |
| ABR | Activates Automatic Busy Redial after dialing a busy outside telephone number |
| ACB | Activates Automatic Callback after reaching a busy station , CO line, or CO line group |
| BUSY | (Busy Override) Sends a call-waiting tone to a busy station |
| CONF | Initiates or completes a conference |
| EXEC | (Executive Override) Breaks into the conversation of a busy called station |
| EXIT | Exits you from a conference; remaining parties are connected |
| JOIN | Joins all parties to a conference while on a conference call |
| LINE | Adds a CO line to an existing call while in the Conference mode. The LCD prompts you to access a CO line after you press this key |
| MESG | Sets a message waiting indication at a busy or unanswered station |
| OVRD | Overrides options, busy mode, or overrides Do Not Disturb mode |
| PGE | Enables you to enter a Page Group number (01-16) |
| RING | Makes a called station ring when making a voice announce call to the station |
| RLS | Disconnects a call and returns telephone to the idle state |
| RTRN | Terminates a feature operation and to return to a previously displayed state |
| SPLT | Enables you to break off from a conference call with another conference call member for a private conversation (split). You can use the Join key to reconnect both of you back into the conference.  |
| STA. | Adds a station to an existing call while in the conference mode.  The LCD prompts you to dial a station number after you press this key |
| TALK | Makes a voice announcement to a called station that is ringing |
| TRNS | Initiates or completes a Transfer while on an outside call.  Press once for an immediate or announced transfer, depending on system programming.  Pressing TRNS again completes the transfer. |

 |

**For additional help please call our office at 249-248-0000 (Michigan) or 239-561-0090 (Florida)** |