Logo, company name

Description automatically generated A drawing of a cartoon character

Description automatically generated Icon

Description automatically generated

Administrative Address: Shipping/Returns Address: Canadian Address:

417 Forest St. Ste. 460 2002 Charles Ave. 1771 Robson St. Suite 1175  
Kalamazoo, MI 49001 Kalamazoo, MI 49048 Vancouver, BC V6G1C9  
 Wholesale Division: 855-927-3066 \* Customer Service: 877-755-2334

Thank You for Purchasing our Dry Eraser Board Hanger

A B  C D E

The Back Board “A”, The Top Trim Board “B”, The Shelf “C”, The Coat/Keys Hook “D”, The Dry Eraser “E”.

STEP 1) Assembling the Top Trim Board “B” to the Back Board “A” you will need two 1-1/4” screws, follow the pencil guidelines for placement about 1-1/2” from the top of “A”. **REMEMBER YOU ARE WORKING ON THE BACKSIDE AND PLACING THE TOP BOARD UNDER THE BACK BOARD**.

STEP2) Assembling the Shelf Board “C” to the Back Board “A”, you will need two 1-1/4”, the pencil marks on this is only showing the lower side placement of the shelf board on the back board. The pencil mark is at 2-1/2” from the bottom of the back board. **REMEMBER YOU ARE WORKING FROM THE BACKSIDE AND THE SHELF SHOULD BE ON THE SAME SIDE AS THE TOP BOARD**.

STEP 3) **YOU ARE NOW WORKIING ON THE FRONT SIDE OF THE BACKBOARD** Assembling the Hooks “E” You can place these anywhere you wish below the Shelf Board.

STEP 4) Hanging on the wall, you will need the two 1-5/8” screws for this. It is recommended that you secure it into a stud. It is also recommended **not** to place anything over a half-pound on the shelf unit. This is mainly just a light-weight shelf for one or two small figurines.

A piece of paper with writing on it

Description automatically generated with low confidence 1-1/4” Screws 1-5/8” Screws

STEP 5) Once the wooden Hanger is securely placed on the wall, you will want to open the dry eraser packet and get the double-sided tape out and un-tape one-side of the squares to each corner placement. Make sure the tape does not show from the frontside. Center the dry eraser (left/right) then adjust it where you would like on the wooden hanger then press the dry eraser into place onto the wooden hanger…