2024 Greene County Fair Minivan Rules

1 Heat Only – Simple Bone Stock Build

1. You may move the wire harness to the backside of the motor. Do not move to the inside of the vehicle. Battery must be inside of the vehicle mounted safely and secured.
2. NO CARB SWAPS or distributor swaps. No aftermarket shifters, no aftermarket pedals. Headers are allowed. No motor swaps.
3. Bumpers must remain 100% stock OEM (no welding or reinforcing.) Can hardnose or weld bumper and shocks (no added metal to mount.) You can have 2 strands of #9 wire per side or 2 chains total from bumper to core support to keep bumper from falling off. Do not strengthen the unibody in any way.
4. Body and frame to remain stock. No pre-bending. Anything can be removed but nothing added.
5. Driver’s door welded, vertical seams only. Two chains or 9 wire (2 strands.) 2 spots on other doors, vertical seams only.
6. Hood and tailgate must be held shut 4 spots max with chain or #9 wire (with 2 strands per location) or 3/8 bolt. If using bolts, stamped washers only ½” max. Tailgate may be removed. Hood and trunk must open at inspection.
7. You can have a maximum of 4-point cage that does not extend more than 12” behind seat. Keep it basic. (No down bars.)
8. All cars MUST have a window bar. Chain or 9 wire to keep the hood from coming into the car.
9. Factory fuel tank preferred to stay under vehicle if in front of rear axle. No factory tanks in the back seat. Aftermarket is okay.
10. Suspension must remain completely stock and bounce. No flipping springs or spacers.
11. No AWD. 6-cylinder max engine size.
12. You may run any tire but only allowed small center.
13. Seatbelts must be worn.
14. 4 or 6-cylinder minivans only. (No cars, suvs, trucks, or full-size vans.) No handicap vans.