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DOCUMENTATION REQUIRED FOR  
RE-STUMPING WORKS
BUILDING PERMIT

Please provide the following information as part of your Building Permit Application, which can be lodged via email to info@viccentral.com.au.  

Alternatively, a User Name and Password can be provided upon request to allow online management of your building permit application via the Applicant Login at www.viccentral.com.au


1. Completed Building Permit Application Form (Form 1)

2. Copy of Title.
Other evidence of ownership will be required if names are not listed on the Title (Rates Notice, etc)

3. Home Warranty Insurance (Registered Building Practitioners) – For works over $20,000 plus a copy of the Contract (or an extract of the Contract) between the builder and the owner.

4. Soil Report (If Underpinning Work)

5. Engineers design and certification (If Underpinning Work)

6. Site Plan

7. Stump layout plan (indicating stumps to be replaced).  Any bearers to be replaced must be also indicated, along with the size and spacing.

8. Stump detail, to include stump type and size, sole plate size (if applicable), footing size and depth, ant cap, minimum clearance beneath sub-floor (150 mm), clearance to underneath side of bearer for termite protection (400mm if applicable), bearer and floor joist general location.


	




