**HOW TO CARE FOR YOUR PAINT JOB**

WASH ONLY WITH TURTLE WAX ICE CLEAR – ANY OTHER WAX COULD DAMAGE THE PAINT JOB

USE ONLY A GARDEN HOSE NOZZLE TO WASH; PRESSURE WASHING OR USING A NEEDLE TIP WAND COULD DAMAGE THE PAINT JOB

KEEP THE PAINT JOB COVERED THE BEST YOU CAN WHEN NOT IN USE; DIRECT SUNLIGHT OVER EXTENDED PERIODS OF TIME CAN CAUSE THE PAINT TO FADE AND CAN DAMAGE THE CLEARCOAT

ANY OIL, GASOLINE, BATTERY ACID AND OTHER TYPES OF CHEMICALS CAN DAMAGE YOUR PAINT JOB

WD-40 IS USED TO LOOSEN RUSTED HARDWARE AND IS ALSO A PAINT REMOVER. DO NOT SPRAY ON ANY PAINTED ITEM!!! USE 100% SILICONE LUBRICANT TO PROTECT PARTS FROM WEATHER