Hanging Guidelines

1. Works submitted for inclusion in exhibits must be ready for secure installation if

those works are intended for to be hung on the wall.

2. Framed pieces must be equipped with d-rings attached to the back of the art, and wire

that has the ends taped (if not using coated wire) to prevent injury to the hanging

committee. Saw tooth hangers or Uni-frames are not acceptable.

3. Wires, when stretched to hang the picture, should not come closer than two inches

from the top of the frame. This prevents the hanger from showing when the art is

hung.

4. Because of increased risk of injury from broken glass in very large pieces, Plexiglas

must be used in lieu of glass for any piece larger that 16x20.

5. In general, pieces should not be larger that 40" wide in order to provide maximum

opportunity for VAL members to participate in exhibits. Larger pieces may

be included if the exhibit committee decides that such pieces don't compromise the

integrity of the exhibit.

6. Artwork that is hung may not be over 40lbs in weight,

7. Artworks that are hung should have a clean, gallery-wrapped (1 ½” – 2”) canvas edges or be

framed. We will not accept unframed canvases below 1 ½” in a gallery exhibit.

8. Any piece that the curator considers to present a hanging problem will not be hung.

The Exhibit committee will consult with the artist to discuss alternatives to framing or

presenting the art.

9. When hanging art on the gallery walls nails with hooks are used. Please do NOT

place nails in the indented vertical lines in the gallery walls.

10. Any hardware or tools that do not belong to the MCL Grand should be put back in

the VAL closet.