**Instructions to making your own Angle Guide**

Purchase an 8” x 8” piece of ¼ inch thick Plexiglas (available from glass/crafts/plastic stores). Place this Plexiglas square on top of the template in the following file (#1206), and using a waterproof fine-tip felt pen, or glass etcher, trace these angles. It is a good idea to bevel or sand the outer edges of the Plexiglas until smooth to prevent cutting yourself.