

**10500 LB 466 Hot Farm Rules**

1. Safety first, always!!!
2. Follow the general rules at all times.
3. Maximum 480 cubic inches.
4. Maximum 3”x3” turbo. No reducers.
5. 20.8 max tire.
6. Roll bar/roll cage and seat belts are MANDATORY.
7. NO intercoolers are allowed.
8. Water injection is allowed.
9. Any pump up to p7100.
10. Driver MUST wear at least a fire jacket, gloves, helmet and leather boots. ALL tractors must be equipped with a WORKING fire extinguisher.

 