Date \_\_\_/\_\_\_\_\_/\_\_\_\_\_\_\_ Inspector: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Pull: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Tractor:\_\_\_\_\_\_\_\_\_\_\_\_\_ Driver: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_

The following **6** safety items are mandatory on all tractors to receive a complete inspection for competition.

The absence of any of the following **6** Safety items will result in **Automatic Disqualification**!

Check the following boxes that apply Satisfactory  Unsatisfactory

-Does the tractor have SFI approved clutch? NO Exceptions! Satisfactory  Unsatisfactory

-Does the tractor have a wheelie bar that supports weight of tractor with 5 X 5 pads Satisfactory  Unsatisfactory horizontal to the ground?

-Does the tractor have a roll bar or cage that supports the weight of tractor? Satisfactory  Unsatisfactory

-Does the tractor have SFI Approved Blanket, or 3/8-inch steel -- ½ inch Satisfactory  Unsatisfactory Aluminum X 6” wide bolted to frame covering bell housing?

-Does the tractor have fuel dump valve that is 3-way dump before injection pump, Satisfactory  Unsatisfactory and is it able to be pulled from seat while strapped in?

-Does the tractor have air shut off that is reachable from seat well strapped in and Satisfactory  Unsatisfactory one on the rear of tractor with the ability to hook to sled? (Mandatory check & Test)

**Is the tractor Automatically Disqualified YES  NO**

-------------------------------------------------------------------------------------------------------------------------------------------------------------- --

Satisfactory Unsatisfactory

-Is the tractor equipped with seat belt or have 5-point harness if equipped with Cage?

- Is the tractor equipped with a neutral safety start? (Must not be able to start well in gear)

- Does the tractor have neutral safety light on rear, clear in color? (Unlimited tractors only)

- Is tractor equipped with 3.5 lbs. Fire Extinguisher?

- Is tractor equipped with a dead man’s throttle with 2 return springs?

- Are the breaks in working condition? (Pump breaks and be sure they hold)

-Is exhaust vertical with 2- 3/8 cross bolts?

-Is Side shields .060 steel or .120 aluminum?

- Is firewall .060 steel or .120 aluminum?

-Is tractor free of metal cooling fan blades? (No Metal Blades on fans)

-Does tractor have 3/8” cable or larger, 360 degrees between cylinder 1 and 2 w/ 4 clamps

-Is the wheel hubs steel or heavy clamp style hubs?

- Draw bar has Horizontal pin 3” X 3.75”? (Hole Must be ridged)

- Does the tractor have tie bars with rear end tied to frame rails?

- Is the tractor equipped with wide front-end ski bars? Mandatory (Except Factory Front Ends)

- Does the tractor have a shield or can withhold the balancer from exiting?

- Is the tractor equipped with a 3 X 3 turbo or smaller?

--------------------------------------------------------------------------------------------------------------------------------------------------- -------------

**The above tractor qualifies for competition: YES  NO**

Inspector: I hereby certify the above tractor for competition. Sign: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Driver: I hereby agree with the above Inspection. Sign: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_