|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  | | --- | |  | | **ELECTRIC BUNSEN BURNER, “AVLAB”**  Very useful for heating test tubes, crucibles small flasks, beakers etc.  The heating element is spiraled Nichrome wire enclosed in refractory casing. Works on electricity.   * This is safe compared to the conventional Bunsen Burner * Can be carried anywhere and connect to the power source * No fire hazards since it gives no flame unlike the conventional   Bunsen Burner   * No smoke, clean atmosphere * Works on electricity, no gas required. * Produces radiant heat. | |  | |  | |  | | --- | | electric bunsen burner “avlab” ***Technical Specifications :***   * Stainless steel body * Aluminium base, powder coated * Max. temperature 1000 deg C * Power consumption 350 Watts * Operates on 220 – 240 V single phase A/C * Supplied with built – in energy regulator. * Light weight 1 kg only | |  | | SYARIKAT SAINTIFIK JAYA NO 69 Jalan Penerbit U1/43, Temasya Industrial Park Glenmarie 40150 Shah Alam  Tel : 603- 5569 0758/0759 HP : 018 274 0955 Fax : 603- 5569 0763 Email : info@saintifikjaya.com  Dates and Times | |

<https://sites.google.com/view/syarikatsaintifikjaya>