|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
|  |
| **ELECTRIC BUNSEN BURNER, “AVLAB”**Very useful for heating test tubes, crucibles small flasks, beakers etc.The heating element is spiraled Nichrome wire enclosed in refractory casing. Works on electricity.* This is safe compared to the conventional Bunsen Burner
* Can be carried anywhere and connect to the power source
* No fire hazards since it gives no flame unlike the conventional

Bunsen Burner* No smoke, clean atmosphere
* Works on electricity, no gas required.
* Produces radiant heat.
 |
|  |

 |  |

|  |
| --- |
| electric bunsen burner “avlab”***Technical Specifications :**** Stainless steel body
* Aluminium base, powder coated
* Max. temperature 1000 deg C
* Power consumption 350 Watts
* Operates on 220 – 240 V single phase A/C
* Supplied with built – in energy regulator.
* Light weight 1 kg only
 |
|  |
| SYARIKAT SAINTIFIK JAYANO 69 Jalan Penerbit U1/43,Temasya Industrial Park Glenmarie 40150 Shah AlamTel : 603- 5569 0758/0759HP : 018 274 0955Fax : 603- 5569 0763Email : info@saintifikjaya.comDates and Times |

 |

 <https://sites.google.com/view/syarikatsaintifikjaya>