SyDri Rotary Airer (split pole)

Please un-wrap the parcel carefully.

Place the un-wrapped Airer on a flat surface

Notice the *uncut tie wraps*……turn the Airer until the *uncut ends are facing upwards*.

Carefully cut away all the tie wraps….do not twist the airer.

Remove the ***SPIKE and its handle***.

Remove the ***BOTTOM POLE*** ***B***.

Next….

Looking at the diagrams…go to description (A) and follow through to (D).

So…. untie the cord wrapping around the canopy.

(A) Unfolding the top of the canopy, (B) unfold the sides if the canopy as you do this you will find a couple more tie wraps to cut from the green straps.

(C) Slide the ***BOTTOM POLE*** ***B*** into the ***middle pole*** so B and B are in line, at this point the poles should clip together.

Next diagram.

(D) with the cable ties cut away locate the ***TOP POLE A*** (do not twist the pole) which is located next to the ***middle pole…..***slide the ***TOP POLE A*** upwards towards the top of the unfolded canopy.

Slide the ***TOP POLE A*** into the ***middle pole*** soA and A are in line, at this point the poles should clip together.

At this point place the Airer into the ground spike.



