lOnl Pickup
_   _ _ .    .       OJ cX pnos» wttn ir* oin* pickuO. Vx»en boboln lic/n bonom p'oi«. Piotuo         QoniiY cxjli out mogn«i orxd lavefM ISO o«gi««».
V STANDARD HUMBUCKING OPERATION/ SINGLE CONDUCTOR WIRING
—Boncm View ol Guile*—
Vohxn*	lon«

2. STANDARD .HUMBUCKING OPERATION 4-CONDUCTOR WIRING —Bottom View ol Gultar-
FronJ Pickup

U one pickup ii oui o< pnoie wim mo oir«(
Bocv Pickup	pickuo.teveria ino"6lock"onO"G(e«n"wuet,

3. SPUniNG-WHEN THE PICKUP IS USED BY ITSELF 4-CONDUCTOR WIRING

a. PHASING-WHEN USED WITH ANOTHER PICKUP 4-CONDUCTOR WIRING

HoiOuipui
KolOulDUI

5. SERIES/PARAOEL OR SERIES/SPUT/PARALLEL 4-CONDUCTOR WIRING

6. SERIES/SPLIT/PHASED WITH ITSELF 4-CONDUCTOR WIRING

n/none/on       wiet'po'oiiei OPOI onianlon      wi«t/u>>il'DO>0««i
Poionai
*- sow—

Ouipui 10 coniioii