The process for labels (label supplied by you)

If you wish to place an order, you would need to submit the completed Order Form to sara@oasthouseengineering.co.uk .

Sara would then process your order and you will receive a proforma invoice as confirmation of this.

You would then organise for your labels to be sent to us as soon as possible. When the labels arrive your job will be scheduled onto our warehouse production plan the following week.

When ordering your labels, you will need to give your label producers the following information;

Information needed for label production

Wind information

 Body labels;]jsxl

* Wind #4
* Left side of Copy dispenses first
* Reel Inner Diameter: 76 mm
* Max Reel Outer Diameter: 370 mm
* Interval Min. 3 mm (between label)

 Preferred roll sizes

* 2100
* 2500
* 1750
* 1500

Lead time

Labelled cans are always produced in our warehouse the week after they are received. To ensure the correct can make and type is in stock you must put your order in at least 1 week prior to your labels arriving.

Packaging and shipping

We use external couriers to ship all of our orders. This means there are height restrictions on our deliveries.

330ml cans can be shipped at a maximum height of 15 layers of cans

440ml cans can be shipped at a maximum height of 13 layers of cans

This maximum heights reduce if your order includes Can Ends. This is simply because where possible, we package can ends on the top of pallets.

Order Quantities

There are 351 cans per layer. All order placed have to be in multiples of 351 because we do not ship cans without filling the layer; this is to ensure the best stability during shipping.

You will also see on the bottom of the order form attached that we recommend all customers build in a slight tolerance within their order quantities.