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Standard Operating Procedures for Pilots

Mid Valley Air Park
Aware, Courteous Pilots are Mid Valley’s Best Safety Assurance 
The following procedures are intended to promote a safe and orderly flow of traffic with minimum inconvenience to all pilots. All questions concerning airport operations should be directed to Airport Manager.
Normal Operating Procedures 
Mid Valley Air Park is a privately-owned, public-access air park. Air park operations are conducted at the pilot’s own risk. Exercise caution for uncontrolled Pedestrian and vehicle traffic. Aircraft shall have the right of way over all other traffic and pedestrians.
All pilots are to operate in conformance with the Federal Aviation Regulations and current published procedures. 

Current traffic pattern is Left traffic. 

Pattern altitude is 5800’ MSL. 

The Common Traffic Advisory Frequency (CTAF) is 122.9 MHz. All aircraft, ultralights, and balloons are encouraged to have an operating 2-way radio on board. Standards calls are to be made in the pattern  and before takeoff. 

All aircraft shall use the full length of the runway for takeoffs. No intersection takeoffs are allowed. The overruns for runway 18 and 36 may be used for takeoffs. Landings will be made beyond the threshold markers.

The East-West dirt strip is sporadically used and is inconsistently maintained. Total length is 1400 feet (not all usable due to obstructions). It should be used at the pilot’s own risk. Due to obstructions and short length, takeoffs are strongly discouraged. 
All aircraft using auto-plane drives between the hours of sunset and sunrise shall use adequate and operational landing/taxi and position lighting.
The Pilot Controlled Lights (PCL) for runway 18/36 and the AWOS are activated by keying the transmitter three (3) times on 122.9 MHz. After activation the lights will remain on approximately twelve (12) minutes.
The Rotating Beacon is activated with the runway lights. 
Four (4) clicks on frequency 122.9 will allow you to transmit for a radio check that will be re-transmitted back to you.
Helicopter operations in the air park vicinity should be conducted to stay inside and below normal fixed-wing traffic. 

Ultralight operations shall use normal aircraft traffic patterns and adhere to all air park operating procedures.

Balloon liftoff and landings are not allowed within 200’ of the runway centerline. If balloon landings are unavoidably made near the runway, prompt removal of balloon and equipment shall be made to clear runway for normal use. 

Unmanned Aerial Vehicles (UAVs aka Drones) shall not be flown near the runway-taxiways environment without prior permission from the Airport Manager.
An owner may fuel his/her airplane in a hangar, however no gasoline sales shall be made out of the hangar. The Air Park has an approved and licensed single source vendor for fuel sales.

Only aircraft shall be allowed on the runway, landing area, or taxiways except for maintenance or emergency vehicles.

No aircraft shall use auto plane drives without adequate brakes.

There shall be no parking on auto plane-drives, near the runway, or near taxiways at any time or in any manner that will obstruct aircraft from taxiing.
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