BUILDERS CHECK LIST (pdf)

**Decks:**

Deck clean and dry

Flashing installed

Sub-wall is exposed minimum of 1 foot above the deck surface

Once surface is waterproofed we recommend limiting construction traffic or covering to protect against damage while waiting for finish floor to be installed. We do not warranty our system for use with outdoor carpet.

**Shower pan**:

Drain concreted in place, level and flush with floor and anchored with screws if wood

2”x10” or 2”x12” Blocking installed flush with wall studs around perimeter

Pan is ready for water testing immediately after spray

**Concrete Walls and Insulated Concrete Form (ICF):**

Free of all loose debris, forms and pins

Cured minimum 28 days, under 28 days may require priming at an additional cost

All holes and honeycombing filled

Dry

2-3 feet minimum clearance for accessibility

Walls ready for backfill within 2 hours after spray