Manifest: (this file)
    switch-2.t-manifest.txt

Licences:
    LICENCE.pdf
    HW-LICENCE-v2.pdf

Hardware Documentation:
    switch-v2.t-bill-of-materials.pdf
    switch-v2.t-assembly-notes.pdf
    destest-switch-manual.pdf

3D-Prints (case options and LED standoffs)
    3d-prints/destest-switch-filled-labels.3mf
    3d-prints/destest-switch-no-labels.stl
    3d-prints/destest-switch-recessed-labels.stl
    3d-prints/led-5mm-standoff-5mm.stl

DesTest-Switch release archive:
    rom/destest-switch-v0.3.zip


Notes:
All 3D-prints work best oriented "face-down".  They can be printed vertically but the edges will tend to be rounded.
The "filled-labels" case is designed to be printed using PLA for the main-case and PETG for the label.  This combination
will result in an excellently defined recess for the label (50mm x 30mm).
The "recessed-labels" case also has a recessed label as above but it is just and empty overhang.  You will want to 
adjust your slicer settings to enable a single layer of support for this overhang.
A 16mm M3 machine screw (or self tapping screw) with a countersink head can be used to secure the case-halves together
if you wish.
