|  |  |
| --- | --- |
| **Company/Supplier Name & Order/ Request #** | **Equipment Description (Type/Year/Make)** |
| **Driver/Operator Signature & Contact Phone #** | **Model & License or Serial/ VIN Number** |
| **FIRELINE WATER TENDER** | **FIRELINE BULLDOZER** |
| [ ]  Reflectors – DOT- set of 3 | [ ]  ROPS with sweeps and side / rear screens |
| [ ]  2 Chock blocks – appropriate for tire size[ ]  Minimum 1 quart drinking water/person/hour | [ ]  Belly pans [ ]  Rock guards (Optional)[ ]  Radiator protection |
| [ ]  Flashlight [ ]  Seat belts (Serviceable) | [ ]  Flashlight [ ]  Seat belts (Serviceable) |
| [ ]  Contractor’s identification on equipment items  | [ ]  Lights – 4 front and 2 rear |
| [ ]  Back-up alarm (97 dB minimum) | [ ]  1 - Shovel and 1 - Axe or Pulaski |
| [ ]  Fire Extinguisher (2A10BC min.) Mounted | [ ]  Backup Alarm (97 dB minimum) |
| [ ]  1 - Shovel and 1 - Axe or Pulaski | [ ]  Fire Extinguisher (2A10BC min.) Mounted |
| [ ]  Road Spraying: forward or rear-facing capable | [ ]  Fire Curtains mounted on front, sides & rear |
| [ ]  Radio: Refer to form FC-100R [ ]  If Radio is mounted; external speaker | [ ]  Minimum 1 quart drinking water per person per hour |
| [ ]  200 GPM Pump (minimum), Drafting capable | [ ]  Radio: Refer to form FC-100R |
| [ ]  Backflow protection device | [ ]  Radio headset |
| [ ]  24’ hard suction hose - 2.5” or 3” connections | **TRANSPORT** |
| [ ]  Legal tank capacity  | [ ]  Record of Safety Inspect within past 12 mo. |
| [ ]  Tank baffles | [ ]  Seat belts (Serviceable) |
| [ ]  Certified weight ticket with legal tare load limit by axle/group | [ ]  Fire Extinguisher (2A10BC min) Mounted[ ]  Reflectors DOT-set of three |
| [ ]  1 - 1” combination nozzle w/ 1.5” x 1” reducer | [ ]  Mirrors, Glass, & Lights  |
| [ ]  100’ x 1½” fire hose with nozzle | [ ]  Radio: Refer to form FC-100R |
| [ ]  2 – 1½” gated male NH discharge outlets or gated wye | [ ]  # Axles # Tires . |
| [ ]  1.5” fire hose clamp and hydrant wrench | **FALLER** |
| [ ]  1- 25’ x 2.5” min. hydrant fill hose with NH fittings | [ ]  Chaps [ ]  Falling Axe & Wedges[ ]  Spark Arrestor [ ]  On/Off switch |
| [ ]  Record of Safety Inspection within past 12 months  | [ ]  Chain Brake [ ]  Headlamp or Flashlight |
| [ ]  Radio: Refer to form FC-100R |
| *\*See requirements for potable water equipment on the following page.* | [ ]  Saw tool kit [ ]  Bar length |

|  |
| --- |
| **Potable Water Equipment***\*\*Equipment less than 500 gallons used for servicing portable hand washing equipment, etc., do not qualify for the potable water tender rate.\*\** |
| [ ]  California DPH Sanitary Certification (sticker affixed to the tank) |
| [ ]  Activity log for each potable water tank that is permanently attached to licensed motor vehicle |
| [ ]  Confirm monthly water tests and vehicle water source log |
| [ ]  Current calendar year DPH seal/sticker affixed to upper left quarter of rear of the hauling tank |
| [ ]  Monthly bacterial analysis results. Must include a coliform and plate count determination.**Coliform levels less than 2.2 are desired, but 2.2 is acceptable. Test certificate indicating a** **coliform level above 2.2 shall not be utilized.** |
| [ ]  Water purification systems attached to water tenders are not accepted. |
| [ ]  Supplier will carry on each vehicle (1) an owner’s manual or (2) a letter from the pump manufacturer stating that the water pump being used is for food grade service. |
| **Special note on potable water equipment:** The DPH recommends that CAL FIRE Units contact the nearest DPH field office to obtain a current listing of licensed potable water haulers for that area. |

|  |  |
| --- | --- |
| **Drivers and Operators:** | FSTEP\* |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | [ ]  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | [ ]  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | [ ]  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | [ ]  |
| [ ]  Workers’ Compensation  | [ ]  Major Medical Insurance | [ ]  Liability Insurance |
| **Operators must wear the following Cal/OSHA approved Personal Protective Equipment (PPE) items. Refer to Chapter 6 of the Hired Equipment Program Supplier Participation Manual.** |
| [ ]  Nomex shirt and pants, or jumpsuit | [ ]  Hardhat with goggles & Nomex face shroud |
| [ ]  Fire shelter: USFS-approved | [ ]  8” Lace-up leather boots |
| [ ]  Radio: Refer to form FC-100R | [ ]  Headlamp or flashlight |
| [ ]  Wildland Firefighting Gloves with gauntlets | *\*Current Fire Safety Training Completion Card* |
| **Re-inspection:** [ ]  **Pass** [ ]  **Fail** |

|  |  |  |
| --- | --- | --- |
| Inspector’s Signature |  | Date |
|  |  |  |
| Printed Name |  |  |