|  |  |
| --- | --- |
| **Company/Supplier Name & Order/ Request #** | **Equipment Description (Type/Year/Make)** |
| **Driver/Operator Signature & Contact Phone #** | **Model & License or Serial/ VIN Number** |
| **FIRELINE WATER TENDER** | **FIRELINE BULLDOZER** |
| Reflectors – DOT- set of 3 | ROPS with sweeps and side / rear screens |
| 2 Chock blocks – appropriate for tire size  Minimum 1 quart drinking water/person/hour | Belly pans  Rock guards (Optional)  Radiator protection |
| Flashlight  Seat belts (Serviceable) | Flashlight  Seat belts (Serviceable) |
| Contractor’s identification on equipment items | Lights – 4 front and 2 rear |
| Back-up alarm (97 dB minimum) | 1 - Shovel and 1 - Axe or Pulaski |
| Fire Extinguisher (2A10BC min.) Mounted | Backup Alarm (97 dB minimum) |
| 1 - Shovel and 1 - Axe or Pulaski | Fire Extinguisher (2A10BC min.) Mounted |
| Road Spraying: forward or rear-facing capable | Fire Curtains mounted on front, sides & rear |
| Radio: Refer to form FC-100R  If Radio is mounted; external speaker | Minimum 1 quart drinking water per person per hour |
| 200 GPM Pump (minimum), Drafting capable | Radio: Refer to form FC-100R |
| Backflow protection device | Radio headset |
| 24’ hard suction hose - 2.5” or 3” connections | **TRANSPORT** |
| Legal tank capacity | Record of Safety Inspect within past 12 mo. |
| Tank baffles | Seat belts (Serviceable) |
| Certified weight ticket with legal tare load limit by axle/group | Fire Extinguisher (2A10BC min) Mounted  Reflectors DOT-set of three |
| 1 - 1” combination nozzle w/ 1.5” x 1” reducer | Mirrors, Glass, & Lights |
| 100’ x 1½” fire hose with nozzle | Radio: Refer to form FC-100R |
| 2 – 1½” gated male NH discharge outlets or gated wye | # Axles # Tires . |
| 1.5” fire hose clamp and hydrant wrench | **FALLER** |
| 1- 25’ x 2.5” min. hydrant fill hose with NH fittings | Chaps  Falling Axe & Wedges  Spark Arrestor  On/Off switch |
| Record of Safety Inspection within past 12 months | Chain Brake  Headlamp or Flashlight |
| Radio: Refer to form FC-100R |
| *\*See requirements for potable water equipment on the following page.* | Saw tool kit  Bar length |

|  |
| --- |
| **Potable Water Equipment**  *\*\*Equipment less than 500 gallons used for servicing portable hand washing equipment, etc., do not qualify for the potable water tender rate.\*\** |
| California DPH Sanitary Certification (sticker affixed to the tank) |
| Activity log for each potable water tank that is permanently attached to licensed motor vehicle |
| Confirm monthly water tests and vehicle water source log |
| Current calendar year DPH seal/sticker affixed to upper left quarter of rear of the hauling tank |
| Monthly bacterial analysis results. Must include a coliform and plate count determination.  **Coliform levels less than 2.2 are desired, but 2.2 is acceptable. Test certificate indicating a** **coliform level above 2.2 shall not be utilized.** |
| Water purification systems attached to water tenders are not accepted. |
| Supplier will carry on each vehicle (1) an owner’s manual or (2) a letter from the pump manufacturer stating that the water pump being used is for food grade service. |
| **Special note on potable water equipment:** The DPH recommends that CAL FIRE Units contact the nearest DPH field office to obtain a current listing of licensed potable water haulers for that area. |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Drivers and Operators:** | | | | FSTEP\* |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |  |
| Class \_\_\_\_ License # \_\_\_\_\_\_\_\_\_\_\_\_\_ Endorsement \_\_\_\_ Operator: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |  |
| Workers’ Compensation | Major Medical Insurance | | Liability Insurance | |
| **Operators must wear the following Cal/OSHA approved Personal Protective Equipment (PPE) items. Refer to Chapter 6 of the Hired Equipment Program Supplier Participation Manual.** | | | | |
| Nomex shirt and pants, or jumpsuit | | Hardhat with goggles & Nomex face shroud | | |
| Fire shelter: USFS-approved | | 8” Lace-up leather boots | | |
| Radio: Refer to form FC-100R | | Headlamp or flashlight | | |
| Wildland Firefighting Gloves with gauntlets | | *\*Current Fire Safety Training Completion Card* | | |
| **Re-inspection:  Pass  Fail** | | | | |

|  |  |  |
| --- | --- | --- |
| Inspector’s Signature |  | Date |
|  |  |  |
| Printed Name |  |  |