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	SEQUENCE OF JOB STEPS:
	HAZARDS
	RECOMMENDATIONS/ COMMENTS

	1. Assess and survey area for any potential hazards fill out JSA 
	Uncontrolled release of hazardous energy
Working area clear of hazards
	Implement control measures before proceeding. 
Document pre-job work plan

	2. Position truck for job
	Obstacles in the area Environmental release Exposure to hazardous liquids
	Position truck to see the load valve. This allows you to see the complete job while you are doing it.

	3. Hook up grounding cable to wellhead
	Worn spots or wickers in grounding cable
Tripping hazard 
	Make sure to pull out extra cable and lay it flat on the ground, so you won't trip on it. Scratch off paint with clamp when installing to get a good connection

	4. Connect hose to tank valve with camlock fitting
	Environmental release
Untethered camlock ears may become loose due to vibration from loading
	Make sure to secure camlock fitting and tie hose ears shut
Inspect all hoses and fittings for excessive wear or abrasions 

	5. Open valve at tank and check for any leaks in connections
	Environmental release
Pinch points
Untethered camlock fittings may become loose due to vibration from loading

	Clean and lube all fittings when installing
Be sure to secure camlock fitting shut while loading
Check all hoses and fittings for leakage before engaging pump

	6. Open vent valve on  truck tank and open fire valves
	Failure to open vent valve may cause damage to truck tank
Hazardous release of vapor gas from tank
	Inspect all plumbing for leakage before engaging pump to load



	7. Open valve on truck and engage roper pump to load product
	Venting gas from truck tank can be hazardous 
	Check tank vent line to make sure its venting do not breathe while checking the vent 
Make sure to have your 4 gas meter on and functioning

	8. When loaded shut valve at tank and open hose ears slowly to give it air to suck out hose
	Environmental release
Muscle strain
	After venting hose lift it and walk it out to truck to suck leftovers out of hose and close valve at truck
Drain any leftovers into metal bucket not on the ground

	10. Disengage pump remove hose and put cap on camlock at truck


	Environmental release
Pinch point

	Always install caps on camlocks of truck before travel


	11. Close vent valve and fire valves on truck


	Release of flammable, toxic and LEL hazards 
	Always keep tank shut in when traveling


	12. Put away hoses and fittings 


	Muscle strain 
Protective gloves
	Always wear PPE, gloves, eye protection, FR clothing, etc.


	13. 



	
	

	14.
	
	

	CAUTION: Flammable liquid (i.e., any liquid with a flashpoint of 140 degrees fahrenheit or less) shall require the use of a combustibility monitor on a continuous basis during fluid transfer to ensure the safe disbursement of vapors. The use of FRC clothing is mandatory. Operations shall be terminated immediately anytime the LEL exceeds 10% in the work environment.   Avoid lines of fire. SDS is required on location prior to transfer operations.
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