The 2005 Harley-Davidson Softail Standard delivers 1450cc of air-cooled V-twin power, paired with a five-speed transmission and belt final drive–key upgrades over earlier models. Max torque (107 Nm at 3000 RPM) ensures responsive low-end performance, ideal for highway cruising and city riding. The 49mm fork suspension with 152mm of travel and hidden coil-over shocks (Softail design) balances comfort and stability, though heavier riders may notice sag under load.
Dry weight sits at 320 kg, with a 2.8-gallon fuel tank (10.6L) offering a 120-mile range (193 km) at a 42-45 mpg average. Stock seat height (660mm) suits most riders, but aftermarket options exist for taller or shorter frames. Twin 292mm disc brakes with four-piston calipers provide adequate stopping power, though aggressive riding may require upgraded pads or rotors.
Factory specs include a single-fire electronic ignition, Keihin 40mm CV carburetor, and self-adjusting cam chain tensioners–a reliability upgrade from earlier rubber-mounted designs. Chrome dual exhausts feature dual catalytic converters, meeting EPA Tier 1 emissions. For maintenance, oil change intervals (3,000 miles/5,000 km) and primary chain tension checks (every 10,000 miles/16,000 km) are critical. Stock tires (MT90B16 front, MU85B16 rear) prioritize longevity over grip; consider Michelin Commander III or Pirelli Night Dragon for improved traction.




