Instruction for setting the Temperature on the Thermostat.

1 Remove clear plastic packaging.

2 Roll out the mat.

3 Insert the power plug to the wall socket and the thermostat light will illuminate.

4 Press and hold the Left hand arrow until the numbers start flashing. Adjust this temp to 26degC by pressing the left arrow to increase and the right arrow to decrease the temp. When 26 is selected. Do not touch for 5seconds and the lights will stop flashing. this indicates the left temp is set. This is the temperature that the heat will turn on at. MIN TEMP

5 Press and hold the Right hand arrow until the numbers start to flash. Adjust this temp to 27degC by pressing the left arrow to increase and the right arrow to decrease the temp. When 27 is selected. Do not touch for 5 seconds and the lights will stop flashing. This indicates the right temp is set. This is the temperature that the heat will turn off. MAX TEMP

6 Please check the settings by holding the temperature probe in your fingers. When the temp rises above the MAX TEMP. The red light will go off. Let go of the heat probe and put to one side. When the temperature drops down to the MIN TEMP, the red light will come on.

7 When set. Tape the probe to the heat mat to stop it coming loose.

8 Place your grow bag or box in the middle of the heat mat and on top of the temp probe. Adding insulation under the heat mat in beneficial.

This thermostat will now maintain the perfect temperature to incubate your colonising mycelium. You must always have the thermostat temp probe between the heat mat and the Box or Tub.

Feel free to email me at Mushbuddiessales@gmail.com if you have any questions