*************************** START ****************************

Chip: ESP32S3
Download mode: uart
Start time: 20250909-16:23
Connect baud: 115200
Com:COM20
connecting...
manufacturer_id: 0x20
device_id: 0x4017
fs:0x200200
address/file: 0 D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\bootloader.bin
address/file: 32768 D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\partitions.bin
address/file: 65536 D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\firmware.bin

Wrote 20256 bytes (13096 compressed) at 0x00000000 in 0.3 seconds (effective 527.1 kbit/s)...


Wrote 3072 bytes (146 compressed) at 0x00008000 in 0.0 seconds (effective 755.7 kbit/s)...


Wrote 1351200 bytes (779199 compressed) at 0x00010000 in 10.8 seconds (effective 997.3 kbit/s)...

File: D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\bootloader.bin
File  md5: dbf8eebb0d251ef251971fa226e342dc
Flash md5: dbf8eebb0d251ef251971fa226e342dc
Hash of data verified.
File: D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\partitions.bin
File  md5: 801ba71678a964614657a6d8fbc6baca
Flash md5: 801ba71678a964614657a6d8fbc6baca
Hash of data verified.
File: D:\Backup\Documents\PlatformIO\Projects\Example for Robot Driver Lite\download_tool\RD_ESP32S3_LITE_Download_Tool\dl_temp\bin_tmp\downloadPanel1\firmware.bin
File  md5: 01ad7e73053906a08841c96b584e37b9
Flash md5: 01ad7e73053906a08841c96b584e37b9
Hash of data verified.

Leaving...

com closed
Total use time: 16 s

Download result: PASS

*************************** END ****************************



