**YXZ Stereo Install Instructions**

For Technical Support Call: (740)858-0707

1. Place straps around bars like shown. One on each side, and two on front.



1. Hold stereo box against the roof, all the way to the very front. (this is easier with someone to help)
2. Screw clamps to box with self-drilling screws, DO NOT tighten until all clamps are installed with screws. SCREWS CAN STRIP OUT!
3. Run wire across cage bar to battery. Keep wire on inside of cage, secure with zip ties. (see photos)


IMPORTANT: wire needs to be under the seat bar!

1. Make the battery connections (this has to be done last!).

IMPORTANT: The fuse goes to +12V red side! (see photo)

**\*IF CONNECTED BACKWARDS IT WILL BLOW FUSE IN HEAD UNIT!!!!!!**



Sony Tuning

Band1: -3

Band2: 2

Band3: 0

Band4: 5

Band5: 9

1. Enjoy your new stereo!!

Note: Use supplied screw spacers if necessary.