#### 8.8.3.5 IfcMaterialProfileSetUsage

| Mise en place d'un ensemble de matériaux de profil
| Gruppe von Profilen mit Material - Verwendung

IfcMaterialProfileSetUsage determines the usage of IfcMaterialProfileSet in terms of its location relative to the associated element geometry. The location of a material profile set shall be compatible with the building element geometry (that is, material profiles shall fit inside the element geometry). The rules to ensure the compatibility depend on the type of the building element. For building elements with shape representations which are based on extruded solids, this is accomplished by referring to the identical profile definition in the shape model as in the material profile set.

> NOTE Model view definitions or implementer agreements may provide more instructions on matching between building element geometry and material profile set usage.

> NOTE The referenced IfcMaterialProfileSet may represent a single material profile, or a composite profile with two or more material profiles.

> HISTORY New entity in IFC4.

XSD Specification:

<xs:element name="IfcMaterialProfileSetUsage" type="ifc:IfcMaterialProfileSetUsage" substitutionGroup="ifc:IfcMaterialUsageDefinition" nillable="true"/>
<xs:complexType name="IfcMaterialProfileSetUsage">
<xs:complexContent>
<xs:extension base="ifc:IfcMaterialUsageDefinition">
<xs:sequence>
<xs:element name="ForProfileSet" type="ifc:IfcMaterialProfileSet" nillable="true"/>
</xs:sequence>
</xs:extension>
</xs:complexContent>
</xs:complexType>

EXPRESS Specification:

ENTITY IfcMaterialProfileSetUsage

| SUBTYPE OF (IfcMaterialUsageDefinition);

ForProfileSet | : | IfcMaterialProfileSet;
CardinalPoint | : | OPTIONAL IfcStrippedOptional;
ReferenceExtent | : | OPTIONAL IfcStrippedOptional;

END_ENTITY;

Attribute Definitions:

ForProfileSet | : | The IfcMaterialProfileSet set to which the usage is applied.
ReferenceExtent | : | Extent of the extrusion of the elements body shape representation to which the IfcMaterialProfileSetUsage applies. It is used as the reference value for the upper OffsetValues[2] provided by the IfcMaterialProfileSetWithOffsets subtype for included material profiles. NOTE The attribute ReferenceExtent shall be asserted if an IfcMaterialProfileSetWithOffsets is included in the ForProfileSet.MaterialProfiles list of material layers. NOTE The ReferenceExtent for IfcBeamStandardCase, IfcColumnStandardCase, and IfcMemberStandardCase is the reference length starting at z=0 being the XY plane of the object coordinate system.

Inheritance Graph:

ENTITY IfcMaterialProfileSetUsage

| ENTITY IfcMaterialUsageDefinition

| INVERSE

AssociatedTo | : | SET [1:?] OF IfcRelAssociatesMaterial FOR RelatingMaterial;

| ENTITY IfcMaterialProfileSetUsage

ForProfileSet | : | IfcMaterialProfileSet;
CardinalPoint | : | OPTIONAL IfcStrippedOptional;
ReferenceExtent | : | OPTIONAL IfcStrippedOptional;

END_ENTITY;

Link to this page