#### 8.9.2.5 IfcElectricCurrentMeasure

The value for the movement of electrically charged particles.

Usually measured in Ampere (A).

Type: REAL

> NOTE Type adapted from electric_current_measure defined in ISO 10303-41.

> HISTORY New type in IFC1.5.1.

XSD Specification:

<xs:simpleType name="IfcElectricCurrentMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
<xs:element name="IfcElectricCurrentMeasure-wrapper" nillable="true">
<xs:complexType>
<xs:simpleContent>
<xs:extension base="ifc:IfcElectricCurrentMeasure">
<xs:attributeGroup ref="ifc:instanceAttributes"/>
</xs:extension>
</xs:simpleContent>
</xs:complexType>
</xs:element>

EXPRESS Specification:

TYPE IfcElectricCurrentMeasure = REAL;
END_TYPE;

Link to this page