#### 7.2.4.3 Pset_CableCarrierSegmentTypeCableTraySegment

PSET_TYPEDRIVENOVERRIDE / IfcCableCarrierSegment / CABLETRAYSEGMENT

| An (typically) open carrier segment onto which cables are laid. HISTORY: IFC4 - NominalLength deleted. To be handled as a quantity measure
| 典型的な開放型ケーブルキャリアに関するプロパティセット定義。

buildingSMART Data Dictionary

PSD-XML

- NominalWidth
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalWidth: The nominal width of the segment.
  | 公称幅: 呼び幅寸法。
  | 공칭 폭: 폭 치수

- NominalHeight
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalHeight: The nominal height of the segment.
  | 公称高: 呼び高寸法。
  | 공칭 높이: 고 치수

- HasCover
  P_SINGLEVALUE / IfcBoolean

  | HasCover: Indication of whether the cable tray has a cover (=TRUE) or not (= FALSE). By default, this value should be set to FALSE..
  | カバー: カバー付かどうか。
  | 커버: 커버 유무

Link to this page