#### 7.2.4.6 Pset_CableCarrierSegmentTypeConduitSegment

PSET_TYPEDRIVENOVERRIDE / IfcCableCarrierSegment / CONDUITSEGMENT

| An enclosed tubular carrier segment through which cables are pulled. HISTORY: IFC4 - NominalLength deleted. To be handled as a quantity measure.
| 電線管のプロパティを設定。

buildingSMART Data Dictionary

PSD-XML

- NominalWidth
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalWidth: The nominal width of the segment.
  | 公称幅: 呼び幅寸法。
  | 공칭 폭: 폭 치수

- NominalHeight
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | NominalHeight: The nominal height of the segment.
  | 公称高: 呼び高寸法。
  | 공칭 높이: 고 치수

- ConduitShapeType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_ConduitShapeType: CIRCULAR, OVAL, OTHER, NOTKNOWN, UNSET

  | ConduitShapeType: The shape of the conduit segment.
  | 電線管のタイプ: 電線管の形状タイプ。 （円筒形,卵形,その他,不明,なし）
  | 전선관의 유형: 전선관의 형상 타입. (원통형, 계란 모양, 기타 알 수 없음) "

- IsRigid
  P_SINGLEVALUE / IfcBoolean

  | IsRigid: Indication of whether the conduit is rigid (= TRUE) or flexible (= FALSE).
  | 鋼管: 鋼管か否か。
  | 강관:

Link to this page