#### 7.2.4.28 Pset_ProtectiveDeviceBreakerUnitI2TFuseCurve

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice

| A coherent set of attributes representing curves for melting- and breaking-energy of a fuse. Note - A fuse may be associated with different instances of this property set providing information related to different basic characteristics.
| フューズの融解-遮断エネルギー曲線を表す一連のプロパティセット。 注記-フューズは、根本的な特性に関連付けられた提供されたプロパティの情報は、　異なる実態に関連しているかもしれません。

buildingSMART Data Dictionary

PSD-XML

- VoltageLevel
  P_ENUMERATEDVALUE / IfcLabel / PEnum_VoltageLevels: U230, U400, U440, U525, U690, U1000, OTHER, NOTKNOWN, UNSET

  | VoltageLevel: The voltage levels of the fuse for which the data of the instance is valid. More than one value may be selected in the enumeration.
  | 電圧レベル: 電圧レベルを選択。
  | 전압레벨: 전압 레벨을 선택합니다.

- BreakerUnitFuseMeltingCurve
  P_TABLEVALUE / IfcElectricCurrentMeasure / IfcReal

  | BreakerUnitFuseMeltingCurve: A curve that establishes the energy required to melt the fuse of a breaker unit when a particular prospective melting current is applied. Note that the breaker unit fuse melting curve is defined within a Cartesian coordinate system and this fact must be: (1) Defining value: ProspectiveCurrentMelting :A list of minimum 2 and maximum 8 numbers providing the currents in [A] for points in the current/melting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value: MeltingEnergy: A list of minimum 2 and maximum 8 numbers providing the energy whereby the fuse is starting to melt, I2t, in [A2s] for points in the current/melting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points.
  | フューズ遮断機融解曲線: 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 （1）定義値：融解電流：電流/ 融解エネルギーで示される最小2から最大8のリストで電流[A]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。 （2）定義値：融解エネルギー：/電流/融解エネルギーの位置[A2s]で示される2～16の想定されるフューズが溶解始める電流[A2s]を定義します。カーブが連続する2つの点を結ぶ直線として描かれています。
  | 퓨즈 차단기 융해 곡선: 예상치 못한 전류가 흐를 때 차단기의 퓨즈를 녹이는 데 필요한 에너지를 나타내는 곡선. 예상외의 전류가 흘렀을 때에 차단기의 퓨즈를 녹이는 데 필요한 에너지를 나타내는 곡선. (1) 정의 값 : 융해 전류 : 전류 / 융해 에너지에 표시된 최소 2에서 최대 8 개의 목록에서 전류 [A]를 정의합니다. 커브가 연속되는 두 개의 점을 연결하는 직선으로 그려져 있습니다. (2) 정의 값 : 융해 에너지 :/ 전류 / 융해 에너지의 위치 [A2s에서 나타나는 2 ~ 16 예상되는 퓨즈가 용해 시작 전류 [A2s을 정의합니다. 커브가 연속되는 두 개의 점을 연결하는 직선으로 그려져 있습니다.

- BreakerUnitFuseBreakingingCurve
  P_TABLEVALUE / IfcElectricCurrentMeasure / IfcReal

  | BreakerUnitFuseBreakingingCurve: A curve that establishes the let through breaking energy of a breaker unit when a particular prospective breaking current is applied. Note that the breaker unit fuse breaking curve is defined within a Cartesian coordinate system and this fact must be: (1) Defining value: ProspectiveCurrentBreaking: A list of minimum 2 and maximum 8 numbers providing the currents in [A] for points in the current/breaking energy log/log coordinate space. The curve is drawn as a straight line between two consecutive points. (2) Defined value: LetThroughBreakingEnergy: A list of minimum 2 and maximum 8 numbers providing the breaking energy whereby the fuse has provided a break, I2t, in [A2s] for points in the current/breakting_energy log/log coordinate space. The curve is drawn as a straight line between two consecutive.
  | フューズ遮断機融解曲線: 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 想定外の電流が流れた時に遮断機のフューズを溶かすために必要なエネルギーを表す曲線。 （1）定義値：融解電流：電流/ 融解エネルギーで示される最小2から最大8のリストで電流[A]を定義します。 カーブが連続する2つの点を結ぶ直線として描かれています。 （2）定義値：融解エネルギー：/電流/融解エネルギーの位置[A2s]で示される2～16の想定されるフューズが溶解始める電流[A2s]を定義します。カーブが連続する2つの点を結ぶ直線として描かれています。
  | 퓨즈 차단기 융해 곡선: 예상치 못한 전류가 흐를 때 차단기의 퓨즈를 녹이는 데 필요한 에너지를 나타내는 곡선. 예상외의 전류가 흘렀을 때에 차단기의 퓨즈를 녹이는 데 필요한 에너지를 나타내는 곡선. (1) 정의 값 : 융해 전류 : 전류 / 융해 에너지에 표시된 최소 2에서 최대 8 개의 목록에서 전류 [A]를 정의합니다. 커브가 연속되는 두 개의 점을 연결하는 직선으로 그려져 있습니다. (2) 정의 값 : 융해 에너지 :/ 전류 / 융해 에너지의 위치 [A2s에서 나타나는 2 ~ 16 예상되는 퓨즈가 용해 시작 전류 [A2s을 정의합니다. 커브가 연속되는 두 개의 점을 연결하는 직선으로 그려져 있습니다.

Link to this page