#### 7.2.4.33 Pset_ProtectiveDeviceTypeCircuitBreaker

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice / CIRCUITBREAKER

| A coherent set of attributes representing different capacities of a circuit breaker or of a motor protection device, defined in accordance with IEC 60947. Note - A protective device may be associated with different instances of this property set providing information related to different basic characteristics.
| IECの60947に基づいて定義されている回路ブレーカ、またはモータ保護装置の異なる容量を表すプロパティセットの定義。 注記-保護装置は、根本的な特性に関連付けられた提供されたプロパティの情報は、　異なる実態に関連しているかもしれません。

buildingSMART Data Dictionary

PSD-XML

- PerformanceClasses
  P_LISTVALUE / IfcLabel

  | PerformanceClasses: A set of designations of performance classes for the breaker unit for which the data of this instance is valid. A breaker unit being a circuit breaker may be constructed for different levels of breaking capacities. A maximum of 7 different performance classes may be provided. Examples of performance classes that may be specified include B, C, N, S, H, L, V.
  | 能力クラス: モータ保護を行う開閉装置は、能力が違う最大7種類がある。名称の例として、B, C, N, S, H, L, Vが含まれる。
  | 능력 클래스: 모터 보호하는 개폐 장치는 능력이 다른 최대 7 종류가있다. 이름의 예로는, B, C, N, S, H, L, V가 포함된다.

- VoltageLevel
  P_ENUMERATEDVALUE / IfcLabel / PEnum_VoltageLevels: U230, U400, U440, U525, U690, U1000, OTHER, NOTKNOWN, UNSET

  | VoltageLevel: The voltage levels for which the data of the instance is valid. More than one value may be selected in the enumeration.
  | 電圧レベル: 電圧レベルを選択。
  | 전압레벨: 전압 레벨을 선택합니다.

- ICU60947
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | ICU60947: The ultimate breaking capacity in [A] for a circuit breaker or motor protection device tested in accordance with the IEC 60947 series.
  | 定格限界短絡遮断容量: IECの60947シリーズに基づいてテストされた回路遮断機及びモータ保護装置の短絡遮断容量[A]。
  | 정격한계단락 차단 용량: IEC의 60947 시리즈를 기반으로 테스트 회로 차단기 및 모터 보호 장치의 단락 차단 용량 [A].

- ICS60947
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | ICS60947: The service breaking capacity in [A] for a circuit breaker or motor protection device tested in accordance with the IEC 60947 series.
  | 定格使用短絡遮断容量: IECの60947シリーズに基づいてテストされた回路遮断機及びモータ保護装置の使用短絡遮断容量[A]。
  | 정격사용 단락 차단 용량: IEC60947 시리즈를 기반으로 테스트 배선 차단기 또는 모터 보호 장치를위한 전류 [A]에 견디는 온도 값은 1s 주어진다.

- ICW60947
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | ICW60947: The thermal withstand current in [A] for a circuit breaker or motor protection device tested in accordance with the IEC 60947 series. The value shall be related to 1 s.
  | ICW60947: IEC60947シリーズに基づいてテストした配線遮断機またはモータ保護装置のための電流[A]に耐える温度。 値は、1sで与えられる。
  | ICW60947: IEC60947 시리즈를 기반으로 테스트 배선 차단기 또는 모터 보호 장치를위한 전류 [A]에 견디는 온도 값은 1s 주어진다.

- ICM60947
  P_SINGLEVALUE / IfcElectricCurrentMeasure

  | ICM60947: The making capacity in [A] for a circuit breaker or motor protection device tested in accordance with the IEC 60947 series.
  | ICM60947: IECの60947シリーズに基づいてテストされた回路遮断機またはモータ保護装置の能力[A]。
  | ICM60947: IEC의 60947 시리즈를 기반으로 테스트 회로 차단 기나 모터 보호 장치의 능력 [A].

Link to this page