#### 7.3.4.27 Pset_ValveTypeFlushing

PSET_TYPEDRIVENOVERRIDE / IfcValve / FLUSHING

| Valve that flushes a predetermined quantity of water to cleanse a WC, urinal or slop hopper. Note that a flushing valve is constrained to have a 2 port pattern.
| 弁タイプフラッシュ

buildingSMART Data Dictionary

PSD-XML

- FlushingRate
  P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

  | FlushingRate: The predetermined quantity of water to be flushed.
  | フラッシュ率: 予め決められた流される水量

- HasIntegralShutOffDevice
  P_SINGLEVALUE / IfcBoolean

  | HasIntegralShutOffDevice: Indication of whether the flushing valve has an integral shut off device fitted (set TRUE) or not (set FALSE).
  | 全体閉止装置がついているかどうか: フラッシュ弁に全体閉止装置がついているかどうかの表示（付きTRUE）又は（無しFALSE）

- IsHighPressure
  P_SINGLEVALUE / IfcBoolean

  | IsHighPressure: Indication of whether the flushing valve is suitable for use on a high pressure water main (set TRUE) or not (set FALSE).
  | 高圧給水の有無: フラッシュ弁の高圧給水主管への使用が適当かどうかの表示（適 TRUE）又は（不適 FALSE）

Link to this page