#### 7.3.4.9 Pset_FlowMeterTypeCommon

PSET_TYPEDRIVENOVERRIDE / IfcFlowMeter

| Common attributes of a flow meter type

buildingSMART Data Dictionary

PSD-XML

- Reference
  P_SINGLEVALUE / IfcIdentifier

  | Reference: Reference ID for this specified type in this project (e.g. type 'A-1').
  | 参照記号: このプロジェクトにおける参照記号(例：A-1)。分類コードではなく内部で使用されるプロジェクトタイプとして使用されるもの。

- Status
  P_ENUMERATEDVALUE / IfcLabel / PEnum_Status: NEW, EXISTING, DEMOLISH, TEMPORARY, OTHER, NOTKNOWN, UNSET

  | Status: Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished, "Temporary" - element will exists only temporary (like a temporary support structure).
  | 状態: 要素（主にリノベーションまたは改修プロジェクトにおいて）の状態。 状態は、「新規(New)」－新しく追加される要素。「既存」－要素は存在し、かつ残りもの。「破壊」－要素は存在したが、廃棄されるもの。「一時的」－一時的に存在する要素（一時的にサポートしている構造のようなもの）。

- ReadOutType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_MeterReadOutType: DIAL, DIGITAL, OTHER, NOTKNOWN, UNSET

  | ReadOutType: Indication of the form that readout from the meter takes. In the case of a dial read out, this may comprise multiple dials that give a cumulative reading and/or a mechanical odometer.

- RemoteReading
  P_SINGLEVALUE / IfcBoolean

  | RemoteReading: Indicates whether the meter has a connection for remote reading through connection of a communication device (set TRUE) or not (set FALSE).

Link to this page