#### 7.3.4.16 Pset_PipeFittingTypeJunction

PSET_TYPEDRIVENOVERRIDE / IfcPipeFitting / JUNCTION

| Pipe fitting type attributes for junction shapes.

buildingSMART Data Dictionary

PSD-XML

- JunctionType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_PipeFittingJunctionType: TEE, CROSS, OTHER, NOTKNOWN, UNSET

  | JunctionType: The type of junction. TEE=3 ports, CROSS = 4 ports.
  | 継ぎ手タイプ: 接合のタイプ　(T継ぎ手は3本　十字継ぎ手は4本)

- JunctionLeftAngle
  P_SINGLEVALUE / IfcPositivePlaneAngleMeasure

  | JunctionLeftAngle: The change of direction of flow for the left junction.
  | 左継ぎ手角度: 左継ぎ手の流れの方向の変化

- JunctionLeftRadius
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | JunctionLeftRadius: The radius of bending for the left junction.
  | 左継ぎ手半径: 左継ぎ手の曲がりの半径

- JunctionRightAngle
  P_SINGLEVALUE / IfcPositivePlaneAngleMeasure

  | JunctionRightAngle: The change of direction of flow for the right junction where 0 indicates straight segment.
  | 右継ぎ手角度: 右継ぎ手の流れの方向の変化

- JunctionRightRadius
  P_SINGLEVALUE / IfcPositiveLengthMeasure

  | JunctionRightRadius: The radius of bending for the right junction where 0 indicates sharp bend.
  | 右継ぎ手半径: 右継ぎ手の曲がりの半径(ゼロは鋭い曲がりを意味する)

Link to this page