#### 7.2.4.8 Pset_SwitchingDeviceTypeEmergencyStop

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / EMERGENCYSTOP

| An emergency stop device acts to remove as quickly as possible any danger that may have arisen unexpectedly.
| IEC 826-08-03の定義: 緊急停止スイッチは予期せずして起こるさまざまな危険を可能な限り迅速に取り除くように動作する装置である。

buildingSMART Data Dictionary

PSD-XML

- SwitchOperation
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchingDeviceEmergencyStopType: MUSHROOM, OTHER, NOTKNOWN, UNSET

  | SwitchOperation: Indicates operation of emergency stop switch.
  | スイッチ操作: 緊急停止スイッチの操作を示す。
  | 스위치 조작: 비상 정지 스위치의 조작을 보여준다.

Link to this page