#### 7.1.4.29 Pset_SensorTypeHumiditySensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / HUMIDITYSENSOR

| A device that senses or detects humidity. HISTORY: HumiditySensorSetPoint changed to SetPointHumidity. Range, accuracy and time constant deleted.
| 湿度を感知または検出するデバイス。

buildingSMART Data Dictionary

PSD-XML

- SetPointHumidity
  P_BOUNDEDVALUE / IfcPositiveRatioMeasure

  | SetPointHumidity: The humidity value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
  | 湿度設定値: 感知される湿度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。
  | 습도 설정: 감지되는 습도. 세트 포인트 값을 넣으려면, IfcPropertyBoundedValue.SetPointValue를 사용하십시오.

Link to this page