ISO-10303-21;
HEADER;
FILE_DESCRIPTION((),'2;1');
FILE_NAME('E:\\MVD_BAMIE\\annex\\annex-a\\default\\ifc4.ifc.txt','2013-03-12T16:53:42',('Sony DUO 11'),('VAIO'),'buildingSMART IFCDOC 5.0','buildingSMART IFC Documentation Generator',$);
FILE_SCHEMA(('IFC4'));
ENDSEC;

DATA;
#1= IFCPROJECT('0Pf1GTW393Mx8p7gOGAIdr',$,'IFC4 Property Set Templates',$,$,$,$,$,$);
#2= IFCLIBRARYINFORMATION('IFC4 Property Set Templates','IFC4',$,'2013-03-12T16:53:42','',$);
#3= IFCRELASSOCIATESLIBRARY('1YEVxLuJLBDPslcQ_qDoQW',$,$,$,(#1),#2);
#4= IFCRELDECLARES('1sQJCgCRb7G8zwlv10S4Dy',$,$,$,#1,(#5,#52,#81,#108,#115,#124,#142,#167,#181,#194,#207,#220,#233,#239,#254,#266,#278,#295,#301,#312,#335,#343,#347,#359,#373,#387,#392,#404,#412,#420,#438,#446,#458,#476,#484,#497,#505,#513,#521,#525,#533,#546,#554,#562,#580,#588,#602,#616,#621,#634,#637,#639,#656,#668,#670,#682,#725,#734,#743,#752,#761,#770,#772,#793,#802,#815));
#5= IFCPROPERTYSETTEMPLATE('1o4TaT2Vr74xAMwHrz$yDp',$,'Pset_TransportElementCommon','Properties common to the definition of all occurrences of IfcTransportElement or IfcTransportElementType',.PSET_TYPEDRIVENOVERRIDE.,'IfcTransportElement',(#12,#21,#29,#36,#43));
#6= IFCLIBRARYREFERENCE($,$,$,'Property Set Definition in German','de-DE',#2);
#7= IFCRELASSOCIATESLIBRARY('0vfdMyn8v6yv90sF_esTzU',$,$,$,(#5),#6);
#8= IFCLIBRARYREFERENCE($,$,$,'D\S\ifinition de l''IAI : propri\S\it\S\is communes \S\` la d\S\ifinition de toutes les instances de la classe IfcTransportElement','fr-FR',#2);
#9= IFCRELASSOCIATESLIBRARY('3sjMPTAuL4su9fcn2XuP9l',$,$,$,(#5),#8);
#10= IFCLIBRARYREFERENCE($,$,$,'\X2\4EA4901A89817D205171901A4E8B98053002\X0\','ja-JP',#2);
#11= IFCRELASSOCIATESLIBRARY('0MAy_AxZ1Aqvbir3IbtFB1',$,$,$,(#5),#10);
#12= IFCSIMPLEPROPERTYTEMPLATE('3S$EdIWbX4HujvV2ZZD$Si',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''). Used to store the non-classification driven internal construction type.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#13= IFCLIBRARYREFERENCE($,$,'Komponententyp','Bezeichnung zur Zusammenfassung gleichartiger Komponenten zu einem Komponententyp (auch Konstruktionstyp genannt). Alternativ zum Namen des "Typobjekts", insbesondere wenn die Software keine Typen unterst\S\|tzt.','de-DE',#2);
#14= IFCRELASSOCIATESLIBRARY('379jJtsRjACxtRuMk91ia4',$,$,$,(#12),#13);
#15= IFCLIBRARYREFERENCE($,$,'Reference','R\S\if\S\irence \S\` l''identifiant d''un type sp\S\icifi\S\i dans le contexte du projet (exemple : "type A1"). Utilis\S\i pour enregistrer un type sans recourir \S\` une classification.','fr-FR',#2);
#16= IFCRELASSOCIATESLIBRARY('3TMlxjYbP2hfL47wqvCOCR',$,$,$,(#12),#15);
#17= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\53C271673059308B\X0\ID\X2\756A53F73002\X0\','ja-JP',#2);
#18= IFCRELASSOCIATESLIBRARY('1tuJEJ6lP4DhtUBzIyaEJ6',$,$,$,(#12),#17);
#19= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\C774\X0\ \X2\D504B85CC81DD2B8C758\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : A-1). \X2\BD84B958\X0\ \X2\CF54B4DCAC00\X0\ \X2\C544B2CC\X0\ \X2\B0B4BD80C5D0C11C\X0\ \X2\C0ACC6A9B418B294\X0\ \X2\D504B85CC81DD2B8\X0\ \X2\D615C2DDC73CB85C\X0\ \X2\C0ACC6A9B429B2C8B2E4\X0\.','ko-KR',#2);
#20= IFCRELASSOCIATESLIBRARY('3HnAKBrtH4GBfDhZyqyphD',$,$,$,(#12),#19);
#21= IFCSIMPLEPROPERTYTEMPLATE('1qZp647PTCy8Ami62sUArh',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#22,$,$,$,.READWRITE.);
#22= IFCPROPERTYENUMERATION('PEnum_ElementStatus',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#23= IFCLIBRARYREFERENCE($,$,'Status','Status bzw. Phase des Bauteils insbesondere beim Bauen im Bestand. "Neu" (new) neues Bauteil als Erg\S\dnzung, "Bestand" (existing) bestehendes Bauteil, dass erhalten bleibt, "Abbruch" (demolish) Bauteil, das abgebrochen wird, "Tempor\S\dr" (temporary) Bauteil und andere Bauelemente, die vor\S\|bergehend eingebaut werden (wie Abst\S\|tzungen, etc.)','de-DE',#2);
#24= IFCRELASSOCIATESLIBRARY('0jZoZlxnv2nwxxGQLklWi1',$,$,$,(#21),#23);
#25= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#26= IFCRELASSOCIATESLIBRARY('3uq2icAkH0ceSYjimtDweM',$,$,$,(#21),#25);
#27= IFCLIBRARYREFERENCE($,$,'Statut','Statut de l''\S\il\S\iment, principalement utilis\S\i dans les projets de r\S\inovation et de r\S\ihabilitation. Le statut a pour valeur NOUVEAU pour un nouvel \S\il\S\iment, EXISTANT pour un \S\il\S\iment existant qui est conserv\S\i, DEMOLI pour un \S\il\S\iment existant \S\` d\S\imolir et TEMPORAIRE pour un \S\il\S\iment temporaire (comme une structure support provisoire).','fr-FR',#2);
#28= IFCRELASSOCIATESLIBRARY('2k6lyS9Rv3Xe4lp8HpePez',$,$,$,(#21),#27);
#29= IFCSIMPLEPROPERTYTEMPLATE('1xGh9fFqz26Pzv1WRE9oo7',$,'CapacityPeople','Capacity of the transportation element measured in numbers of person.',.P_SINGLEVALUE.,'IfcCountMeasure','',$,$,$,$,.READWRITE.);
#30= IFCLIBRARYREFERENCE($,$,'Personenkapazit\S\dt','Kapazit\S\dt nach Anzahl der Personen, die maximal bef\S\vrdert werden k\S\vnnen.','de-DE',#2);
#31= IFCRELASSOCIATESLIBRARY('33en0wLQb9jAWZaIeTY$cA',$,$,$,(#29),#30);
#32= IFCLIBRARYREFERENCE($,$,'\X2\642D4E574EBA65705B9A54E1\X0\','\X2\642C900189817D20306E4EBA6570306B95A23059308B5BB991CF3002\X0\','ja-JP',#2);
#33= IFCRELASSOCIATESLIBRARY('30b4dfwy5FAQeO2XSkPQZ4',$,$,$,(#29),#32);
#34= IFCLIBRARYREFERENCE($,$,'Capacit\S\i en nombre de personnes','Capacit\S\i de transport de l''\S\il\S\iment mesur\S\ie en nombre de personnes.','fr-FR',#2);
#35= IFCRELASSOCIATESLIBRARY('083AGx6W5E2uZFcbqHs8S$',$,$,$,(#29),#34);
#36= IFCSIMPLEPROPERTYTEMPLATE('1a20gPBjj8uwfRZZeT9q3U',$,'CapacityWeight','Capacity of the transport element measured by weight.',.P_SINGLEVALUE.,'IfcMassMeasure','',$,$,$,$,.READWRITE.);
#37= IFCLIBRARYREFERENCE($,$,'Lastkapazit\S\dt','Kapazit\S\dt nach Gewicht, das maximal bef\S\vrdert werden kann.','de-DE',#2);
#38= IFCRELASSOCIATESLIBRARY('1VC_g_XHnEsxO0lTZzwLid',$,$,$,(#36),#37);
#39= IFCLIBRARYREFERENCE($,$,'\X2\642D8F0991CD91CF\X0\','\X2\642C900189817D20306E91CD3055306B95A23059308B5BB991CF3002\X0\','ja-JP',#2);
#40= IFCRELASSOCIATESLIBRARY('3qzQAsTxD4AQef6oBrkzNB',$,$,$,(#36),#39);
#41= IFCLIBRARYREFERENCE($,$,'Capacit\S\i en poids','Capacit\S\i de transport de l''\S\il\S\iment mesur\S\ie par le poids.','fr-FR',#2);
#42= IFCRELASSOCIATESLIBRARY('22EiJnzLX1QxbPPO5KOxLX',$,$,$,(#36),#41);
#43= IFCSIMPLEPROPERTYTEMPLATE('1hKxDz0tb2svD0fl7WeQ2E',$,'FireExit','Indication whether this object is designed to serve as an exit in the case of fire (TRUE) or not (FALSE).\X\0AHere whether the transport element (in case of e.g., a lift) is designed to serve as a fire exit, e.g., for fire escape purposes.',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#44= IFCLIBRARYREFERENCE($,$,'Rettungsweg','Angabe ob dieses Transportelement als Rettungsweg im Brandfall zul\S\dssig ist (WAHR) oder nicht (FALSCH).','de-DE',#2);
#45= IFCRELASSOCIATESLIBRARY('0MoZkgGMP8Og14V8tnKXaO',$,$,$,(#43),#44);
#46= IFCLIBRARYREFERENCE($,$,'SortieSecours','Indication si l''objet est con\S\gu pour servir de sortie en cas d''incendie (VRAI) ou non (FAUX). Cas d''un \S\il\S\iment de transport comme un ascenseur con\S\gu pour l''\S\ivacuation en cas d''incendie.','fr-FR',#2);
#47= IFCRELASSOCIATESLIBRARY('1EDQkTVVD7Zhs6m1jS_Tpr',$,$,$,(#43),#46);
#48= IFCLIBRARYREFERENCE($,$,'\X2\907F96E351FA53E3\X0\','\X2\907F96E351FA53E3\X0\(TRUE)\X2\304B3001901A5E38306E51FA53E3\X0\(FALSE)\X2\304B3092793A305930D530E930B03002\X0\','ja-JP',#2);
#49= IFCRELASSOCIATESLIBRARY('1lCr8QihbDTuAquODefxzX',$,$,$,(#43),#48);
#50= IFCLIBRARYREFERENCE($,$,'\X2\D654C7AC\X0\ \X2\CD9CAD6C\X0\ (\X2\D53CB09C\X0\ \X2\CD9CAD6C\X0\)','\X2\C774\X0\ \X2\BB3CCCB4AC00\X0\ \X2\D654C7ACC758\X0\ \X2\ACBDC6B0\X0\ \X2\CD9CAD6CB85C\X0\ \X2\C0ACC6A9B418B3C4B85D\X0\ \X2\C124ACC4B418C5C8B294C9C0\X0\ \X2\C5ECBD80B97C\X0\ \X2\B098D0C0B0B4B294\X0\ \X2\BD80C6B8\X0\ \X2\AC12C785B2C8B2E4\X0\. \X2\C5ECAE30C5D0\X0\ \X2\ACF5AC04\X0\ (\X2\C608\X0\ \X2\BCF5B3C4\X0\), \X2\C608B97C\X0\ \X2\B4E4BA74\X0\ \X2\D654C7AC\X0\ \X2\D53CB09C\X0\ \X2\BAA9C801C744\X0\ \X2\C704D574\X0\ \X2\CD9CAD6C\X0\ \X2\ACF5AC04C73CB85C\X0\ \X2\C0ACC6A9D558B3C4B85D\X0\ \X2\C124ACC4B418C5C8B294C9C0\X0\ \X2\C5ECBD80\X0\','ko-KR',#2);
#51= IFCRELASSOCIATESLIBRARY('03m8hLrrb9WBXuD4ZuqJrI',$,$,$,(#43),#50);
#52= IFCPROPERTYSETTEMPLATE('1hMcz$YoTDHfUORlf55jaq',$,'Pset_TransportElementElevator','Properties common to the definition of all occurrences of IfcTransportElement with the predefined type ="ELEVATOR"',.PSET_TYPEDRIVENOVERRIDE.,'IfcTransportElement/ELEVATOR',(#59,#66,#71,#76));
#53= IFCLIBRARYREFERENCE($,$,$,'Property Set Definition in German','de-DE',#2);
#54= IFCRELASSOCIATESLIBRARY('30gUNhdTfA$RKllDvh$L9v',$,$,$,(#52),#53);
#55= IFCLIBRARYREFERENCE($,$,$,'D\S\ifinition de l''IAI : propri\S\it\S\is communes \S\` la d\S\ifinition de toutes les instances de la classe IfcTransportElement de type ELEVATOR.','fr-FR',#2);
#56= IFCRELASSOCIATESLIBRARY('0SlKxBtE50OeXYMK9s$DKU',$,$,$,(#52),#55);
#57= IFCLIBRARYREFERENCE($,$,$,'\X2\30BF30A430D7304C65E25B9A7FA9306E\X0\"ELEVATOR"\X2\30673042308B\X0\IfcTransportElement\X2\305930793066306B5171901A306A5C5E6027306E5B9A7FA93002\X0\','ja-JP',#2);
#58= IFCRELASSOCIATESLIBRARY('1H7EkFJfvEG8VJ$johFtHn',$,$,$,(#52),#57);
#59= IFCSIMPLEPROPERTYTEMPLATE('2UVHSC7gv1$P9g39TAiTUz',$,'FireFightingLift','Indication whether the elevator is designed to serve as a fire fighting lift the case of fire (TRUE) or not (FALSE). A fire fighting lift is used by fire fighters to access the location of fire and to evacuate people.',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#60= IFCLIBRARYREFERENCE($,$,'Feuerwehraufzug','Angabe, ob der Aufzug als ein Feuerwerksaufzug vorgesehen ist (WAHR) oder nicht (FALSCH). Ein Feuerwehraufzug ist ein besonders abgesicherter Aufzug der der Feuerwehr im Branfall ein Erreichen der Branetage erm\S\vglicht.','de-DE',#2);
#61= IFCRELASSOCIATESLIBRARY('1OzILyMkT9JOtQwDCA2Riw',$,$,$,(#59),#60);
#62= IFCLIBRARYREFERENCE($,$,'LargeurPassage','Indique si l''ascenseur est con\S\gu pour servir d''ascenseur pompier (VRAI) ou non (FAUX). Un ascenseur pompier est utilis\S\i par les pompiers pour acc\S\ider \S\` l''endroit du feu et \S\ivacuer les personnes.','fr-FR',#2);
#63= IFCRELASSOCIATESLIBRARY('1uTgXZuZn9ZgvuL9mKGNs$',$,$,$,(#59),#62);
#64= IFCLIBRARYREFERENCE($,$,'\X2\6D88963230A830EC30D930FC30BF30FC\X0\','\X2\706B707D6642306B6D88963230A830EC30D930FC30BF30FC306830573066306E52297528309260F35B9A305730668A2D8A083055308C30663044308B304B30693046304B3092793A305930026D88963230A830EC30D930FC30BF30FC306F706B707D73FE583430786D88963258EB3092904B30933060308A4EBA3092907F96E33055305B308B305F3081306B4F7F308F308C308B3002\X0\','ja-JP',#2);
#65= IFCRELASSOCIATESLIBRARY('0D9asJld58lPgTW_5wkqId',$,$,$,(#59),#64);
#66= IFCSIMPLEPROPERTYTEMPLATE('1CztU8x1L2chT0s7fQPpn0',$,'ClearWidth','Clear width of the object (elevator). It indicates the distance from the inner surfaces of the elevator car left and right from the elevator door. \X\0AThe shape information is provided in addition to the shape representation and the geometric parameters used within. In cases of inconsistency between the geometric parameters and the shape properties, provided in the attached property, the geometric parameters take precedence.',.P_SINGLEVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#67= IFCLIBRARYREFERENCE($,$,'\X2\5E4554E1\X0\','\X2\30AA30D630B830A730AF30C8FF0830A830EC30D930FC30BFFF09306E5E45300230A830EC30D930FC30BF6607964D6A5F518590E888689762306E5DE6304B308953F3306E8DDD96E23092793A30593002\X0\\X\0A\X2\5F6272B6886873FE306F3001\X0\Shape representation\X2\FF08\X0\IFC\X2\306E5E7E4F555F6272B6886873FEFF09304A30883073305D305330678A2D5B9A3055308C30663044308B5E7E4F555F6272B630D130E930E130FC30BF306B3088308A4E0E30483089308C308B30023082305730015E7E4F555F6272B630D130E930E130FC30BF30685F6272B630D730ED30D130C630A360C55831304C4E0081F43057306A304458345408306F30015F6272B630D130E930E130FC30BF306E50243092512A51483059308B3002\X0\','ja-JP',#2);
#68= IFCRELASSOCIATESLIBRARY('2hF9oQNvH8f8C4QS$KcJLP',$,$,$,(#66),#67);
#69= IFCLIBRARYREFERENCE($,$,'Largeur du passage','Largeur du passage de l''ascenseur. Elle indique la distance entre les surfaces int\S\irieures gauche et droite de la cabine depuis la porte de l''ascenseur. Cette propri\S\it\S\i est donn\S\ie en compl\S\iment de la repr\S\isentation de la forme de l''\S\il\S\iment et des param\S\htres g\S\iom\S\itriques qui la d\S\iterminent. En cas d''incoh\S\irence entre ces param\S\htres g\S\iom\S\itriques et cette propri\S\it\S\i, ce sont les param\S\htres g\S\iom\S\itriques qui priment.','fr-FR',#2);
#70= IFCRELASSOCIATESLIBRARY('24vyRh36X05BPLVGN$$SRo',$,$,$,(#66),#69);
#71= IFCSIMPLEPROPERTYTEMPLATE('2DUyKOkFv3vgUWu9ZTlNC6',$,'ClearDepth','Clear depth of the object (elevator). It indicates the distance from the inner surface of the elevator door to the opposite surface of the elevator car. \X\0AThe shape information is provided in addition to the shape representation and the geometric parameters used within. In cases of inconsistency between the geometric parameters and the shape properties, provided in the attached property, the geometric parameters take precedence.',.P_SINGLEVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#72= IFCLIBRARYREFERENCE($,$,'\X2\5965884C304D\X0\','\X2\30AA30D630B830A730AF30C8FF0830A830EC30D930FC30BFFF09306E5965884C304D300230A830EC30D930FC30BF30C930A2306E518590E888689762304B3089300153CD5BFE5074306E88689762307E3067306E8DDD96E23092793A30593002\X0\\X\0A\X2\5F6272B6886873FE306F3001\X0\Shape representation\X2\FF08\X0\IFC\X2\306E5E7E4F555F6272B6886873FEFF09304A30883073305D305330678A2D5B9A3055308C30663044308B5E7E4F555F6272B630D130E930E130FC30BF306B3088308A4E0E30483089308C308B30023082305730015E7E4F555F6272B630D130E930E130FC30BF30685F6272B630D730ED30D130C630A360C55831304C4E0081F43057306A304458345408306F30015F6272B630D130E930E130FC30BF306E50243092512A51483059308B3002\X0\','ja-JP',#2);
#73= IFCRELASSOCIATESLIBRARY('19TSOSBLHFdf9bh9f9GPAP',$,$,$,(#71),#72);
#74= IFCLIBRARYREFERENCE($,$,'Profondeur de passage','Profondeur de l''ascenseur. Elle indique la distance entre la face int\S\irieure de la porte et la face oppos\S\ie de la cabine de l''ascenseur. Cette propri\S\it\S\i est donn\S\ie en compl\S\iment de la repr\S\isentation de la forme de l''\S\il\S\iment et des param\S\htres g\S\iom\S\itriques qui la d\S\iterminent. En cas d''incoh\S\irence entre ces param\S\htres g\S\iom\S\itriques et cette propri\S\it\S\i, ce sont les param\S\htres g\S\iom\S\itriques qui priment.','fr-FR',#2);
#75= IFCRELASSOCIATESLIBRARY('3Pv4NdVZT4SxAVvOCDVH17',$,$,$,(#71),#74);
#76= IFCSIMPLEPROPERTYTEMPLATE('32Z7WNng5ATPrzm8nYwGpv',$,'ClearHeight','Clear height of the object (elevator).  \X\0AThe shape information is provided in addition to the shape representation and the geometric parameters used within. In cases of inconsistency between the geometric parameters and the shape properties, provided in the attached property, the geometric parameters take precedence.',.P_SINGLEVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#77= IFCLIBRARYREFERENCE($,$,'\X2\9AD83055\X0\','\X2\30AA30D630B830A730AF30C8FF0830A830EC30D930FC30BFFF09306E9AD83055300230A830EC30D930FC30BF30C930A2306E518590E8306E5E8A9762304B308959294E95307E3067306E8DDD96E23092793A30593002\X0\\X\0A\X2\5F6272B6886873FE306F3001\X0\Shape representation\X2\FF08\X0\IFC\X2\306E5E7E4F555F6272B6886873FEFF09304A30883073305D305330678A2D5B9A3055308C30663044308B5E7E4F555F6272B630D130E930E130FC30BF306B3088308A4E0E30483089308C308B30023082305730015E7E4F555F6272B630D130E930E130FC30BF30685F6272B630D730ED30D130C630A360C55831304C4E0081F43057306A304458345408306F30015F6272B630D130E930E130FC30BF306E50243092512A51483059308B3002\X0\','ja-JP',#2);
#78= IFCRELASSOCIATESLIBRARY('20tlm$UDP8bATh6SiM2kyD',$,$,$,(#76),#77);
#79= IFCLIBRARYREFERENCE($,$,'Hauteur de passage','Hauteur du passage de l''ascenseur. Cette propri\S\it\S\i est donn\S\ie en compl\S\iment de la repr\S\isentation de la forme de l''\S\il\S\iment et des param\S\htres g\S\iom\S\itriques qui la d\S\iterminent. En cas d''incoh\S\irence entre ces param\S\htres g\S\iom\S\itriques et cette propri\S\it\S\i, ce sont les param\S\htres g\S\iom\S\itriques qui priment.','fr-FR',#2);
#80= IFCRELASSOCIATESLIBRARY('0M95oPgBrEz8b6nHS21T_f',$,$,$,(#76),#79);
#81= IFCPROPERTYSETTEMPLATE('39eTyhsT9BOBKkKTcoNDgc',$,'Pset_DistributionPortPHistoryCable','Log of electrical activity attached to an instance of IfcPerformanceHistory having an assigned IfcDistributionPort of type CABLE.',.PSET_PERFORMANCEDRIVEN.,'IfcDistributionPort/ELECTRICAL',(#84,#87,#90,#93,#96,#99,#102,#105));
#82= IFCLIBRARYREFERENCE($,$,$,'IfcDistributionPort\X2\30AA30D630B830A730AF30C8304C\X0\ELECTRICAL\X2\578B306E969B306B95A290233059308B\X0\IfcPerformanceHistory\X2\306B8A2D5B9A3055308C308B96FB529B4F7F7528306E30ED30B03002\X0\','ja-JP',#2);
#83= IFCRELASSOCIATESLIBRARY('18piD0gJz8FOO8hBj21XeN',$,$,$,(#81),#82);
#84= IFCSIMPLEPROPERTYTEMPLATE('3XWRO9tTL5kxTlRrufbwCx',$,'Current','Log of electrical current.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcElectricCurrentMeasure',$,$,$,$,.READWRITE.);
#85= IFCLIBRARYREFERENCE($,$,'\X2\96FB6D41\X0\','\X2\96FB6D41306E30ED30B03002\X0\','ja-JP',#2);
#86= IFCRELASSOCIATESLIBRARY('2WtOSsIKD41AN0s3DN18XU',$,$,$,(#84),#85);
#87= IFCSIMPLEPROPERTYTEMPLATE('0hK0LrcWvCuRsD7bWfUU0e',$,'Voltage','Log of electrical voltage.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcElectricVoltageMeasure',$,$,$,$,.READWRITE.);
#88= IFCLIBRARYREFERENCE($,$,'\X2\96FB5727\X0\','\X2\96FB5727306E30ED30B03002\X0\','ja-JP',#2);
#89= IFCRELASSOCIATESLIBRARY('2wsVJmx0n4Cur_fX1eXsEp',$,$,$,(#87),#88);
#90= IFCSIMPLEPROPERTYTEMPLATE('0$PSec2Lr268I2n5ibakQX',$,'RealPower','Real power.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcPowerMeasure',$,$,$,$,.READWRITE.);
#91= IFCLIBRARYREFERENCE($,$,'\X2\670952B996FB529B\X0\','\X2\670952B996FB529B3002\X0\','ja-JP',#2);
#92= IFCRELASSOCIATESLIBRARY('10uH20v_99yB45eMdsXnTJ',$,$,$,(#90),#91);
#93= IFCSIMPLEPROPERTYTEMPLATE('0Pv248vGb7oPrkTbfi0PIt',$,'ReactivePower','Reactive power.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcPowerMeasure',$,$,$,$,.READWRITE.);
#94= IFCLIBRARYREFERENCE($,$,'\X2\712152B996FB529B\X0\','\X2\712152B996FB529B3002\X0\','ja-JP',#2);
#95= IFCRELASSOCIATESLIBRARY('0zFbfcgtX8rBVDrQf6tYvA',$,$,$,(#93),#94);
#96= IFCSIMPLEPROPERTYTEMPLATE('1Nd9tG_tPBkv46KVlhPxNK',$,'ApparentPower','Apparent power.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcPowerMeasure',$,$,$,$,.READWRITE.);
#97= IFCLIBRARYREFERENCE($,$,'\X2\76AE76F896FB529B\X0\','\X2\76AE76F896FB529B3002\X0\','ja-JP',#2);
#98= IFCRELASSOCIATESLIBRARY('06Rom3ear2zfUZoPXN5Y5y',$,$,$,(#96),#97);
#99= IFCSIMPLEPROPERTYTEMPLATE('3V0TuwdjH05OMzhj0X4dkf',$,'PowerFactor','Power factor.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcRatioMeasure',$,$,$,$,.READWRITE.);
#100= IFCLIBRARYREFERENCE($,$,'\X2\30D130EF30FC30D530A130AF30BF\X0\','\X2\30D130EF30FC30D530A130AF30BF3002\X0\','ja-JP',#2);
#101= IFCRELASSOCIATESLIBRARY('2vX8rqV5v3ofsz_svMDmnM',$,$,$,(#99),#100);
#102= IFCSIMPLEPROPERTYTEMPLATE('3gbWQNSjjEMQQhesZay6Su',$,'DataTransmitted','For data ports, captures log of data transmitted.  The LIST at IfcTimeSeriesValue.Values may split out data according to Pset_DistributionPortTypeCable.Protocols.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcText',$,$,$,$,.READWRITE.);
#103= IFCLIBRARYREFERENCE($,$,'\X2\767A4FE1\X0\','\X2\767A4FE130C730FC30BF306E30ED30B03002\X0\IfcTimeSeriesValue.Values\X2\306E30EA30B930C85024306B306F\X0\Pset_DistributionPortTypeCable.Protocols\X2\3088308A30C730FC30BF309290014FE13059308B3002\X0\','ja',#2);
#104= IFCRELASSOCIATESLIBRARY('2GfXbM$H58pwv1TZVlSKcq',$,$,$,(#102),#103);
#105= IFCSIMPLEPROPERTYTEMPLATE('2I2hCVO8D9yhhaWr8YLFaG',$,'DataReceived','For data ports, captures log of data received.  The LIST at IfcTimeSeriesValue.Values may split out data according to Pset_DistributionPortTypeCable.Protocols.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcText',$,$,$,$,.READWRITE.);
#106= IFCLIBRARYREFERENCE($,$,'\X2\53D74FE1\X0\','\X2\53D74FE130C730FC30BF306E30ED30B03002\X0\IfcTimeSeriesValue.Values\X2\306E30EA30B930C85024306B306F\X0\Pset_DistributionPortTypeCable.Protocols\X2\3088308A30C730FC30BF309253D74FE13059308B3002\X0\','ja',#2);
#107= IFCRELASSOCIATESLIBRARY('0PGOnsrhLDKOfTsjpSURME',$,$,$,(#105),#106);
#108= IFCPROPERTYSETTEMPLATE('0mXyVn$C105vtpw6CCULt9',$,'Pset_ManufacturerOccurrence','Defines properties of individual instances of manufactured products that may be given by the manufacturer.\X\0AHISTORY: IFC 2x4: AssemblyPlace property added. This property does not need to be asserted if Pset_ManufacturerTypeInformation is allocated to the type and the AssemblyPlace property is asserted there.',.PSET_OCCURRENCEDRIVEN.,'IfcElement',(#109,#110,#111,#112,#113));
#109= IFCSIMPLEPROPERTYTEMPLATE('3zw58zp_59LBXJg3vHRhYC',$,'AcquisitionDate','The date that the manufactured item was purchased.',.P_SINGLEVALUE.,'IfcDate','',$,$,$,$,.READWRITE.);
#110= IFCSIMPLEPROPERTYTEMPLATE('3ef4NMLpr1880QuzLWMTuJ',$,'BarCode','The identity of the bar code given to an occurrence of the product.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#111= IFCSIMPLEPROPERTYTEMPLATE('1RgnOJISz7gBaqwnTmIiNC',$,'SerialNumber','The serial number assigned to an occurrence of a product.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#112= IFCSIMPLEPROPERTYTEMPLATE('1CTzoPAHn9LPfCBh8K12Rf',$,'BatchReference','The identity of the batch reference from which an occurrence of a product is taken.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#113= IFCSIMPLEPROPERTYTEMPLATE('2J37Lbboj7F8oWQftL0GFt',$,'AssemblyPlace','Enumeration defining where the assembly is intended to take place, either in a factory, other offsite location or on the building site.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#114,$,$,$,.READWRITE.);
#114= IFCPROPERTYENUMERATION('PEnum_AssemblyPlace',(IFCLABEL('FACTORY'),IFCLABEL('OFFSITE'),IFCLABEL('SITE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#115= IFCPROPERTYSETTEMPLATE('0G20z5PFL62PCH1DDt2Ab2',$,'Pset_ManufacturerTypeInformation','Defines characteristics of types (ranges) of manufactured products that may be given by the manufacturer. Note that the term ''manufactured'' may also be used to refer to products that are supplied and identified by the supplier or that are assembled off site by a third party provider. \X\0AHISTORY: This property set replaces the entity IfcManufacturerInformation from previous IFC releases. IFC 2x4: AssemblyPlace property added.',.PSET_TYPEDRIVENOVERRIDE.,'IfcElement',(#116,#117,#118,#119,#120,#121,#122));
#116= IFCSIMPLEPROPERTYTEMPLATE('1xErr5V615b82HTlBvi0PS',$,'GlobalTradeItemNumber','The Global Trade Item Number (GTIN) is an identifier for trade items developed by GS1 (www.gs1.org).',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#117= IFCSIMPLEPROPERTYTEMPLATE('0tSy5PGqnCUeOt2D0DGgev',$,'ArticleNumber','Article number or reference that is be applied to a configured product according to a standard scheme for article number definition as defined by the manufacturer. It is often used as the purchasing number.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#118= IFCSIMPLEPROPERTYTEMPLATE('03aFVO1Kr6BRrfXPW6uySJ',$,'ModelReference','The model number or designator of the product model (or product line) as assigned by the manufacturer of the manufactured item.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#119= IFCSIMPLEPROPERTYTEMPLATE('0PeVg8yzv07gGsnhttW0SD',$,'ModelLabel','The descriptive model name of the product model (or product line) as assigned by the manufacturer of the manufactured item.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#120= IFCSIMPLEPROPERTYTEMPLATE('0e2HnJl5v1xhxBtxIe8dF$',$,'Manufacturer','The organization that manufactured and/or assembled the item.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#121= IFCSIMPLEPROPERTYTEMPLATE('1$wjj_37PEMwSsxv2MTzFb',$,'ProductionYear','The year of production of the manufactured item.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#122= IFCSIMPLEPROPERTYTEMPLATE('2AmeEcx9X1ixOaO3qRi9a2',$,'AssemblyPlace','Enumeration defining where the assembly is intended to take place, either in a factory or on the building site.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#123,$,$,$,.READWRITE.);
#123= IFCPROPERTYENUMERATION('PEnum_AssemblyPlace',(IFCLABEL('FACTORY'),IFCLABEL('OFFSITE'),IFCLABEL('SITE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#124= IFCPROPERTYSETTEMPLATE('1lDvcPgXDAnPbe5ITnGYPd',$,'Pset_ActuatorPHistory','Properties for history of actuators. HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcActuator',(#127,#132,#137));
#125= IFCLIBRARYREFERENCE($,$,$,'\X2\30A230AF30C130E530A830FC30BF306E602780FD5C656B74306E5C5E60273002\X0\IFC4\X2\306B30668FFD52A03002\X0\','ja-JP',#2);
#126= IFCRELASSOCIATESLIBRARY('1DpWaa9NzEn8pl0YpfgNYq',$,$,$,(#124),#125);
#127= IFCSIMPLEPROPERTYTEMPLATE('1pW7Mw0tT0r82DOW4i6IIv',$,'Position','Indicates position of the actuator over time where 0.0 is fully closed and 1.0 is fully open.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcNormalisedRatioMeasure',$,$,$,$,.READWRITE.);
#128= IFCLIBRARYREFERENCE($,$,'\X2\4F4D7F6E\X0\','\X2\30A230AF30C130E530A830FC30BF306E6642959330543068306E4F4D7F6E3092793A305950243002\X0\0.0\X2\304C5B8C5168306B958930583089308C305F72B6614B30673001\X0\1.0\X2\304C5B8C5168306B958B3044305F72B6614B3002\X0\','ja-JP',#2);
#129= IFCRELASSOCIATESLIBRARY('3sw_mAYCnCewgIJAvt4kEr',$,$,$,(#127),#128);
#130= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#131= IFCRELASSOCIATESLIBRARY('30YhymUtb7lOInPZA7WeAn',$,$,$,(#127),#130);
#132= IFCSIMPLEPROPERTYTEMPLATE('3Kt6PkYRH8xeqtjFfpSnUn',$,'Quality','Indicates the quality of measurement or failure condition, which may be further qualified by the Status.  True: measured values are considered reliable; False: measured values are considered not reliable (i.e. a fault has been detected); Unknown: reliability of values is uncertain.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#133= IFCLIBRARYREFERENCE($,$,'\X2\54C18CEA\X0\','\X2\8A086E2C306E54C18CEA3092793A305950243002\X0\','ja-JP',#2);
#134= IFCRELASSOCIATESLIBRARY('2MKhHLLUH3u9TrMm5zw169',$,$,$,(#132),#133);
#135= IFCLIBRARYREFERENCE($,$,'\X2\D398C77C\X0\ \X2\C138C774D504\X0\ \X2\C720D615\X0\','\X2\C694CCADD55C\X0\ \X2\C561CE04C5D0C774D130C758\X0\ \X2\C548C804\X0\ \X2\C7A5CE58\X0\ \X2\C720D615C744\X0\ \X2\D45CC2DC\X0\','ko-KR',#2);
#136= IFCRELASSOCIATESLIBRARY('1zxlMwOqn289GmaoXBl7c$',$,$,$,(#132),#135);
#137= IFCSIMPLEPROPERTYTEMPLATE('1E4Q$SXGv7VhFh1XPCXpd8',$,'Status','Indicates an error code or identifier, whose meaning is specific to the particular automation system.  Example values include: ''ConfigurationError'', ''NotConnected'', ''DeviceFailure'', ''SensorFailure'', ''LastKnown, ''CommunicationsFailure'', ''OutOfService''.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLabel',$,$,$,$,.READWRITE.);
#138= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\30A830E930FC30B330FC30C9307E305F306F\X0\ID\X2\3092793A305930024F8BFF1A\X0\''ConfigurationError'', ''NotConnected'', ''DeviceFailure'', ''SensorFailure'', ''LastKnown, ''CommunicationsFailure'', ''OutOfService''.','ja-JP',#2);
#139= IFCRELASSOCIATESLIBRARY('0a3kK0fuv0L98HnPS2_qxy',$,$,$,(#137),#138);
#140= IFCLIBRARYREFERENCE($,$,'\X2\C7ACC815\X0\ \X2\AE30B2A5C758\X0\ \X2\C720BB34\X0\','\X2\B300CCB4\X0\ \X2\AE30B2A5C73CB85C\X0\ \X2\C218B3D9\X0\ \X2\C870C791C774\X0\ \X2\C81CACF5B418B294C9C0\X0\ (= TRUE) \X2\C5ECBD80\X0\ (= FALSE)\X2\B97C\X0\ \X2\D655C778D55CB2E4\X0\. \X2\C218B3D9C73CB85C\X0\ \X2\C870C791D558B294\X0\ \X2\C561CE04C5D0C774D130C758\X0\ \X2\ACBDC6B0B294C774\X0\ \X2\AC12C744\X0\ \X2\AE30BCF8AC12C73CB85C\X0\ FALSE\X2\B85C\X0\ \X2\C124C815D574C57CD558BBC0B85CC8FCC758D55CB2E4\X0\.','ko-KR',#2);
#141= IFCRELASSOCIATESLIBRARY('3nXH4yXUL6c8iM$6rzepce',$,$,$,(#137),#140);
#142= IFCPROPERTYSETTEMPLATE('1WIr_Qme9ATBIp12xr12xm',$,'Pset_ActuatorTypeCommon','Actuator type common attributes.',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator',(#145,#150,#156,#162,#165));
#143= IFCLIBRARYREFERENCE($,$,$,'\X2\30A230AF30C130E530A830FC30BF30BF30A430D7306E5171901A5C5E60273002\X0\','ja-JP',#2);
#144= IFCRELASSOCIATESLIBRARY('2TfCnY2vjArg93sxJlh2Ry',$,$,$,(#142),#143);
#145= IFCSIMPLEPROPERTYTEMPLATE('2BfmU0d3jC$hOfUb63pYjB',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#146= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#147= IFCRELASSOCIATESLIBRARY('2dJvsMMpbDSA4yWlBOixqm',$,$,$,(#145),#146);
#148= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#149= IFCRELASSOCIATESLIBRARY('0gaf1KOnj7_B4nKsjHW8cM',$,$,$,(#145),#148);
#150= IFCSIMPLEPROPERTYTEMPLATE('1FWJhCPOvBmuI4IJIBzQsj',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#151,$,$,$,.READWRITE.);
#151= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#152= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#153= IFCRELASSOCIATESLIBRARY('1sciosCir6k826O4KxBtv9',$,$,$,(#150),#152);
#154= IFCLIBRARYREFERENCE($,$,'\X2\D398C77C\X0\ \X2\C138C774D504\X0\ \X2\C720D615\X0\','\X2\C694CCADD55C\X0\ \X2\C561CE04C5D0C774D130C758\X0\ \X2\C548C804\X0\ \X2\C7A5CE58\X0\ \X2\C720D615C744\X0\ \X2\D45CC2DC\X0\','ko-KR',#2);
#155= IFCRELASSOCIATESLIBRARY('022Mk22D5CI90HV4buYtpU',$,$,$,(#150),#154);
#156= IFCSIMPLEPROPERTYTEMPLATE('09LQxUbxL6_AdfuzimzRsX',$,'FailPosition','Specifies the required fail-safe position of the actuator.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#157,$,$,$,.READWRITE.);
#157= IFCPROPERTYENUMERATION('PEnum_FailPosition',(IFCLABEL('FAILOPEN'),IFCLABEL('FAILCLOSED'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#158= IFCLIBRARYREFERENCE($,$,'\X2\30D530A730FC30EB30BB30FC30D530BF30A430D7\X0\','\X2\89816C423055308C305F30A230AF30C130E530A830FC30BF306E30D530A730FC30EB30BB30FC30D530BF30A430D73092793A30593002\X0\','ja-JP',#2);
#159= IFCRELASSOCIATESLIBRARY('2AilFIgTP56eQk6jeJEShw',$,$,$,(#156),#158);
#160= IFCLIBRARYREFERENCE($,$,'\X2\C7ACC815\X0\ \X2\AE30B2A5C758\X0\ \X2\C720BB34\X0\','\X2\B300CCB4\X0\ \X2\AE30B2A5C73CB85C\X0\ \X2\C218B3D9\X0\ \X2\C870C791C774\X0\ \X2\C81CACF5B418B294C9C0\X0\ (= TRUE) \X2\C5ECBD80\X0\ (= FALSE)\X2\B97C\X0\ \X2\D655C778D55CB2E4\X0\. \X2\C218B3D9C73CB85C\X0\ \X2\C870C791D558B294\X0\ \X2\C561CE04C5D0C774D130C758\X0\ \X2\ACBDC6B0B294C774\X0\ \X2\AC12C744\X0\ \X2\AE30BCF8AC12C73CB85C\X0\ FALSE\X2\B85C\X0\ \X2\C124C815D574C57CD558BBC0B85CC8FCC758D55CB2E4\X0\.','ko-KR',#2);
#161= IFCRELASSOCIATESLIBRARY('3Go9cd0Tv6MBvZFkV9KH$S',$,$,$,(#156),#160);
#162= IFCSIMPLEPROPERTYTEMPLATE('0st3snlyzB0QhSHR70l$q7',$,'ManualOverride','Identifies whether hand-operated operation is provided as an override (= TRUE) or not (= FALSE). Note that this value should be set to FALSE by default in the case of a Hand Operated Actuator.',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#163= IFCLIBRARYREFERENCE($,$,'\X2\30AA30FC30D030FC30E930A430C96A5F80FD306E67097121\X0\','\X2\30AA30FC30D030FC30E930A430C96A5F80FD306830573066624B52D564CD4F5C304C63D04F9B3055308C308B304B\X0\ (= TRUE) \X2\30015426304B\X0\ \X2\FF08\X0\= FALSE)\X2\30928B5852253059308B3002624B52D5306764CD4F5C3059308B30A230AF30C130E530A830FC30BF306E58345408306F30013053306E5024309230C730D530A930EB30C8306830573066\X0\FALSE\X2\306B8A2D5B9A3059308B5FC58981304C3042308B306E30676CE8610F3059308B305330683002\X0\','ja-JP',#2);
#164= IFCRELASSOCIATESLIBRARY('2BgRhcBf9AYPTqzhinCZ87',$,$,$,(#162),#163);
#165= IFCSIMPLEPROPERTYTEMPLATE('2FTreXd7fFbBZqJBzZ$qTv',$,'Application','Indicates application of actuator.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#166,$,$,$,.READWRITE.);
#166= IFCPROPERTYENUMERATION('PEnum_ActuatorApplication',(IFCLABEL('EntryExitDevice'),IFCLABEL('\X\0AFireSmokeDamperActuator'),IFCLABEL('\X\0ADamperActuator'),IFCLABEL('\X\0AValvePositioner'),IFCLABEL('\X\0ALampActuator'),IFCLABEL('\X\0ASunblindActuator'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#167= IFCPROPERTYSETTEMPLATE('2mUR3PtfT1fO5XnyKQhneL',$,'Pset_ActuatorTypeElectricActuator','A device that electrically actuates a control element.',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator/ELECTRICACTUATOR',(#170,#175));
#168= IFCLIBRARYREFERENCE($,$,$,'\X2\52365FA189817D20309296FB6C177684306B4F5C52D53055305B308B30C730D030A430B93002\X0\','ja-JP',#2);
#169= IFCRELASSOCIATESLIBRARY('0UyXZRzcX0XwBhPAIf83V9',$,$,$,(#167),#168);
#170= IFCSIMPLEPROPERTYTEMPLATE('0fefofZcD0j9VNSAB9IveK',$,'ActuatorInputPower','Maximum input power requirement.',.P_SINGLEVALUE.,'IfcPowerMeasure','',$,$,$,$,.READWRITE.);
#171= IFCLIBRARYREFERENCE($,$,'\X2\5165529B96FB529B\X0\','\X2\670059275165529B96FB529B3002\X0\','ja-JP',#2);
#172= IFCRELASSOCIATESLIBRARY('1MRIbaSSL0vhI4EGkVcJu6',$,$,$,(#170),#171);
#173= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\ \X2\C804B825\X0\','\X2\CD5CB300\X0\ \X2\C785B825\X0\ \X2\C804B825\X0\','ko-KR',#2);
#174= IFCRELASSOCIATESLIBRARY('0M1ruAIWX77eo7mLg2EFHU',$,$,$,(#170),#173);
#175= IFCSIMPLEPROPERTYTEMPLATE('363Ahgfjz8hRE2xXK92OB4',$,'ElectricActuatorType','Enumeration that identifies electric actuator as defined by its operational principle.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#176,$,$,$,.READWRITE.);
#176= IFCPROPERTYENUMERATION('PEnum_ElectricActuatorType',(IFCLABEL('MOTORDRIVE'),IFCLABEL('MAGNETIC'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#177= IFCLIBRARYREFERENCE($,$,'\X2\96FB6C175F0F30A230AF30C130E530A830FC30BF30BF30A430D7\X0\','\X2\4F5C52D5539F7406306B3088306330665B9A7FA93055308C305F96FB6C175F0F30A230AF30C130E530A830FC30BF30928B5852253059308B4E0089A73002\X0\','ja-JP',#2);
#178= IFCRELASSOCIATESLIBRARY('22j1vDD4b9KgM13OeX952X',$,$,$,(#175),#177);
#179= IFCLIBRARYREFERENCE($,$,'\X2\C804AE30C2DD\X0\ \X2\C561CD94C5D0C774D130\X0\ \X2\C720D615\X0\','\X2\C791B3D9\X0\ \X2\C6D0B9ACC5D0\X0\ \X2\C758D574\X0\ \X2\C815C758B41C\X0\ \X2\C804AE30C2DD\X0\ \X2\C561CE04C5D0C774D130B97C\X0\ \X2\C2DDBCC4D558B294\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#180= IFCRELASSOCIATESLIBRARY('0Wybi0$7D9swazCtogDfJQ',$,$,$,(#175),#179);
#181= IFCPROPERTYSETTEMPLATE('3vvVpVcNv6GwRDDVupFh20',$,'Pset_ActuatorTypeHydraulicActuator','A device that hydraulically actuates a control element.',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator/HYDRAULICACTUATOR',(#184,#189));
#182= IFCLIBRARYREFERENCE($,$,$,'\X2\52365FA189817D2030926C345727FF086CB95727FF0930674F5C52D53055305B308B30C730D030A430B93002\X0\','ja-JP',#2);
#183= IFCRELASSOCIATESLIBRARY('0SE$ji93v8N9curq6ZuX_F',$,$,$,(#181),#182);
#184= IFCSIMPLEPROPERTYTEMPLATE('2XoVs9gmT9fgjbt4lESsgp',$,'InputPressure','Maximum design pressure for the actuator.',.P_SINGLEVALUE.,'IfcPressureMeasure','',$,$,$,$,.READWRITE.);
#185= IFCLIBRARYREFERENCE($,$,'\X2\5165529B5727529B\X0\','\X2\30A230AF30C130E530A830FC30BF3078306E670059278A2D8A085727529B3002\X0\','ja-JP',#2);
#186= IFCRELASSOCIATESLIBRARY('1X0TJTmWr4DeBlMDE5Iyv1',$,$,$,(#184),#185);
#187= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\ \X2\C555B825\X0\','\X2\C561CE04C5D0C774D130C758\X0\ \X2\CD5CB300\X0\ \X2\C124ACC4\X0\ \X2\C555B825\X0\','ko-KR',#2);
#188= IFCRELASSOCIATESLIBRARY('2$0p7Is_T4JR8W70Gt2vn2',$,$,$,(#184),#187);
#189= IFCSIMPLEPROPERTYTEMPLATE('2ngFI6i35CDxvUFDVSkTCp',$,'InputFlowrate','Maximum hydraulic flowrate requirement.',.P_SINGLEVALUE.,'IfcVolumetricFlowRateMeasure','',$,$,$,$,.READWRITE.);
#190= IFCLIBRARYREFERENCE($,$,'\X2\5165529B6D4191CF\X0\','\X2\670059276D4191CF3002\X0\','ja-JP',#2);
#191= IFCRELASSOCIATESLIBRARY('14aF6ZBu18L9F1h_e9ZGA3',$,$,$,(#189),#190);
#192= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\ \X2\C720B7C9\X0\','\X2\CD5CB300\X0\ \X2\C720B7C9\X0\','ko-KR',#2);
#193= IFCRELASSOCIATESLIBRARY('0cbOM$qMn3XA9wkWm0yLtb',$,$,$,(#189),#192);
#194= IFCPROPERTYSETTEMPLATE('1M45ce5DD3F8h$tXGP8rpn',$,'Pset_ActuatorTypeLinearActuation','Characteristics of linear actuation of an actuator\X\0AHistory: Replaces Pset_LinearActuator',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator',(#197,#202));
#195= IFCLIBRARYREFERENCE($,$,$,'\X2\30A230AF30C130E530A830FC30BF306E76F47DDA52D54F5C306E727960273002\X0\','ja-JP',#2);
#196= IFCRELASSOCIATESLIBRARY('3E2fsnH1j5XeOYIKeE2ziX',$,$,$,(#194),#195);
#197= IFCSIMPLEPROPERTYTEMPLATE('1_huS9l1DBnP4Roeci4JJC',$,'Force','Indicates the maximum close-off force for the actuator.',.P_SINGLEVALUE.,'IfcForceMeasure','',$,$,$,$,.READWRITE.);
#198= IFCLIBRARYREFERENCE($,$,'\X2\6700592763A8529B\X0\','\X2\30A230AF30C130E530A830FC30BF306E670059277DE030815207308A529B3092793A30593002\X0\','ja-JP',#2);
#199= IFCRELASSOCIATESLIBRARY('0g3rYJidX6iPNy9bJic5XR',$,$,$,(#197),#198);
#200= IFCLIBRARYREFERENCE($,$,'\X2\CD5CB300CD94B825\X0\','\X2\C561CE04C5D0C774D130C758\X0\ \X2\CD5CB300\X0\ \X2\B9C8AC10\X0\ \X2\D798C744\X0\ \X2\BCF4C5ECC900B2E4\X0\.','ko-KR',#2);
#201= IFCRELASSOCIATESLIBRARY('19Fe3D_DL9Z8hhc63hcdlX',$,$,$,(#197),#200);
#202= IFCSIMPLEPROPERTYTEMPLATE('2np53ip15FNganiOiPah5M',$,'Stroke','Indicates the maximum distance the actuator must traverse.',.P_SINGLEVALUE.,'IfcLengthMeasure','',$,$,$,$,.READWRITE.);
#203= IFCLIBRARYREFERENCE($,$,'\X2\30B930C830ED30FC30AF\X0\','\X2\30A230AF30C130E530A830FC30BF304C52D5304F670059278DDD96E23092793A30593002\X0\','ja-JP',#2);
#204= IFCRELASSOCIATESLIBRARY('1lWVOcHmL0hOuprwCQd_yI',$,$,$,(#202),#203);
#205= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\','\X2\C561CE04C5D0C774D130AC00\X0\ \X2\C6C0C9C1C774B294\X0\ \X2\CD5CB300\X0\ \X2\AC70B9ACB97C\X0\ \X2\BCF4C5ECC900B2E4\X0\.','ko-KR',#2);
#206= IFCRELASSOCIATESLIBRARY('0ShzHUlkr4Yv4WePJ4OTdE',$,$,$,(#202),#205);
#207= IFCPROPERTYSETTEMPLATE('28$VLXpLX4KfZX$hkeCOVV',$,'Pset_ActuatorTypePneumaticActuator','A device that pneumatically actuates a control element',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator/PNEUMATICACTUATOR',(#210,#215));
#208= IFCLIBRARYREFERENCE($,$,$,'\X2\52365FA189817D2030927A7A6C17572730674F5C52D53055305B308B30C730D030A430B93002\X0\','ja-JP',#2);
#209= IFCRELASSOCIATESLIBRARY('3qqEADalj8d9q$WAxTnIY9',$,$,$,(#207),#208);
#210= IFCSIMPLEPROPERTYTEMPLATE('3GneTQmwH7kO5qWM5Qf9j0',$,'InputPressure','Maximum input control air pressure requirement.',.P_SINGLEVALUE.,'IfcPressureMeasure','',$,$,$,$,.READWRITE.);
#211= IFCLIBRARYREFERENCE($,$,'\X2\5165529B5727529B\X0\','\X2\6700592752365FA17A7A6C1757273002\X0\','ja-JP',#2);
#212= IFCRELASSOCIATESLIBRARY('1znkhQrhj4d9G0M6_k$hUw',$,$,$,(#210),#211);
#213= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\ \X2\C555B825\X0\','\X2\CD5CB300\X0\ \X2\C81CC5B4\X0\ \X2\ACF5C555\X0\','ko-KR',#2);
#214= IFCRELASSOCIATESLIBRARY('34k8fJhrvFNxCQG5By3iF0',$,$,$,(#210),#213);
#215= IFCSIMPLEPROPERTYTEMPLATE('2zbtUFTS53YBNWqVFq0bhj',$,'InputFlowrate','Maximum input control air flowrate requirement.',.P_SINGLEVALUE.,'IfcVolumetricFlowRateMeasure','',$,$,$,$,.READWRITE.);
#216= IFCLIBRARYREFERENCE($,$,'\X2\5165529B6D4191CF\X0\','\X2\6700592752365FA17A7A6C176D4191CF3002\X0\','ja-JP',#2);
#217= IFCRELASSOCIATESLIBRARY('3vzl_eBKb6GB6uAKAV_AtK',$,$,$,(#215),#216);
#218= IFCLIBRARYREFERENCE($,$,'\X2\C785B825\X0\ \X2\C720B7C9\X0\','\X2\CD5CB300\X0\ \X2\C81CC5B4\X0\ \X2\ACF5AE30\X0\ \X2\C720B7C9\X0\','ko-KR',#2);
#219= IFCRELASSOCIATESLIBRARY('1CukiGd3HC2ex0sV_7cwCC',$,$,$,(#215),#218);
#220= IFCPROPERTYSETTEMPLATE('11KiexmGr299OEqjq_0L11',$,'Pset_ActuatorTypeRotationalActuation','Characteristics of rotational actuation of an actuator\X\0AHistory: Replaces Pset_RotationalActuator',.PSET_TYPEDRIVENOVERRIDE.,'IfcActuator',(#223,#228));
#221= IFCLIBRARYREFERENCE($,$,$,'\X2\30A230AF30C130E530A830FC30BF306E56DE8EE252D54F5C306E727960273002\X0\','ja-JP',#2);
#222= IFCRELASSOCIATESLIBRARY('1X0V3o$An7xeonW5_KT$f6',$,$,$,(#220),#221);
#223= IFCSIMPLEPROPERTYTEMPLATE('3O5TL5PGLFpfIn1$3wmj9V',$,'Torque','Indicates the maximum close-off torque for the actuator.',.P_SINGLEVALUE.,'IfcTorqueMeasure','',$,$,$,$,.READWRITE.);
#224= IFCLIBRARYREFERENCE($,$,'\X2\6700592730C830EB30AF\X0\','\X2\30A230AF30C130E530A830FC30BF306E670059277DE030815207308A30C830EB30AF3092793A30593002\X0\','ja-JP',#2);
#225= IFCRELASSOCIATESLIBRARY('34l8oH1MX5EBEaC2vEjQJe',$,$,$,(#223),#224);
#226= IFCLIBRARYREFERENCE($,$,'\X2\CD5CB300\X0\ \X2\D1A0D06C\X0\','\X2\C561CE04C5D0C774D130C758\X0\ \X2\CD5CB300\X0\ \X2\B9C8AC10\X0\ \X2\D1A0D06CB97C\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#227= IFCRELASSOCIATESLIBRARY('2817M2YyjFxwaNCMXNNyDw',$,$,$,(#223),#226);
#228= IFCSIMPLEPROPERTYTEMPLATE('0L0Yj2JuDD1eofpguDTSCW',$,'RangeAngle','Indicates the maximum rotation the actuator must traverse.',.P_SINGLEVALUE.,'IfcPlaneAngleMeasure','',$,$,$,$,.READWRITE.);
#229= IFCLIBRARYREFERENCE($,$,'\X2\6700592756DE8EE289D2\X0\','\X2\30A230AF30C130E530A830FC30BF304C52D5304F6700592756DE8EE289D23092793A30593002\X0\','ja-JP',#2);
#230= IFCRELASSOCIATESLIBRARY('1YEurTEk10qwasBgzo4PvL',$,$,$,(#228),#229);
#231= IFCLIBRARYREFERENCE($,$,'\X2\CD5CB300\X0\ \X2\D68CC804AC01\X0\','\X2\C561CE04C5D0C774D130AC00\X0\ \X2\C6C0C9C1C774B294\X0\ \X2\CD5CB300\X0\ \X2\D68CC804AC01C744\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#232= IFCRELASSOCIATESLIBRARY('1eKFDdjXH2axcVmbstoUL0',$,$,$,(#228),#231);
#233= IFCPROPERTYSETTEMPLATE('3CXRCVnML2g9_YjQhG$LvI',$,'Pset_AlarmPHistory','Properties for history of alarm values.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcAlarm',(#234,#235,#236,#237,#238));
#234= IFCSIMPLEPROPERTYTEMPLATE('00MFZvT8jE$wCRj1FopG3x',$,'Enabled','Indicates whether alarm is enabled or disabled over time.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcBoolean',$,$,$,$,.READWRITE.);
#235= IFCSIMPLEPROPERTYTEMPLATE('2PqwXUmWnD1OPSwYlBmSVL',$,'Condition','Indicates alarm condition over time.  The range of possible values and their meanings is defined by Pset_AlarmTypeCommon.Condition.  An empty value indicates no present alarm condition.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcIdentifier',$,$,$,$,.READWRITE.);
#236= IFCSIMPLEPROPERTYTEMPLATE('00BjUz1bn5dAGxoaIbW5dL',$,'Severity','Indicates alarm severity over time, where the scale of values is determined by the control system configuration.  A zero value indicates no present alarm.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcInteger',$,$,$,$,.READWRITE.);
#237= IFCSIMPLEPROPERTYTEMPLATE('36FBa_td51luhE0HXdzbfp',$,'Acknowledge','Indicates acknowledgement status where False indicates acknowlegement is required and outstanding, True indicates condition has been acknowedged, and Unknown indicates no acknowledgement is required.  Upon resetting the condition, then acknowledgement reverts to Unknown.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#238= IFCSIMPLEPROPERTYTEMPLATE('0tOI7CI6H99uxiuMGvHe$3',$,'User','Indicates acknowledging user over time by identification corresponding to IfcPerson.Identification on an IfcActor.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcIdentifier',$,$,$,$,.READWRITE.);
#239= IFCPROPERTYSETTEMPLATE('3IuJJnxpj5EwZn3s7Modjr',$,'Pset_AlarmTypeCommon','Alarm type common attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcAlarm',(#242,#247,#251));
#240= IFCLIBRARYREFERENCE($,$,$,'\X2\30A230E930FC30E030BF30A430D7306E5171901A5C5E60273002\X0\','ja-JP',#2);
#241= IFCRELASSOCIATESLIBRARY('3AXkB9DQb0AxD0MFWfsKfx',$,$,$,(#239),#240);
#242= IFCSIMPLEPROPERTYTEMPLATE('0CkuA2$AvCLASCD0KURR6U',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#243= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#244= IFCRELASSOCIATESLIBRARY('2KIw57vo938w41ojBdK4lo',$,$,$,(#242),#243);
#245= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#246= IFCRELASSOCIATESLIBRARY('0JVm7E6yr3hBkkKx00RFuv',$,$,$,(#242),#245);
#247= IFCSIMPLEPROPERTYTEMPLATE('3aYrXwhA17JPX$KO5Isg6r',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#248,$,$,$,.READWRITE.);
#248= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#249= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#250= IFCRELASSOCIATESLIBRARY('0UDnMrgHD0h8vzrJUEEitj',$,$,$,(#247),#249);
#251= IFCSIMPLEPROPERTYTEMPLATE('0ETyTTbFHAevS_2HDlpyp2',$,'Condition','Table mapping alarm condition identifiers to descriptive labels, which may be used for interpreting Pset_AlarmPHistory.Condition.',.P_TABLEVALUE.,'IfcIdentifier','IfcLabel',$,$,$,$,.READWRITE.);
#252= IFCLIBRARYREFERENCE($,$,'\X2\67614EF6\X0\','Pset_AlarmPHistory.Condition\X2\30674F7F75283055308C308B30018B66583167614EF6306E8B5852255B50306830E930D930EB60C55831306E30DE30C330D430F330B03092884C30463002\X0\','ja-JP',#2);
#253= IFCRELASSOCIATESLIBRARY('3ItsjVWLvE2RIarF18eNLF',$,$,$,(#251),#252);
#254= IFCPROPERTYSETTEMPLATE('0ir2YV6BH0QQIMak4fESaT',$,'Pset_ControllerPHistory','Properties for history of controller values.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcController',(#257,#262,#265));
#255= IFCLIBRARYREFERENCE($,$,$,'\X2\30B330F330C830ED30FC30E9306E602780FD5C656B745C5E60273002\X0\\X\0AIFC4 \X2\306B306665B0898F8FFD52A03002\X0\','ja-JP',#2);
#256= IFCRELASSOCIATESLIBRARY('3wsE2LawPE8eEtdOscTPcu',$,$,$,(#254),#255);
#257= IFCSIMPLEPROPERTYTEMPLATE('04QeecgPjAIufWycGnjV0L',$,'Value','Indicates values over time which may be recorded continuously or only when changed beyond a particular deadband.  The range of possible values is defined by the Value property on the corresponding occurrence property set (Pset_ControllerTypeFloating, Pset_ControllerTypeProportional, Pset_ControllerTypeMultiPosition, or Pset_ControllerTypeTwoPosition).',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcReal',$,$,$,$,.READWRITE.);
#258= IFCLIBRARYREFERENCE($,$,'\X2\30C730D530A930EB30C851FA529B66427CFB52175B9A6570\X0\','\X2\66429593306830683082306B50243092793A30593002\X0\\X\0APset_ControllerTypeValue.Value\X2\306B5BFE5FDC\X0\\X\0A\X2\203B\X0\ \X2\8A2D5B9A53EF80FD60C55831306F\X0\ IfcTimeSeries\X2\30D730ED30D130C630A353C27167\X0\','ja-JP',#2);
#259= IFCRELASSOCIATESLIBRARY('0N8RRZKtnE6vcGo7wsy4GN',$,$,$,(#257),#258);
#260= IFCLIBRARYREFERENCE($,$,'\X2\C774C0C1\X0\ \X2\CD9CB825\X0\ \X2\C2DCACC4C5F4\X0\ \X2\C0C1C218\X0\','\X2\C2DCAC04C774\X0\ \X2\C9C0B0A8C5D0\X0\ \X2\C624B958\X0\ \X2\C0C1D0DCB97C\X0\ \X2\B098D0C0B0B4B294\X0\ Pset_ControllerTypeValue.Fault\X2\C5D0\X0\ \X2\B300C751\X0\ \X2\203B\X0\ \X2\C124C815\X0\ \X2\AC00B2A5D55C\X0\ \X2\C815BCF4B294\X0\ IfcTimeSeries \X2\C18DC131\X0\ \X2\CC38C870\X0\','ko-KR',#2);
#261= IFCRELASSOCIATESLIBRARY('1Z7PGEnFnCvP$W6Geq19Lw',$,$,$,(#257),#260);
#262= IFCSIMPLEPROPERTYTEMPLATE('0xnq6Qlfv8CubPPsQw7oM7',$,'Quality','Indicates the quality of measurement or failure condition, which may be further qualified by the Status.  True: measured values are considered reliable; False: measured values are considered not reliable (i.e. a fault has been detected); Unknown: reliability of values is uncertain.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#263= IFCLIBRARYREFERENCE($,$,'\X2\AE30BCF8\X0\ \X2\CD9CB825\X0\ \X2\C2DCACC4C5F4\X0\ \X2\C0C1C218\X0\','\X2\C2DCAC04C774\X0\ \X2\C9C0B0A8C5D0\X0\ \X2\AC12C744\X0\ \X2\B098D0C0B0B4B294\X0\ Pset_ControllerTypeValue.Value\X2\C5D0\X0\ \X2\B300C751\X0\ \X2\203B\X0\ \X2\C124C815\X0\ \X2\AC00B2A5D55C\X0\ \X2\C815BCF4B294\X0\ IfcTimeSeries \X2\C18DC131\X0\ \X2\CC38C870\X0\','ko-KR',#2);
#264= IFCRELASSOCIATESLIBRARY('2rB0tMDaf7OR3kde$w5K88',$,$,$,(#262),#263);
#265= IFCSIMPLEPROPERTYTEMPLATE('2AzN9C2f98y8azdu6mLwxB',$,'Status','Indicates an error code or identifier, whose meaning is specific to the particular automation system.  Example values include: ''ConfigurationError'', ''NotConnected'', ''DeviceFailure'', ''SensorFailure'', ''LastKnown, ''CommunicationsFailure'', ''OutOfService''.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLabel',$,$,$,$,.READWRITE.);
#266= IFCPROPERTYSETTEMPLATE('2QkUxljjrDgQ8ZnhtlXyv8',$,'Pset_ControllerTypeCommon','Controller type common attributes.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController',(#269,#274));
#267= IFCLIBRARYREFERENCE($,$,$,'\X2\30B330F330C830ED30FC30E95171901A5C5E60273002\X0\','ja-JP',#2);
#268= IFCRELASSOCIATESLIBRARY('1B1PsDdRD8S8dEN_Wxshud',$,$,$,(#266),#267);
#269= IFCSIMPLEPROPERTYTEMPLATE('32xbrDDz1BWfTU0h7d6O5h',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#270= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#271= IFCRELASSOCIATESLIBRARY('35XtubqvXCzO5j6x45eFXt',$,$,$,(#269),#270);
#272= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#273= IFCRELASSOCIATESLIBRARY('2QwVyxCuTFSAqhsvHr4etS',$,$,$,(#269),#272);
#274= IFCSIMPLEPROPERTYTEMPLATE('0AlPfiIbv9OBEJiwR8hsE3',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#275,$,$,$,.READWRITE.);
#275= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#276= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#277= IFCRELASSOCIATESLIBRARY('1N9rVVb0T4TA_aas3Dl3YB',$,$,$,(#274),#276);
#278= IFCPROPERTYSETTEMPLATE('2ndzYiMzH2AuMrcbJhasYR',$,'Pset_ControllerTypeFloating','Properties for signal handling for an analog controller taking disparate valued multiple inputs and creating a single valued output.  HISTORY: IFC4 adapted from Pset_ControllerTypeCommon and applicable predefined type made specific to FLOATING; ACCUMULATOR and PULSECONVERTER types added; additional properties added to replace Pset_AnalogInput and Pset_AnalogOutput.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController/FLOATING',(#279,#283,#284,#285,#286,#289,#292));
#279= IFCSIMPLEPROPERTYTEMPLATE('1C15c0RDb54wqQ_p495feU',$,'ControlType','The type of signal modification effected and applicable ports: \X\0A\X\0ACONSTANT: No inputs; SignalOffset is written to the output value.\X\0AMODIFIER: Single analog input is read, added to SignalOffset, multiplied by SignalFactor, and written to the output value.\X\0AABSOLUTE: Single analog input is read and absolute value is written to the output value.\X\0AINVERSE: Single analog input is read, 1.0 is divided by the input value and written to the output value.\X\0AHYSTERISIS: Single analog input is read, delayed according to SignalTime, and written to the output value.\X\0ARUNNINGAVERAGE: Single analog input is read, averaged over SignalTime, and written to the output value.\X\0ADERIVATIVE: Single analog input is read and the rate of change during the SignalTime is written to the output value.\X\0AINTEGRAL: Single analog input is read and the average value during the SignalTime is written to the output value.\X\0ABINARY: Single binary input is read and SignalOffset is written to the output value if True.\X\0AACCUMULATOR: Single binary input is read, and for each pulse the SignalOffset is added to the accumulator, and while the accumulator is greater than the SignalFactor, the accumulator is decremented by SignalFactor and the integer result is incremented by one.\X\0APULSECONVERTER: Single integer input is read, and for each increment the SignalMultiplier is added and written to the output value.\X\0ASUM: Two analog inputs are read, added, and written to the output value.\X\0ASUBTRACT: Two analog inputs are read, subtracted, and written to the output value.\X\0APRODUCT: Two analog inputs are read, multiplied, and written to the output value.\X\0ADIVIDE: Two analog inputs are read, divided, and written to the output value.\X\0AAVERAGE: Two analog inputs are read and the average is written to the output value.\X\0AMAXIMUM: Two analog inputs are read and the maximum is written to the output value.\X\0AMINIMUM: Two analog inputs are read and the minimum is written to the output value..\X\0AINPUT: Controller element is a dedicated input.\X\0AOUTPUT: Controller element is a dedicated output.\X\0AVARIABLE: Controller element is an in-memory variable.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#280,$,$,$,.READWRITE.);
#280= IFCPROPERTYENUMERATION('PEnum_ControllerTypeFloating',(IFCLABEL('CONSTANT'),IFCLABEL('MODIFIER'),IFCLABEL('ABSOLUTE'),IFCLABEL('INVERSE'),IFCLABEL('HYSTERESIS'),IFCLABEL('RUNNINGAVERAGE'),IFCLABEL('DERIVATIVE'),IFCLABEL('INTEGRAL'),IFCLABEL('BINARY'),IFCLABEL('ACCUMULATOR'),IFCLABEL('PULSECONVERTER'),IFCLABEL('LOWERLIMITCONTROL'),IFCLABEL('UPPERLIMITCONTROL'),IFCLABEL('SUM'),IFCLABEL('SUBTRACT'),IFCLABEL('PRODUCT'),IFCLABEL('DIVIDE'),IFCLABEL('AVERAGE'),IFCLABEL('MAXIMUM'),IFCLABEL('MINIMUM'),IFCLABEL('REPORT'),IFCLABEL('SPLIT'),IFCLABEL('INPUT'),IFCLABEL('OUTPUT'),IFCLABEL('VARIABLE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#281= IFCLIBRARYREFERENCE($,$,'FLOATING \X2\C720D615\X0\','\X2\CEE8D2B8B864B7ECB294\X0\ \X2\D56DC0C1\X0\ \X2\D558B098C758\X0\ \X2\CD9CB825\X0\ \X2\D3ECD2B8C640\X0\ \X2\AC00BCC0\X0\ \X2\C785B825\X0\ \X2\D3ECD2B8\X0\ \X2\C720D615C5D0\X0\ \X2\B530B77CC788B294\X0\ \X2\D55CACB0\X0\ : output = SignalOffset \X2\C218C815C790\X0\ : output = input * SignalFactor + SignalOffset \X2\C808B300CE58\X0\ : output = | input | \X2\C5EDC218\X0\ : output = 1.0 / input \X2\C9C0C5F0\X0\ : output = \X2\C9C0C5F0\X0\ (input, SignalTime \X2\D6C4\X0\) \X2\C774B3D9\X0\ \X2\D3C9ADE0\X0\ : output = \X2\D3C9ADE0\X0\ (inputN, SignalTime \X2\C0ACC774\X0\) \X2\BBF8BD84\X0\ : output = \X2\BBF8BD84\X0\ (inputN, SignalTime \X2\C0ACC774\X0\) \X2\C801BD84\X0\ : output = \X2\C801BD84\X0\ (inputN, SignalTime \X2\C0ACC774\X0\) \X2\BC14C774B108B9AC\X0\ : output = SignalOffset \X2\203B\X0\ input = TRUE\X2\C758\X0\ \X2\ACBDC6B0\X0\ \X2\B204C801\X0\ : output = accumulator       \X2\203B\X0\ accumulator = \X2\D384C2A4\X0\ \X2\CE74C6B4D2B8\X0\ * SignalOffset       \X2\203B\X0\ if (accumulator> SignalFactor) accumulator - = SignalFactor       ??? \X2\D384C2A4\X0\ \X2\CE74C6B4D130\X0\ : output = input * SignalMultiplier       \X2\203B\X0\ input \X2\D384C2A4\X0\ \X2\CE74C6B4D2B8\X0\, SignalMultiplier\X2\C740\X0\ \X2\C6D0C778\X0\ \X2\BD88BA85\X0\       ??? \X2\CD1D\X0\ : output = input1 + input2 \X2\BE84C148\X0\ : output = input1 - input2 \X2\C801B9BD\X0\ : output = input1 * input2 \X2\B098B204AE30\X0\ : output = input1 / input2 \X2\D3C9ADE0\X0\ : output = (input1 + input2) / 2 \X2\CD5CB300\X0\ : output = input1 or input2 \X2\203BBCF4B2E4\X0\ \X2\D070\X0\ \X2\CD5CC18C\X0\ : output = input1 or input2 \X2\203BBCF4B2E4\X0\ \X2\C791C740\X0\','ko-KR',#2);
#282= IFCRELASSOCIATESLIBRARY('1GKhqfXjz3OOAErTQy9Oof',$,$,$,(#279),#281);
#283= IFCSIMPLEPROPERTYTEMPLATE('17s$1ZXL1E$xYIHpxwzzxK',$,'Labels','Table mapping values to labels, where such labels indicate transition points such as ''Hi'', ''Lo'', ''HiHi'', or ''LoLo''.',.P_TABLEVALUE.,'IfcReal','IfcLabel',$,$,$,$,.READWRITE.);
#284= IFCSIMPLEPROPERTYTEMPLATE('3$UgXmj8n5yvLyHFJ2oEfR',$,'Range','The physical range of values supported by the device.',.P_BOUNDEDVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#285= IFCSIMPLEPROPERTYTEMPLATE('2Nj7MbtYT01R4dl08QUFlM',$,'Value','The expected range and default value.  While the property data type is IfcReal (to support all cases including when the units are unknown), a unit may optionally be provided to indicate the measure and unit.  The LowerLimitValue and UpperLimitValue must fall within the physical Range and may be used to determine extents when charting Pset_ControllerPHistory.Value.',.P_BOUNDEDVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#286= IFCSIMPLEPROPERTYTEMPLATE('1FTFw1Ezz8sAWtGUURWdK2',$,'SignalOffset','Offset constant added to modfied signal.',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#287= IFCLIBRARYREFERENCE($,$,'\X2\C635C14B\X0\','\X2\C624D504C14B\X0\ \X2\C0C1C218\X0\ \X2\BCC0ACBD\X0\ \X2\C2E0D638C5D0\X0\ \X2\CD94AC00B428\X0\','ko-KR',#2);
#288= IFCRELASSOCIATESLIBRARY('0nlLExqK57geOWNoXHP_Dq',$,$,$,(#286),#287);
#289= IFCSIMPLEPROPERTYTEMPLATE('06yem83ST7Af2c4LqTDwH7',$,'SignalFactor','Factor multiplied onto offset signal.',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#290= IFCLIBRARYREFERENCE($,$,'\X2\C694C18C\X0\','\X2\C778C790B294\X0\ \X2\C624D504C14B\X0\ \X2\C2E0D638\X0\ \X2\ACF1C148\X0\','ko-KR',#2);
#291= IFCRELASSOCIATESLIBRARY('2swTCDCGL8W8C6fAGuAy1f',$,$,$,(#289),#290);
#292= IFCSIMPLEPROPERTYTEMPLATE('1ARu9Vm9z8HRoVhwATah88',$,'SignalTime','Time factor used for integral and running average controllers.',.P_SINGLEVALUE.,'IfcTimeMeasure','',$,$,$,$,.READWRITE.);
#293= IFCLIBRARYREFERENCE($,$,'\X2\C2DCAC04\X0\ \X2\C694C18C\X0\','\X2\C2DCAC04\X0\ \X2\C694C18CB294\X0\ INTEGRAL (\X2\C801BD84\X0\)\X2\ACFC\X0\ AVERAGE ((\X2\C774B3D9\X0\) \X2\D3C9ADE0\X0\) \X2\CEE8D2B8B864B7ECC5D0\X0\ \X2\C0ACC6A9B428\X0\','ko-KR',#2);
#294= IFCRELASSOCIATESLIBRARY('04X$Sx4bHFFx7CMdUDwXh0',$,$,$,(#292),#293);
#295= IFCPROPERTYSETTEMPLATE('30X8Ni_8X8_P16PwjzqPhN',$,'Pset_ControllerTypeMultiPosition','Properties for discrete inputs, outputs, and values within a programmable logic controller. HISTORY: New in IFC4, replaces Pset_MultiStateInput and Pset_MultiStateOutput.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController/MULTIPOSITION',(#296,#298,#299,#300));
#296= IFCSIMPLEPROPERTYTEMPLATE('2Pzw9COdzBgx7AtUuRG6$h',$,'ControlType','The type of signal modification effected and applicable ports:\X\0A\X\0AINPUT: Controller element is a dedicated input.\X\0AOUTPUT: Controller element is a dedicated output.\X\0AVARIABLE: Controller element is an in-memory variable.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#297,$,$,$,.READWRITE.);
#297= IFCPROPERTYENUMERATION('PEnum_ControllerMultiPositionType',(IFCLABEL('INPUT'),IFCLABEL('OUTPUT'),IFCLABEL('VARIABLE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#298= IFCSIMPLEPROPERTYTEMPLATE('1TJNaBhXj9AAorK6vFSquS',$,'Labels','Table mapping values to labels, where each entry corresponds to an integer within the ValueRange.',.P_TABLEVALUE.,'IfcInteger','IfcLabel',$,$,$,$,.READWRITE.);
#299= IFCSIMPLEPROPERTYTEMPLATE('1BTgcIE6P5URrG6TSfUpI4',$,'Range','The physical range of values supported by the device.',.P_BOUNDEDVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#300= IFCSIMPLEPROPERTYTEMPLATE('1RO5q3jgPE5vl1WsB34FKU',$,'Value','The expected range and default value.  The LowerLimitValue and UpperLimitValue must fall within the physical Range.',.P_BOUNDEDVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#301= IFCPROPERTYSETTEMPLATE('3niFgjkmP19e6xah2tkjLE',$,'Pset_ControllerTypeProgrammable','Properties for Discrete Digital Control (DDC) or programmable logic controllers.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController/PROGRAMMABLE',(#302,#304,#307,#310));
#302= IFCSIMPLEPROPERTYTEMPLATE('1eHqSFOhf4TegRRLIhnsiP',$,'ControlType','The type of discrete digital controller: \X\0A\X\0APRIMARY: Controller has built-in communication interface for PC connection, may manage secondary controllers.\X\0ASECONDARY: Controller communicates with primary controller and its own managed devices.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#303,$,$,$,.READWRITE.);
#303= IFCPROPERTYENUMERATION('PEnum_ControllerTypeProgrammable',(IFCLABEL('PRIMARY'),IFCLABEL('SECONDARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#304= IFCSIMPLEPROPERTYTEMPLATE('0m$smZKhn5ehFWeGrnWynK',$,'FirmwareVersion','Indicates version of device firmware according to device manufacturer.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#305= IFCLIBRARYREFERENCE($,$,'\X2\D38CC6E8C5B4\X0\ \X2\BC84C804\X0\','\X2\CEE8D2B8B864B7EC\X0\ \X2\D38CC6E8C5B4\X0\ \X2\BC84C804\X0\','ko-KR',#2);
#306= IFCRELASSOCIATESLIBRARY('1pIaIAj4H2C8MJW6qaWHgl',$,$,$,(#304),#305);
#307= IFCSIMPLEPROPERTYTEMPLATE('3imWCZmy16GhcYqRE62Tpk',$,'SoftwareVersion','Indicates version of application software according to systems integrator.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#308= IFCLIBRARYREFERENCE($,$,'\X2\C18CD504D2B8C6E8C5B4\X0\ \X2\BC84C804\X0\','\X2\CEE8D2B8B864B7EC\X0\ \X2\C18CD504D2B8C6E8C5B4\X0\ \X2\BC84C804\X0\','ko-KR',#2);
#309= IFCRELASSOCIATESLIBRARY('0LG2EG_JP42wRgezDozqRC',$,$,$,(#307),#308);
#310= IFCSIMPLEPROPERTYTEMPLATE('30zXhBkAL1GBLLQ6L5Gg2V',$,'Application','Indicates application of controller.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#311,$,$,$,.READWRITE.);
#311= IFCPROPERTYENUMERATION('PEnum_ControllerApplication',(IFCLABEL('ModemController'),IFCLABEL('TelephoneDirectory'),IFCLABEL('FanCoilUnitController'),IFCLABEL('RoofTopUnitController'),IFCLABEL('UnitVentilatorController'),IFCLABEL('SpaceConfortController'),IFCLABEL('VAV'),IFCLABEL('PumpController'),IFCLABEL('BoilerController'),IFCLABEL('DischargeAirController'),IFCLABEL('OccupancyController'),IFCLABEL('ConstantLightController'),IFCLABEL('SceneController'),IFCLABEL('PartitionWallController'),IFCLABEL('RealTimeKeeper'),IFCLABEL('RealTimeBasedScheduler'),IFCLABEL('LightingPanelController'),IFCLABEL('SunblindController'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#312= IFCPROPERTYSETTEMPLATE('1EZwKkAa98IvbQ01Vqfi02',$,'Pset_ControllerTypeProportional','Properties for signal handling for an proportional controller taking setpoint and feedback inputs and creating a single valued output. HISTORY: In IFC4, SignalFactor1, SignalFactor2 and SignalFactor3 changed to ProportionalConstant, IntegralConstant and DerivativeConstant.  SignalTime1 and SignalTime2 changed to SignalTimeIncrease and SignalTimeDecrease.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController/PROPORTIONAL',(#313,#317,#318,#319,#320,#323,#326,#329,#332));
#313= IFCSIMPLEPROPERTYTEMPLATE('1lRTyXlrL4P9jgbrGveQqx',$,'ControlType','The type of signal modification.\X\0APROPORTIONAL: Output is proportional to the control error. The gain of a proportional control (Kp) will have the effect of reducing the rise time and reducing , but never eliminating, the steady-state error of the variable controlled. \X\0APROPORTIONALINTEGRAL: Part of the output is proportional to the control error and part is proportional to the time integral of the control error. Adding the gain of an integral control (Ki) will have the effect of eliminating the steady-state error of the variable controlled, but it may make the transient response worse. \X\0APROPORTIONALINTEGRALDERIVATIVE: Part of the output is proportional to the control error, part is proportional to the time integral of the control error and part is proportional to the time derivative of the control error. Adding the gain of a derivative control (Kd) will have the effect of increasing the stability of the system, reducing the overshoot, and improving the transient response of the variable controlled.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#314,$,$,$,.READWRITE.);
#314= IFCPROPERTYENUMERATION('PEnum_ControllerProportionalType',(IFCLABEL('PROPORTIONAL'),IFCLABEL('PROPORTIONALINTEGRAL'),IFCLABEL('PROPORTIONALINTEGRALDERIVATIVE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#315= IFCLIBRARYREFERENCE($,$,'PROPORTIONAL \X2\C720D615\X0\','\X2\C2E0D638\X0\ \X2\BCC0ACBD\X0\ \X2\C720D615\X0\   P (\X2\BE44B840\X0\), I (\X2\C801BD84\X0\), D (\X2\BBF8BD84\X0\)\X2\C758\X0\ \X2\C870D569\X0\ PROPORTIONAL :   P (\X2\BE44B840\X0\) \X2\C81CC5B4\X0\ PROPORTIONALINTEGRAL :   PI (\X2\BE44B840\X0\ \X2\C801BD84\X0\) \X2\C81CC5B4\X0\ PROPORTIONALINTEGRALDERIVATIVE :   PID (\X2\BE44B840\X0\ \X2\C801BD84\X0\ \X2\BBF8BD84\X0\) \X2\C81CC5B4\X0\','ko-KR',#2);
#316= IFCRELASSOCIATESLIBRARY('1p3Mljod17CeLIqGDsO5Y2',$,$,$,(#313),#315);
#317= IFCSIMPLEPROPERTYTEMPLATE('0TcD9N_lb6jvncYCXywG1T',$,'Labels','Table mapping values to labels, where such labels indicate transition points such as ''Hi'', ''Lo'', ''HiHi'', or ''LoLo''.',.P_TABLEVALUE.,'IfcReal','IfcLabel',$,$,$,$,.READWRITE.);
#318= IFCSIMPLEPROPERTYTEMPLATE('034uUTZX5AcvIHhUsncmjm',$,'Range','The physical range of values.',.P_BOUNDEDVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#319= IFCSIMPLEPROPERTYTEMPLATE('2T8sWQNmvAT8GdcS1pBn7I',$,'Value','The expected range and default value.  While the property data type is IfcReal (to support all cases including when the units are unknown), a unit may optionally be provided to indicate the measure and unit.',.P_BOUNDEDVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#320= IFCSIMPLEPROPERTYTEMPLATE('3AHEeASKXBixRh3kqOJ16T',$,'ProportionalConstant','The proportional gain factor of the controller (usually referred to as Kp).',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#321= IFCLIBRARYREFERENCE($,$,'\X2\BE44B840\X0\ \X2\AC8CC778\X0\ (Kp)','\X2\BE44B840\X0\ \X2\AC8CC778\X0\ (Kp)','ko-KR',#2);
#322= IFCRELASSOCIATESLIBRARY('08tS$vpSTFIPhTUcctDUCV',$,$,$,(#320),#321);
#323= IFCSIMPLEPROPERTYTEMPLATE('3nJFDue5v1cQKJh5g39ZTt',$,'IntegralConstant','The integral gain factor of the controller (usually referred to as Ki).  Asserted where ControlType is PROPORTIONALINTEGRAL or PROPORTIONALINTEGRALDERIVATIVE.',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#324= IFCLIBRARYREFERENCE($,$,'\X2\C801BD84\X0\ \X2\AC8CC778\X0\ (Ki)','\X2\C801BD84\X0\ \X2\AC8CC778\X0\ (Ki)','ko-KR',#2);
#325= IFCRELASSOCIATESLIBRARY('3vSGopAjD3ag5$32MdGgE4',$,$,$,(#323),#324);
#326= IFCSIMPLEPROPERTYTEMPLATE('0J6X1VGGH5HBQIjNF6bXQ6',$,'DerivativeConstant','The derivative gain factor of the controller (usually referred to as Kd).  Asserted where ControlType is PROPORTIONALINTEGRALDERIVATIVE.',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#327= IFCLIBRARYREFERENCE($,$,'\X2\BBF8BD84\X0\ \X2\AC8CC778\X0\ (Kd)','\X2\BBF8BD84\X0\ \X2\AC8CC778\X0\ (Kd)','ko-KR',#2);
#328= IFCRELASSOCIATESLIBRARY('2lU78xa9v5uwDN$njKhOU4',$,$,$,(#326),#327);
#329= IFCSIMPLEPROPERTYTEMPLATE('3VEqTLe0TEIQMgHESSUL8l',$,'SignalTimeIncrease','Time factor used for exponential increase.',.P_SINGLEVALUE.,'IfcTimeMeasure','',$,$,$,$,.READWRITE.);
#330= IFCLIBRARYREFERENCE($,$,'\X2\C801BD84\X0\ \X2\C2DCAC04\X0\ (Ti)','\X2\C801BD84\X0\ \X2\C2DCAC04\X0\ (Ti)','ko-KR',#2);
#331= IFCRELASSOCIATESLIBRARY('15KBh7SgH6oPCyZ0sG7smw',$,$,$,(#329),#330);
#332= IFCSIMPLEPROPERTYTEMPLATE('0W8hixIYT0ERVlO6gHM8qD',$,'SignalTimeDecrease','Time factor used for exponential decrease.',.P_SINGLEVALUE.,'IfcTimeMeasure','',$,$,$,$,.READWRITE.);
#333= IFCLIBRARYREFERENCE($,$,'\X2\BBF8BD84\X0\ \X2\C2DCAC04\X0\ (Td)','\X2\BBF8BD84\X0\ \X2\C2DCAC04\X0\ (Td)','ko-KR',#2);
#334= IFCRELASSOCIATESLIBRARY('38p7XyVCr12emsHqAg$OMt',$,$,$,(#332),#333);
#335= IFCPROPERTYSETTEMPLATE('2wf$xAkNr8Evx3A1EgOXFV',$,'Pset_ControllerTypeTwoPosition','Properties for signal handling for an analog controller taking disparate valued multiple inputs and creating a single valued binary output. HISTORY: In IFC4, extended properties to replace Pset_BinaryInput and Pset_BinaryOutput.',.PSET_TYPEDRIVENOVERRIDE.,'IfcController/TWOPOSITION',(#336,#340,#341,#342));
#336= IFCSIMPLEPROPERTYTEMPLATE('2I1cpzU1H6X9RVmzzsaCcM',$,'ControlType','The type of signal modification effected and applicable ports:\X\0A\X\0ALOWERLIMITSWITCH: Single analog input is read and if less than Value.LowerBound then True is written to the output value.\X\0AUPPERLIMITSWITCH: Single analog input is read and if more than Value.UpperBound then True is written to the output value.\X\0ALOWERBANDSWITCH: Single analog input is read and if less than Value.LowerBound+BandWidth then True is written to the output value.\X\0AUPPERBANDSWITCH: Single analog input is read and if more than Value.UpperBound-BandWidth then True is written to the output value.\X\0ANOT: Single binary input is read and the opposite value is written to the output value.\X\0AAND: Two binary inputs are read and if both are True then True is written to the output value.\X\0AOR: Two binary inputs are read and if either is True then True is written to the output value.\X\0AXOR: Two binary inputs are read and if one is true then True is written to the output value.\X\0ACALENDAR: No inputs; the current time is compared with an IfcWorkCalendar to which the IfcController is assigned and True is written if active.\X\0AINPUT: Controller element is a dedicated input.\X\0AOUTPUT: Controller element is a dedicated output.\X\0AVARIABLE: Controller element is an in-memory variable.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#337,$,$,$,.READWRITE.);
#337= IFCPROPERTYENUMERATION('PEnum_ControllerTwoPositionType',(IFCLABEL('NOT'),IFCLABEL('AND'),IFCLABEL('OR'),IFCLABEL('XOR'),IFCLABEL('LOWERLIMITSWITCH'),IFCLABEL('UPPERLIMITSWITCH'),IFCLABEL('LOWERBANDSWITCH'),IFCLABEL('UPPERBANDSWITCH'),IFCLABEL('AVERAGE'),IFCLABEL('CALENDAR'),IFCLABEL('INPUT'),IFCLABEL('OUTPUT'),IFCLABEL('VARIABLE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#338= IFCLIBRARYREFERENCE($,$,'TWOPOSITION \X2\C720D615\X0\','\X2\C2E0D638\X0\ \X2\BCC0ACBD\X0\ \X2\C720D615\X0\ \X2\B9ACBBF8D2B8\X0\ \X2\C2A4C704CE58AC00\X0\ \X2\BC94C704B97C\X0\ Pset_ControllerTypeValue \X2\AC12C744\X0\ \X2\BB36C5EC\X0\ \X2\C18DC131C5D0\X0\ \X2\C758D574\X0\ \X2\ACB0C815\X0\ \X2\D558D55C\X0\ : if (Value.LowerBound> Input) output = TRUE \X2\C0C1D55C\X0\ : if (Value.UpperBound <Input) output = TRUE \X2\D558D55C\X0\ + \X2\BD88AC10B300\X0\ : if (Value.LowerBound + BandWidth> Input) output = TRUE \X2\CD5CB300\X0\ - \X2\BD88AC10B300\X0\ : if (Value.UpperBound - BandWidth <Input) output = TRUE \X2\B17CB9AC\X0\ \X2\BD80C815\X0\ : output = NOT (input) \X2\B17CB9ACC801\X0\ : output = AND (input1, input2) \X2\B17CB9ACD569\X0\ : output = OR (input, input2) \X2\BC30D0C0C801\X0\ \X2\B17CB9ACD569\X0\ : output = XOR (input, input2) \X2\B2ECB825\X0\ : output = TRUE \X2\203B\X0\ \X2\CEE8D2B8B864B7ECC5D0\X0\ \X2\C785B825C5C6C774D558ACE0\X0\ IfcWorkCalendar \X2\CEE8D2B8B864B7ECAC00\X0\ \X2\D560B2F9B418C5B4\X0\ \X2\D604C7AC\X0\ \X2\C2DCAC04C778\X0\ \X2\ACBDC6B0\X0\','ko-KR',#2);
#339= IFCRELASSOCIATESLIBRARY('06A1SdvJjDIAaAUf5swKR3',$,$,$,(#336),#338);
#340= IFCSIMPLEPROPERTYTEMPLATE('2E24iJ2ez5xPdx$elWhxk5',$,'Labels','Table mapping values to labels, where such labels indicate the meanings of True and False, such as ''Open'' and ''Closed''',.P_TABLEVALUE.,'IfcBoolean','IfcLabel',$,$,$,$,.READWRITE.);
#341= IFCSIMPLEPROPERTYTEMPLATE('1YXppz9HP1r8OVU$m73_GL',$,'Polarity','True indicates normal polarity; False indicates reverse polarity.',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#342= IFCSIMPLEPROPERTYTEMPLATE('3EUJTdpxbDSwX15SKxUsLO',$,'Value','The default value such as normally-closed or normally-open.',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#343= IFCPROPERTYSETTEMPLATE('25Gk4NUnf1Qvob2aiT6CVk',$,'Pset_FlowInstrumentPHistory','Properties for history of flow instrument values.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcFlowInstrument',(#344,#345,#346));
#344= IFCSIMPLEPROPERTYTEMPLATE('0LsdtYfeHC1eISNb$kyD3y',$,'Value','Indicates measured values over time which may be recorded continuously or only when changed beyond a particular deadband.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcReal',$,$,$,$,.READWRITE.);
#345= IFCSIMPLEPROPERTYTEMPLATE('3Q9pvdNG95cP46q5wDm_L7',$,'Quality','Indicates the quality of measurement or failure condition, which may be further qualified by the Status.  True: measured values are considered reliable; False: measured values are considered not reliable (i.e. a fault has been detected); Unknown: reliability of values is uncertain.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#346= IFCSIMPLEPROPERTYTEMPLATE('16RIcyUeL6oRSEKaS8uWyw',$,'Status','Indicates an error code or identifier, whose meaning is specific to the particular automation system.  Example values include: ''ConfigurationError'', ''NotConnected'', ''DeviceFailure'', ''SensorFailure'', ''LastKnown, ''CommunicationsFailure'', ''OutOfService''.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLabel',$,$,$,$,.READWRITE.);
#347= IFCPROPERTYSETTEMPLATE('1sadV18Qr75wp91Nv7sn91',$,'Pset_FlowInstrumentTypeCommon','Flow Instrument type common attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcFlowInstrument',(#350,#355));
#348= IFCLIBRARYREFERENCE($,$,$,'\X2\6D414F538A085668306E5171901A5C5E60273002\X0\','ja-JP',#2);
#349= IFCRELASSOCIATESLIBRARY('3qZ8IQKw16hwpnjBQnXdrn',$,$,$,(#347),#348);
#350= IFCSIMPLEPROPERTYTEMPLATE('1vjG8Qkf18oQV0EFmO8xpl',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#351= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#352= IFCRELASSOCIATESLIBRARY('0y3XVVBN5Cfum8xrwVMcjm',$,$,$,(#350),#351);
#353= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#354= IFCRELASSOCIATESLIBRARY('3fyJwFhwjC9v2lzJtVq6l6',$,$,$,(#350),#353);
#355= IFCSIMPLEPROPERTYTEMPLATE('3KsB0_2qr6KA$hhIYcGTjW',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#356,$,$,$,.READWRITE.);
#356= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#357= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#358= IFCRELASSOCIATESLIBRARY('2czgRBG_n5Hhj22Tk8Dwdc',$,$,$,(#355),#357);
#359= IFCPROPERTYSETTEMPLATE('3QjshE6J15cBNmKGztRBmL',$,'Pset_FlowInstrumentTypePressureGauge','A device that reads and displays a pressure value at a point or the pressure difference between two points.',.PSET_TYPEDRIVENOVERRIDE.,'IfcFlowInstrument/PRESSUREGAUGE',(#362,#368));
#360= IFCLIBRARYREFERENCE($,$,$,'\X2\305D306E4F4D7F6E306E5727529B3001307E305F306F3001\X0\2\X2\304B6240306E5DEE572730926E2C5B9A30578868793A3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#361= IFCRELASSOCIATESLIBRARY('0EMS6bUX92WQgTjz$y1X8L',$,$,$,(#359),#360);
#362= IFCSIMPLEPROPERTYTEMPLATE('3BLbse3vnDrfl$KSN2SN_$',$,'PressureGaugeType','Identifies the means by which pressure is displayed.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#363,$,$,$,.READWRITE.);
#363= IFCPROPERTYENUMERATION('PEnum_PressureGaugeType',(IFCLABEL('DIAL'),IFCLABEL('DIGITAL'),IFCLABEL('MANOMETER'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#364= IFCLIBRARYREFERENCE($,$,'\X2\5727529B8A0830BF30A430D7\X0\','\X2\5727529B304C8868793A3055308C308B624B6BB530928B5852253059308B3002\X0\','ja-JP',#2);
#365= IFCRELASSOCIATESLIBRARY('0kod0NE1r9aey5bkE8_J4r',$,$,$,(#362),#364);
#366= IFCLIBRARYREFERENCE($,$,'\X2\C555B825ACC4\X0\ \X2\C720D615\X0\','\X2\C555B825C774\X0\ \X2\D45CC2DCB418B294\X0\ \X2\BC29BC95C744\X0\ \X2\D655C778D55CB2E4\X0\.','ko-KR',#2);
#367= IFCRELASSOCIATESLIBRARY('0W$whPgl1CIv98aJiClkPI',$,$,$,(#362),#366);
#368= IFCSIMPLEPROPERTYTEMPLATE('03T5WWL11CDRX0EcPpGvWO',$,'DisplaySize','The physical size of the display. For a dial pressure gauge it will be the diameter of the dial.',.P_SINGLEVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#369= IFCLIBRARYREFERENCE($,$,'\X2\8868793A30B530A430BA\X0\','\X2\8868793A306E30B530A430BA3002\X0\ \X2\30C030A430E430EB5727529B8A08306B95A230573066306F300130C030A430E430EB306E76F45F84306B306A308B3002\X0\','ja-JP',#2);
#370= IFCRELASSOCIATESLIBRARY('2ZkBdYKkH0qxkC_TrN6w84',$,$,$,(#368),#369);
#371= IFCLIBRARYREFERENCE($,$,'\X2\B514C2A4D50CB808C774\X0\ \X2\D06CAE30\X0\','\X2\D45CC2DCC758\X0\ \X2\D06CAE30C785B2C8B2E4\X0\. \X2\B2E4C774C5BC\X0\ \X2\AC8CC774C9C0C5D0\X0\ \X2\AD00D574C11CB294\X0\ \X2\C804D654\X0\ \X2\C9C1ACBDB41CB2E4\X0\.','ko-KR',#2);
#372= IFCRELASSOCIATESLIBRARY('0QqKTwJH90CABefPh2X5fL',$,$,$,(#368),#371);
#373= IFCPROPERTYSETTEMPLATE('2R5o7gaq95Gxi00Zv2YVk3',$,'Pset_FlowInstrumentTypeThermometer','A device that reads and displays a temperature value at a point.',.PSET_TYPEDRIVENOVERRIDE.,'IfcFlowInstrument/THERMOMETER',(#376,#382));
#374= IFCLIBRARYREFERENCE($,$,$,'\X2\6E295EA630926E2C5B9A30578868793A3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#375= IFCRELASSOCIATESLIBRARY('203FM23D969By_anSYJgTw',$,$,$,(#373),#374);
#376= IFCSIMPLEPROPERTYTEMPLATE('03mjYzi31ClP3iinPOnt8M',$,'ThermometerType','Identifies the means by which temperature is displayed.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#377,$,$,$,.READWRITE.);
#377= IFCPROPERTYENUMERATION('PEnum_ThermometerType',(IFCLABEL('DIAL'),IFCLABEL('DIGITAL'),IFCLABEL('STEM'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#378= IFCLIBRARYREFERENCE($,$,'\X2\6E295EA68A0830BF30A430D7\X0\','\X2\6E295EA6304C8868793A3055308C308B624B6BB530928B5852253059308B3002\X0\','ja-JP',#2);
#379= IFCRELASSOCIATESLIBRARY('1dk1vgxS98dPiSGowU1Ex4',$,$,$,(#376),#378);
#380= IFCLIBRARYREFERENCE($,$,'\X2\C628B3C4ACC4\X0\ \X2\C720D615\X0\','\X2\C628B3C4AC00\X0\ \X2\D45CC2DCB418B294\X0\ \X2\BC29BC95C744\X0\ \X2\D655C778D55CB2E4\X0\.','ko-KR',#2);
#381= IFCRELASSOCIATESLIBRARY('2Gw2OSieH23v1rtv5jyPNW',$,$,$,(#376),#380);
#382= IFCSIMPLEPROPERTYTEMPLATE('25t_Tuj$f8ZBZhu5lrBszm',$,'DisplaySize','The physical size of the display. In the case of a stem thermometer, this will be the length of the stem. For a dial thermometer, it will be the diameter of the dial.',.P_SINGLEVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#383= IFCLIBRARYREFERENCE($,$,'\X2\8868793A30B530A430BA\X0\','\X2\8868793A306E30B530A430BA3002\X0\ \X2\68D26E295EA68A08306E583454083067306F30018EF8306E95773055306B306A308B3002\X0\ \X2\30C030A430E430EB6E295EA68A08306B95A230573066306F300130C030A430E430EB306E76F45F84306B306A308B3002\X0\','ja-JP',#2);
#384= IFCRELASSOCIATESLIBRARY('0zFZ_Zc1vEovAQg_qaz_4r',$,$,$,(#382),#383);
#385= IFCLIBRARYREFERENCE($,$,'\X2\B514C2A4D50CB808C774\X0\ \X2\D06CAE30\X0\','\X2\D45CC2DCC758\X0\ \X2\D06CAE30C785B2C8B2E4\X0\. \X2\B9C9B300\X0\ \X2\C628B3C4ACC4C758\X0\ \X2\ACBDC6B0\X0\, \X2\CD95C758\X0\ \X2\AE38C774AC00B41CB2E4\X0\. \X2\B2E4C774C5BC\X0\ \X2\C628B3C4ACC4C5D0\X0\ \X2\B300D574C11CB294\X0\ \X2\B2E4C774C5BC\X0\ \X2\C9C1ACBDB41CB2E4\X0\.','ko-KR',#2);
#386= IFCRELASSOCIATESLIBRARY('0UN4zHaW14F8UpLm7bp3bO',$,$,$,(#382),#385);
#387= IFCPROPERTYSETTEMPLATE('1xgCnOYQLENRpElFVQLZ3k',$,'Pset_SensorPHistory','Properties for history of controller values.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcSensor',(#388,#389,#390,#391));
#388= IFCSIMPLEPROPERTYTEMPLATE('1lf6Bs7kb1MP704HDKaQyq',$,'Value','Indicates sensed values over time which may be recorded continuously or only when changed beyond a particular deadband.  The range of possible values is defined by the SetPoint property of the corresponding sensor type property set.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcReal',$,$,$,$,.READWRITE.);
#389= IFCSIMPLEPROPERTYTEMPLATE('2QdhTztjj1URf_53NsZNx$',$,'Direction','Indicates sensed direction for sensors capturing magnitude and direction measured from True North (0 degrees) in a clockwise direction.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcPlaneAngleMeasure',$,$,$,$,.READWRITE.);
#390= IFCSIMPLEPROPERTYTEMPLATE('3CnjLFzlD7Q9UFWUbr0Flv',$,'Quality','Indicates the quality of measurement or failure condition, which may be further qualified by the Status.  True: measured values are considered reliable; False: measured values are considered not reliable (i.e. a fault has been detected); Unknown: reliability of values is uncertain.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#391= IFCSIMPLEPROPERTYTEMPLATE('12Eb3qN854mPFCjBn3Zq6s',$,'Status','Indicates an error code or identifier, whose meaning is specific to the particular automation system.  Example values include: ''ConfigurationError'', ''NotConnected'', ''DeviceFailure'', ''SensorFailure'', ''LastKnown, ''CommunicationsFailure'', ''OutOfService''.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLabel',$,$,$,$,.READWRITE.);
#392= IFCPROPERTYSETTEMPLATE('00rrd6Gs97UP8$_ekQyNeu',$,'Pset_SensorTypeCommon','Sensor type common attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor',(#395,#400));
#393= IFCLIBRARYREFERENCE($,$,$,'\X2\30BB30F330B530FC30BF30A430D7306E5171901A5C5E60273002\X0\','ja-JP',#2);
#394= IFCRELASSOCIATESLIBRARY('2SLvP9O8vE5P$3dTyyp6u2',$,$,$,(#392),#393);
#395= IFCSIMPLEPROPERTYTEMPLATE('2n_kZuJ7P3R9GZ$fdnvM2A',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#396= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#397= IFCRELASSOCIATESLIBRARY('3TbAy7OGjCf8nGh41o4spY',$,$,$,(#395),#396);
#398= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#399= IFCRELASSOCIATESLIBRARY('24t8oDcbbAPPW1ERCHRF0F',$,$,$,(#395),#398);
#400= IFCSIMPLEPROPERTYTEMPLATE('2r923g8x5FJuuAxukYtRbv',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#401,$,$,$,.READWRITE.);
#401= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#402= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#403= IFCRELASSOCIATESLIBRARY('0VxdOF80rB39StY6WWINzD',$,$,$,(#400),#402);
#404= IFCPROPERTYSETTEMPLATE('1LgYnhoCz7RBDPy2rijQCr',$,'Pset_SensorTypeConductanceSensor','A device that senses or detects electrical conductance.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/CONDUCTANCESENSOR',(#407));
#405= IFCLIBRARYREFERENCE($,$,$,'\X2\96FB6C174F1D5C0E60273092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#406= IFCRELASSOCIATESLIBRARY('0jTfIta$H2$PclOJ6oqEAB',$,$,$,(#404),#405);
#407= IFCSIMPLEPROPERTYTEMPLATE('3evKdp4sL5HumAETnOEsaU',$,'SetPointConductance','The fill level value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcElectricConductanceMeasure','',$,$,$,$,.READWRITE.);
#408= IFCLIBRARYREFERENCE($,$,'\X2\96FB6C174F1D5C0E73878A2D5B9A5024\X0\','\X2\611F77E53055308C308B96FB6C174F1D5C0E73873002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#409= IFCRELASSOCIATESLIBRARY('3_rVXe9cP8EhL$plGjBzE4',$,$,$,(#407),#408);
#410= IFCLIBRARYREFERENCE($,$,'\X2\C804AE30\X0\ \X2\C804B3C4C728\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C804AE30\X0\ \X2\C804B3C4C728\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#411= IFCRELASSOCIATESLIBRARY('3Fu9ImpHr2Yv9h9VIwcJCh',$,$,$,(#407),#410);
#412= IFCPROPERTYSETTEMPLATE('1uOoWL1U1788lyt_W0x3Au',$,'Pset_SensorTypeContactSensor','A device that senses or detects contact. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/CONTACTSENSOR',(#415));
#413= IFCLIBRARYREFERENCE($,$,$,'\X2\63A589E63092611F77E5307E305F306F691C51FA3059308B30C730D030A430B9\X0\','ja-JP',#2);
#414= IFCRELASSOCIATESLIBRARY('3zhZ7kXnz1ju_GMeTnIIuv',$,$,$,(#412),#413);
#415= IFCSIMPLEPROPERTYTEMPLATE('0Le4BADUX4_9bBVwgSV002',$,'SetPointContact','The contact value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#416= IFCLIBRARYREFERENCE($,$,'\X2\63A589E672B6614B8A2D5B9A5024\X0\','\X2\611F77E53055308C308B63A589E672B6614B3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#417= IFCRELASSOCIATESLIBRARY('20a5YQdJH6HgYswEOpn0MI',$,$,$,(#415),#416);
#418= IFCLIBRARYREFERENCE($,$,'\X2\C811CD09\X0\ \X2\C0C1D0DC\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C811CD09\X0\ \X2\C0C1D0DC\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#419= IFCRELASSOCIATESLIBRARY('18g6ikblPBUBSO_ao9fGCZ',$,$,$,(#415),#418);
#420= IFCPROPERTYSETTEMPLATE('2fx9Dm0ZT4nP$sP2iQGI40',$,'Pset_SensorTypeFireSensor','A device that senses or detects the presence of fire.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/FIRESENSOR',(#423,#428,#433));
#421= IFCLIBRARYREFERENCE($,$,$,'\X2\708E306E5B5857283092611F77E5307E305F306F691C51FA3059308B30C730D030A430B9\X0\','ja-JP',#2);
#422= IFCRELASSOCIATESLIBRARY('0JV2FIzBP1NRk0WiNXR$pa',$,$,$,(#420),#421);
#423= IFCSIMPLEPROPERTYTEMPLATE('0K1TDRu5L79glpfxttrBr2',$,'FireSensorSetPoint','The temperature value to be sensed to indicate the presence of fire.',.P_SINGLEVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#424= IFCLIBRARYREFERENCE($,$,'\X2\611F77E56E295EA6\X0\','\X2\708E306E5B5857283092793A3059305F3081306B611F77E53055308C308B6E295EA650243002\X0\','ja-JP',#2);
#425= IFCRELASSOCIATESLIBRARY('1GPGJb8qvBvOOJ$kkTlToi',$,$,$,(#423),#424);
#426= IFCLIBRARYREFERENCE($,$,'\X2\AC10C9C0\X0\ \X2\C628B3C4\X0\','\X2\BD88AF43C758\X0\ \X2\C874C7ACB97C\X0\ \X2\BCF4C5ECC8FCAE30\X0\ \X2\C704D558C5EC\X0\ \X2\AC10C9C0B418B294\X0\ \X2\C628B3C4\X0\ \X2\AC12\X0\.','ko-KR',#2);
#427= IFCRELASSOCIATESLIBRARY('34u3agWYLB0OcOv0WM9LLi',$,$,$,(#423),#426);
#428= IFCSIMPLEPROPERTYTEMPLATE('301iiZ1E55WvT7B93xQ9sH',$,'AccuracyOfFireSensor','The accuracy of the sensor.',.P_SINGLEVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#429= IFCLIBRARYREFERENCE($,$,'\X2\7CBE5EA6\X0\','\X2\30BB30F330B5306E7CBE5EA63002\X0\','ja-JP',#2);
#430= IFCRELASSOCIATESLIBRARY('39J9M0wrD9tudFi2I4_iMf',$,$,$,(#428),#429);
#431= IFCLIBRARYREFERENCE($,$,'\X2\C815D655B3C4\X0\','\X2\C13CC11CC758\X0\ \X2\C815BC00B3C4\X0\.','ko-KR',#2);
#432= IFCRELASSOCIATESLIBRARY('0qA2yYi3r1pRgQvE2JMxua',$,$,$,(#428),#431);
#433= IFCSIMPLEPROPERTYTEMPLATE('3Dt088T2LCZ8syPW6WoxWT',$,'TimeConstant','The time constant of the sensor.',.P_SINGLEVALUE.,'IfcTimeMeasure','',$,$,$,$,.READWRITE.);
#434= IFCLIBRARYREFERENCE($,$,'\X2\66425B9A6570\X0\','\X2\30BB30F330B5306E66425B9A65703002\X0\','ja-JP',#2);
#435= IFCRELASSOCIATESLIBRARY('32Nu9ZOu11agjUI4sJo3we',$,$,$,(#433),#434);
#436= IFCLIBRARYREFERENCE($,$,'\X2\C2DCC815\X0\','\X2\C13CC11CC758\X0\ \X2\C2DCC815\X0\.','ko-KR',#2);
#437= IFCRELASSOCIATESLIBRARY('2yxsCBym59afFTsZP2dPH7',$,$,$,(#433),#436);
#438= IFCPROPERTYSETTEMPLATE('3LCir3CVv3vBs7DvjZTs_p',$,'Pset_SensorTypeFlowSensor','A device that senses or detects flow. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/FLOWSENSOR',(#441));
#439= IFCLIBRARYREFERENCE($,$,$,'\X2\6D41308C3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#440= IFCRELASSOCIATESLIBRARY('1gjt5_e4f4J9jgJIci2ukV',$,$,$,(#438),#439);
#441= IFCSIMPLEPROPERTYTEMPLATE('3Zf6YA8iT7O8D7l3JnBbfQ',$,'SetPointFlow','The volumetric flow value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcVolumetricFlowRateMeasure','',$,$,$,$,.READWRITE.);
#442= IFCLIBRARYREFERENCE($,$,'\X2\6D4191CF8A2D5B9A5024\X0\','\X2\611F77E53055308C308B6D4191CF3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#443= IFCRELASSOCIATESLIBRARY('1riRtcjlz5uxHz_kEv6l2Z',$,$,$,(#441),#442);
#444= IFCLIBRARYREFERENCE($,$,'\X2\C720B7C9\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C720B7C9\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#445= IFCRELASSOCIATESLIBRARY('04qFz8XKP28OdIVr1FcTQ8',$,$,$,(#441),#444);
#446= IFCPROPERTYSETTEMPLATE('1Zn6lU_Fb2GRX9V8ZhxzWJ',$,'Pset_SensorTypeGasSensor','A device that senses or detects gas. HISTORY: Changed in IFC4. Gas detected made into enumeration, set point concentration and coverage area added. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/GASSENSOR',(#449,#452,#455));
#447= IFCLIBRARYREFERENCE($,$,$,'\X2\30AC30B93092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#448= IFCRELASSOCIATESLIBRARY('3FJbDI37XENehiQVlblpP1',$,$,$,(#446),#447);
#449= IFCSIMPLEPROPERTYTEMPLATE('1_iQDbgcn8S8trQ95QEd0c',$,'GasDetected','Identification of the gas that is being detected, according to chemical formula.  For example, carbon monoxide is ''CO'', carbon dioxide is ''CO2'', oxygen is ''O2''.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#450= IFCLIBRARYREFERENCE($,$,'\X2\5BFE8C6130AC30B9\X0\','\X2\691C51FA3055308C30663044308B30AC30B9306E8B5852253002\X0\','ja-JP',#2);
#451= IFCRELASSOCIATESLIBRARY('2bjGZC36v4netFts2Qogxq',$,$,$,(#449),#450);
#452= IFCSIMPLEPROPERTYTEMPLATE('31aD7KqyT7rQDHwqks9AqK',$,'SetPointConcentration','The gas concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPositiveRatioMeasure','',$,$,$,$,.READWRITE.);
#453= IFCLIBRARYREFERENCE($,$,'\X2\30AC30B96FC35EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B30AC30B96FC35EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#454= IFCRELASSOCIATESLIBRARY('16B2xg9ff0yeHz3eqYDUfw',$,$,$,(#452),#453);
#455= IFCSIMPLEPROPERTYTEMPLATE('0F1M3yN5zEdRh5YjBs$5s6',$,'CoverageArea','The floor area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).',.P_SINGLEVALUE.,'IfcAreaMeasure','',$,$,$,$,.READWRITE.);
#456= IFCLIBRARYREFERENCE($,$,'\X2\6E2C5B9A7BC456F2\X0\','\X2\30BB30F330B5306730AB30D030FC3055308C30663044308B5E8A97627A4D3002\X0\(\X2\901A5E38300130BB30F330BF30FC304C30BB30F330B5306E4F4D7F6E306B3042308B51863068305730666E2C5B9A3055308C308B\X0\)','ja-JP',#2);
#457= IFCRELASSOCIATESLIBRARY('2gs9mrvMDAweoE3qDQadVA',$,$,$,(#455),#456);
#458= IFCPROPERTYSETTEMPLATE('2ueSHixHD64QAuvGG9ippa',$,'Pset_SensorTypeHeatSensor','A device that senses or detects heat. HISTORY: In IFC4, incorporates Fire Sensor. HeatSensorSetPoint changed to SetPointTemperature',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/HEATSENSOR',(#461,#466,#471));
#459= IFCLIBRARYREFERENCE($,$,$,'\X2\71B13092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#460= IFCRELASSOCIATESLIBRARY('0glJe1_Hf9LvsuaUjr0VPQ',$,$,$,(#458),#459);
#461= IFCSIMPLEPROPERTYTEMPLATE('2NYHEoWbLCoQ2KwwWs6Fvk',$,'CoverageArea','The area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).',.P_SINGLEVALUE.,'IfcAreaMeasure','',$,$,$,$,.READWRITE.);
#462= IFCLIBRARYREFERENCE($,$,'\X2\6E2C5B9A7BC456F2\X0\','\X2\30BB30F330B5306730AB30D030FC3055308C30663044308B7BC456F23002\X0\(\X2\901A5E38300130BB30F330BF30FC304C30BB30F330B5306E4F4D7F6E306B3042308B51863068305730666E2C5B9A3055308C308B\X0\)','ja-JP',#2);
#463= IFCRELASSOCIATESLIBRARY('1h2B5XgV57Hu5ykdZzA3K8',$,$,$,(#461),#462);
#464= IFCLIBRARYREFERENCE($,$,'\X2\CE21C815\X0\ \X2\BC94C704\X0\','\X2\C13CC11C\X0\ \X2\CEE4BC84D558B294\X0\ \X2\BC94C704\X0\. (\X2\C77CBC18C801C73CB85C\X0\ \X2\C13CD130\X0\ \X2\C13CC11CC758\X0\ \X2\C704CE58C5D0C788B294\X0\ \X2\C6D0D615C73CB85C\X0\ \X2\CE21C815B418B294\X0\)','ko-KR',#2);
#465= IFCRELASSOCIATESLIBRARY('1CkLl4wGD8gwla$KcxMfhG',$,$,$,(#461),#464);
#466= IFCSIMPLEPROPERTYTEMPLATE('13_b3IxSj7g8uybQZEAx2P',$,'SetPointTemperature','The temperature value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#467= IFCLIBRARYREFERENCE($,$,'\X2\6E295EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B6E295EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#468= IFCRELASSOCIATESLIBRARY('0OTOWSHLD1EgfZJChZWxX2',$,$,$,(#466),#467);
#469= IFCLIBRARYREFERENCE($,$,'\X2\C628B3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C628B3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#470= IFCRELASSOCIATESLIBRARY('1hl7bxhrrAPv_yMzGLjLRV',$,$,$,(#466),#469);
#471= IFCSIMPLEPROPERTYTEMPLATE('2uJjgLMsv09OUQXXWYx6NH',$,'RateOfTemperatureRise','The rate of temperature rise that is to be sensed as being hazardous.',.P_SINGLEVALUE.,'IfcTemperatureRateOfChangeMeasure','',$,$,$,$,.READWRITE.);
#472= IFCLIBRARYREFERENCE($,$,'\X2\6E295EA64E0A66077387\X0\','\X2\5371967A30673042308B306830573066611F30583089308C308B30533068306B306A306330663044308B6E295EA64E0A660773873002\X0\','ja-JP',#2);
#473= IFCRELASSOCIATESLIBRARY('0SOmGdSrr8LvAzS5HZmx8F',$,$,$,(#471),#472);
#474= IFCLIBRARYREFERENCE($,$,'\X2\C628B3C4\X0\ \X2\C0C1C2B9B960\X0\','\X2\C704D5D8\X0\ \X2\AC83C73CB85C\X0\ \X2\B290AEF4C9C0AC8CD558B294\X0\ \X2\C628B3C4\X0\ \X2\C0C1C2B9B960\X0\.','ko-KR',#2);
#475= IFCRELASSOCIATESLIBRARY('3hVgVzwpTFiBbWOhIfJad1',$,$,$,(#471),#474);
#476= IFCPROPERTYSETTEMPLATE('0d_BIHbObE6BSjKe$IvjNt',$,'Pset_SensorTypeHumiditySensor','A device that senses or detects humidity. HISTORY: HumiditySensorSetPoint changed to SetPointHumidity. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/HUMIDITYSENSOR',(#479));
#477= IFCLIBRARYREFERENCE($,$,$,'\X2\6E7F5EA63092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#478= IFCRELASSOCIATESLIBRARY('3o67cjEYX7c85tDlN9hGqe',$,$,$,(#476),#477);
#479= IFCSIMPLEPROPERTYTEMPLATE('1X2ssWcdr0OeMgqOZgkMsy',$,'SetPointHumidity','The humidity value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPositiveRatioMeasure','',$,$,$,$,.READWRITE.);
#480= IFCLIBRARYREFERENCE($,$,'\X2\6E7F5EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B6E7F5EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#481= IFCRELASSOCIATESLIBRARY('13Rl5S3xr1sAJxI9etOR0k',$,$,$,(#479),#480);
#482= IFCLIBRARYREFERENCE($,$,'\X2\C2B5B3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C2B5B3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#483= IFCRELASSOCIATESLIBRARY('3E_np20Y98PA_ISgjt4TDn',$,$,$,(#479),#482);
#484= IFCPROPERTYSETTEMPLATE('2dswSIuTLCx9jFnTFZK22S',$,'Pset_SensorTypeIonConcentrationSensor','A device that senses or detects ion concentration such as water hardness. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/IONCONCENTRATIONSENSOR',(#487,#492));
#485= IFCLIBRARYREFERENCE($,$,$,'\X2\6C34306E786C5EA6306A3069306E30A430AA30F36FC35EA63092611F77E5307E305F306F691C51FA3059308B88C57F6E\X0\','ja-JP',#2);
#486= IFCRELASSOCIATESLIBRARY('2eZQ4PvWH7ig9jVYaEcA7X',$,$,$,(#484),#485);
#487= IFCSIMPLEPROPERTYTEMPLATE('1y2MfKDRXC7AvP9p0tZqcU',$,'SubstanceDetected','Identification of the substance that is being detected according to chemical formula.  For example, calcium carbonate is ''CaCO3''',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#488= IFCLIBRARYREFERENCE($,$,'\X2\5BFE8C6172698CEA\X0\','\X2\691C51FA3055308C30663044308B72698CEA306E8B5852253002\X0\','ja-JP',#2);
#489= IFCRELASSOCIATESLIBRARY('2O81z$qDT08OVfKDarxL_u',$,$,$,(#487),#488);
#490= IFCLIBRARYREFERENCE($,$,'\X2\B300C0C1\X0\ \X2\BB3CC9C8\X0\','\X2\AC80CD9CB418B294\X0\ \X2\BB3CC9C8C758\X0\ \X2\C2DDBCC4\X0\.','ko-KR',#2);
#491= IFCRELASSOCIATESLIBRARY('3q9nHZdOHEtfgcWiLL_SIa',$,$,$,(#487),#490);
#492= IFCSIMPLEPROPERTYTEMPLATE('27bY56a4bBSeEd6zl8bQRv',$,'SetPointConcentration','The ion concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcIonConcentrationMeasure','',$,$,$,$,.READWRITE.);
#493= IFCLIBRARYREFERENCE($,$,'\X2\30A430AA30F36FC35EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B30A430AA30F36FC35EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#494= IFCRELASSOCIATESLIBRARY('1QgnosC6XAXBnlfZH3PFEA',$,$,$,(#492),#493);
#495= IFCLIBRARYREFERENCE($,$,'\X2\C774C628\X0\ \X2\B18DB3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C774C628\X0\ \X2\B18DB3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#496= IFCRELASSOCIATESLIBRARY('2RkrHGAen8NRruQwpA7N9c',$,$,$,(#492),#495);
#497= IFCPROPERTYSETTEMPLATE('2Ppe9KAsrBnOFxEuvxU3HD',$,'Pset_SensorTypeLevelSensor','A device that senses or detects fill level.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/LEVEL',(#500));
#498= IFCLIBRARYREFERENCE($,$,$,'\X2\30EC30D930EB3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#499= IFCRELASSOCIATESLIBRARY('0f0kP0XMP0aB14CYwnGBha',$,$,$,(#497),#498);
#500= IFCSIMPLEPROPERTYTEMPLATE('3iPkIQkdH2MfOng8PGvfNE',$,'SetPointLevel','The fill level value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPositiveLengthMeasure','',$,$,$,$,.READWRITE.);
#501= IFCLIBRARYREFERENCE($,$,'\X2\30EC30D930EB8A2D5B9A5024\X0\','\X2\611F77E53055308C308B30EC30D930EB3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#502= IFCRELASSOCIATESLIBRARY('2IPzUuawvFegeA$E1lDVS6',$,$,$,(#500),#501);
#503= IFCLIBRARYREFERENCE($,$,'\X2\B808BCA8\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C218C900\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#504= IFCRELASSOCIATESLIBRARY('3KY$9BqvfFW9_ESJAxN$Cy',$,$,$,(#500),#503);
#505= IFCPROPERTYSETTEMPLATE('1HweyhYEPCPA7wfdwjMb80',$,'Pset_SensorTypeLightSensor','A device that senses or detects light. HISTORY: LightSensorSensorSetPoint changed to SetPointIlluminance. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/LIGHTSENSOR',(#508));
#506= IFCLIBRARYREFERENCE($,$,$,'\X2\51493092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#507= IFCRELASSOCIATESLIBRARY('1qXu3IlUr9EOJF3ciSDCV$',$,$,$,(#505),#506);
#508= IFCSIMPLEPROPERTYTEMPLATE('24uwujziXD3PqY_RiAGWzy',$,'SetPointIlluminance','The illuminance value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcIlluminanceMeasure','',$,$,$,$,.READWRITE.);
#509= IFCLIBRARYREFERENCE($,$,'\X2\71675EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B71675EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#510= IFCRELASSOCIATESLIBRARY('1tdR8UOefDLQd1gErRxAvt',$,$,$,(#508),#509);
#511= IFCLIBRARYREFERENCE($,$,'\X2\C870B3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0D558B294\X0\ \X2\C870B3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#512= IFCRELASSOCIATESLIBRARY('3ooWeQFRD8tx6aq_5GNk43',$,$,$,(#508),#511);
#513= IFCPROPERTYSETTEMPLATE('27Xrk0pZ1Evx0d3xp6toqV',$,'Pset_SensorTypeMoistureSensor','A device that senses or detects moisture. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/MOISTURESENSOR',(#516));
#514= IFCLIBRARYREFERENCE($,$,$,'\X2\6C3452063092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#515= IFCRELASSOCIATESLIBRARY('1gUbetbf50bhhP$pkrelvB',$,$,$,(#513),#514);
#516= IFCSIMPLEPROPERTYTEMPLATE('0lZne1psPEZAlee2qxNrGi',$,'SetPointMoisture','The moisture value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPositiveRatioMeasure','',$,$,$,$,.READWRITE.);
#517= IFCLIBRARYREFERENCE($,$,'\X2\6C3452068A2D5B9A5024\X0\','\X2\611F77E53055308C308B6C3452063002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#518= IFCRELASSOCIATESLIBRARY('1F1YJYcDT2pxiJf4rj5EgK',$,$,$,(#516),#517);
#519= IFCLIBRARYREFERENCE($,$,'\X2\C218BD84\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C218BD84\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#520= IFCRELASSOCIATESLIBRARY('3hGgtzXcHDthMSRWUZRD3C',$,$,$,(#516),#519);
#521= IFCPROPERTYSETTEMPLATE('0JbKjJ_6j6vBCo00PdRNtt',$,'Pset_SensorTypeMovementSensor','A device that senses or detects movement. HISTORY: In IFC4, time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/MOVEMENTSENSOR',(#522,#524));
#522= IFCSIMPLEPROPERTYTEMPLATE('1AlCDwqmb9SeuOcKZhNpm3',$,'MovementSensingType','Enumeration that identifies the type of movement sensing mechanism.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#523,$,$,$,.READWRITE.);
#523= IFCPROPERTYENUMERATION('PEnum_MovementSensingType',(IFCLABEL('PHOTOELECTRICCELL'),IFCLABEL('PRESSUREPAD'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#524= IFCSIMPLEPROPERTYTEMPLATE('0vkRPz7Vf1C8VT24kREJZO',$,'SetPointMovement','The movement to be sensed.',.P_BOUNDEDVALUE.,'IfcPositiveRatioMeasure','',$,$,$,$,.READWRITE.);
#525= IFCPROPERTYSETTEMPLATE('2fUklnz7L88OYg_L$RZXht',$,'Pset_SensorTypePHSensor','A device that senses or detects acidity.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/PHSENSOR',(#528));
#526= IFCLIBRARYREFERENCE($,$,$,'\X2\917860275EA63092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#527= IFCRELASSOCIATESLIBRARY('2nwVO1KNz3rOeIO3HKdXgt',$,$,$,(#525),#526);
#528= IFCSIMPLEPROPERTYTEMPLATE('1BsjlYALX8igoGkUkwtBwq',$,'SetPointPH','The fill level value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPHMeasure','',$,$,$,$,.READWRITE.);
#529= IFCLIBRARYREFERENCE($,$,'\X2\917860275EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B917860275EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#530= IFCRELASSOCIATESLIBRARY('1UmY$TRxr3q8A3DpE$kxl7',$,$,$,(#528),#529);
#531= IFCLIBRARYREFERENCE($,$,'\X2\C0B0C131B3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C0B0B3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#532= IFCRELASSOCIATESLIBRARY('1aZuKyOwXF$wD5lhwr1Vcw',$,$,$,(#528),#531);
#533= IFCPROPERTYSETTEMPLATE('3H7_QOSebASO3dF_6IkcAT',$,'Pset_SensorTypePressureSensor','A device that senses or detects pressure. HISTORY: PressureSensorSensorSetPoint changed to SetPointPressure. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/PRESSURESENSOR',(#536,#541));
#534= IFCLIBRARYREFERENCE($,$,$,'\X2\5727529B3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#535= IFCRELASSOCIATESLIBRARY('1yao8lXZz68wd9Qwk5zF4G',$,$,$,(#533),#534);
#536= IFCSIMPLEPROPERTYTEMPLATE('0VruhW9pjAihdfIddgBiO$',$,'SetPointPressure','The pressure value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPressureMeasure','',$,$,$,$,.READWRITE.);
#537= IFCLIBRARYREFERENCE($,$,'\X2\5727529B8A2D5B9A5024\X0\','\X2\611F77E53055308C308B5727529B3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#538= IFCRELASSOCIATESLIBRARY('3qtl2WRK9F1PBIBYDFHGOP',$,$,$,(#536),#537);
#539= IFCLIBRARYREFERENCE($,$,'\X2\C555B825\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C555B825\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#540= IFCRELASSOCIATESLIBRARY('0vnW6czbD7s8gUfppUhloB',$,$,$,(#536),#539);
#541= IFCSIMPLEPROPERTYTEMPLATE('3h_X_YJlL2JBzet_KGp9Jr',$,'IsSwitch','Identifies if the sensor also functions as a switch at the set point (=TRUE) or not (= FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#542= IFCLIBRARYREFERENCE($,$,'\X2\30B930A430C330C16A5F80FD306E67097121\X0\','\X2\30BB30F330B530FC304C8A2D5B9A5024306730B930A430C330C13068305730666A5F80FD3059308BFF08\X0\TRUE)\X2\304B30015426304BFF08\X0\FALSE)\X2\30928B5852253059308B3002\X0\','ja-JP',#2);
#543= IFCRELASSOCIATESLIBRARY('3gu1eg_CX1ix4h21Gv617g',$,$,$,(#541),#542);
#544= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\AE30B2A5C758\X0\ \X2\C720BB34\X0\','\X2\C13CC11C\X0\ \X2\C124C815C5D0C11C\X0\ \X2\C2A4C704CE58\X0\ \X2\C5EDD560\X0\ (TRUE) \X2\B610B294\X0\ \X2\C5ECBD80\X0\ (FALSE)\X2\B97C\X0\ \X2\D655C778D55CB2E4\X0\.','ko-KR',#2);
#545= IFCRELASSOCIATESLIBRARY('1adlPu79LBt8uX8bNlqvvP',$,$,$,(#541),#544);
#546= IFCPROPERTYSETTEMPLATE('1N21pTWA90UhP3NOUM15E$',$,'Pset_SensorTypeRadiationSensor','A device that senses or detects radiation. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/RADIATIONSENSOR',(#549));
#547= IFCLIBRARYREFERENCE($,$,$,'\X2\653E5C047DDA3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#548= IFCRELASSOCIATESLIBRARY('3_R2Ce6799auhrlA3NR0sI',$,$,$,(#546),#547);
#549= IFCSIMPLEPROPERTYTEMPLATE('2fEm$Y1yb3lfXZX9evxGIW',$,'SetPointRadiation','The radiation power value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPowerMeasure','',$,$,$,$,.READWRITE.);
#550= IFCLIBRARYREFERENCE($,$,'\X2\653E5C047DDA8A2D5B9A5024\X0\','\X2\611F77E53055308C308B653E5C047DDA91CF3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#551= IFCRELASSOCIATESLIBRARY('0LFPxkSHrCKAg5M_7lZTz2',$,$,$,(#549),#550);
#552= IFCLIBRARYREFERENCE($,$,'\X2\BC29C0ACC120\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\BC29C0ACC120\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#553= IFCRELASSOCIATESLIBRARY('2s0u4xeeT26PBYj7SqtvlQ',$,$,$,(#549),#552);
#554= IFCPROPERTYSETTEMPLATE('3b3i4hFar6MuSNkImK3IgM',$,'Pset_SensorTypeRadioactivitySensor','A device that senses or detects atomic decay. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/RADIOACTIVITYSENSOR',(#557));
#555= IFCLIBRARYREFERENCE($,$,$,'\X2\539F5B506838306E5D2958CA3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#556= IFCRELASSOCIATESLIBRARY('1NyTaDNCb5Wg9tduJ55scO',$,$,$,(#554),#555);
#557= IFCSIMPLEPROPERTYTEMPLATE('0xJRZ1dYP4YhPhhQS0hG6n',$,'SetPointRadioactivity','The radioactivity value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcRadioActivityMeasure','',$,$,$,$,.READWRITE.);
#558= IFCLIBRARYREFERENCE($,$,'\X2\653E5C0480FD8A2D5B9A5024\X0\','\X2\611F77E53055308C308B653E5C0480FD3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#559= IFCRELASSOCIATESLIBRARY('1e6NdBJD15wgLOU869W5s8',$,$,$,(#557),#558);
#560= IFCLIBRARYREFERENCE($,$,'\X2\BC29C0ACB2A5\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\BC29C0ACB2A5\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#561= IFCRELASSOCIATESLIBRARY('01pe4MeZ90l9wuJ6co1YdV',$,$,$,(#557),#560);
#562= IFCPROPERTYSETTEMPLATE('2wZ5fOJ7n9$Qzo0IptCrDU',$,'Pset_SensorTypeSmokeSensor','A device that senses or detects smoke. HISTORY: PressureSensorSensorSetPoint (error in previous release) changed to SetPointConcentration. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/SMOKESENSOR',(#565,#570,#575));
#563= IFCLIBRARYREFERENCE($,$,$,'\X2\71593092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#564= IFCRELASSOCIATESLIBRARY('2lfQSZ$3D8GglydcUbjWF3',$,$,$,(#562),#563);
#565= IFCSIMPLEPROPERTYTEMPLATE('3Rn6dlSF58ggBjdjC3LCbt',$,'CoverageArea','The floor area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).',.P_SINGLEVALUE.,'IfcAreaMeasure','',$,$,$,$,.READWRITE.);
#566= IFCLIBRARYREFERENCE($,$,'\X2\6E2C5B9A7BC456F2\X0\','\X2\30BB30F330B5306730AB30D030FC3055308C30663044308B5E8A97627A4D3002\X0\(\X2\901A5E38300130BB30F330BF30FC304C30BB30F330B5306E4F4D7F6E306B3042308B51863068305730666E2C5B9A3055308C308B\X0\)','ja-JP',#2);
#567= IFCRELASSOCIATESLIBRARY('3rs2zHywXEnwvLo2QPePgK',$,$,$,(#565),#566);
#568= IFCLIBRARYREFERENCE($,$,'\X2\CE21C815\X0\ \X2\BC94C704\X0\','\X2\C13CC11C\X0\ \X2\CEE4BC84B418B294\X0\ \X2\BC14B2E5\X0\ \X2\BA74C801\X0\. (\X2\C77CBC18C801C73CB85C\X0\ \X2\C13CD130\X0\ \X2\C13CC11CC758\X0\ \X2\C704CE58C5D0C788B294\X0\ \X2\C6D0D615C73CB85C\X0\ \X2\CE21C815B418B294\X0\)','ko-KR',#2);
#569= IFCRELASSOCIATESLIBRARY('0piFa4pcL9RhPwz4qeB2W1',$,$,$,(#565),#568);
#570= IFCSIMPLEPROPERTYTEMPLATE('3Gn5On6Gj7TBNfaWGXl_D2',$,'SetPointConcentration','The smoke concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcPositiveRatioMeasure','',$,$,$,$,.READWRITE.);
#571= IFCLIBRARYREFERENCE($,$,'\X2\71596FC35EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B71596FC35EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#572= IFCRELASSOCIATESLIBRARY('2AAFZ2TabB4A9yMg9_dkRE',$,$,$,(#570),#571);
#573= IFCLIBRARYREFERENCE($,$,'\X2\C5F0AE30\X0\ \X2\B18DB3C4\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C5F0AE30\X0\ \X2\B18DB3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#574= IFCRELASSOCIATESLIBRARY('328nnga_DDCvJl4xwJkdH2',$,$,$,(#570),#573);
#575= IFCSIMPLEPROPERTYTEMPLATE('1dyey2hivFdQNfdv3kiX3$',$,'HasBuiltInAlarm','Indicates whether the smoke sensor is included as an element within a smoke alarm/sensor unit (TRUE) or not (FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#576= IFCLIBRARYREFERENCE($,$,'\X2\71598B6658315668306B542B307E308C30663044308B304B\X0\','\X2\715930BB30F330B530FC304C71598B66583130BB30F330B530E630CB30C330C8306E4E2D306B89817D20306830573066542B307E308C30663044308B304B\X0\(TRUE)\X2\30015426304B\X0\(FALSE)\X2\30928B5852253059308B3002\X0\','ja-JP',#2);
#577= IFCRELASSOCIATESLIBRARY('3do3mmrSzAB9DES6GKhqyc',$,$,$,(#575),#576);
#578= IFCLIBRARYREFERENCE($,$,'\X2\C5F0AE30\X0\ \X2\ACBDBCF4AE30C5D0\X0\ \X2\D3ECD568C5ECBD80\X0\','\X2\C5F0AE30\X0\ \X2\C13CC11CAC00\X0\ \X2\D654C7AC\X0\ \X2\ACBDBCF4\X0\ \X2\C13CC11C\X0\ \X2\C720B2DBC758\X0\ \X2\C694C18CB85C\X0\ \X2\D3ECD568B418C5B4\X0\ \X2\C788B294C9C0\X0\ (TRUE) \X2\C5ECBD80\X0\ (FALSE)\X2\B97C\X0\ \X2\D655C778D55CB2E4\X0\.','ko-KR',#2);
#579= IFCRELASSOCIATESLIBRARY('1jvAd1G0vBoOmFszxlyZTy',$,$,$,(#575),#578);
#580= IFCPROPERTYSETTEMPLATE('1tmy$ZChP25wTjXRkpJtVh',$,'Pset_SensorTypeSoundSensor','A device that senses or detects sound. HISTORY: SoundSensorSensorSetPoint changed to SetPointSound. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/SOUNDSENSOR',(#583));
#581= IFCLIBRARYREFERENCE($,$,$,'\X2\97F33092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#582= IFCRELASSOCIATESLIBRARY('2Y1uu_L4nAr9EIKtYRGa4G',$,$,$,(#580),#581);
#583= IFCSIMPLEPROPERTYTEMPLATE('16B_4$0$X2SQH0NVFEmozr',$,'SetPointSound','The sound pressure value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcSoundPressureMeasure','',$,$,$,$,.READWRITE.);
#584= IFCLIBRARYREFERENCE($,$,'\X2\97F357278A2D5B9A5024\X0\','\X2\611F77E53055308C308B97F357273002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#585= IFCRELASSOCIATESLIBRARY('1KricTp3L4Z9SC_3dVaraQ',$,$,$,(#583),#584);
#586= IFCLIBRARYREFERENCE($,$,'\X2\C74DC555\X0\ \X2\C124C815CE58\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C74CC555\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#587= IFCRELASSOCIATESLIBRARY('0Vs6Uw6YHClQxKaDg9y1sI',$,$,$,(#583),#586);
#588= IFCPROPERTYSETTEMPLATE('03y_O0w993gRMcJdmFM6hK',$,'Pset_SensorTypeTemperatureSensor','A device that senses or detects temperature. HISTORY: TemperatureSensorSensorSetPoint changed to SetPointTemperature. Range, accuracy and time constant deleted.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/TEMPERATURESENSOR',(#591,#597));
#589= IFCLIBRARYREFERENCE($,$,$,'\X2\6E295EA63092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#590= IFCRELASSOCIATESLIBRARY('1x_wxVAzH039g6ivsVHBQV',$,$,$,(#588),#589);
#591= IFCSIMPLEPROPERTYTEMPLATE('1FolJl1L96dAidIYhaWwHb',$,'TemperatureSensorType','Enumeration that Identifies the types of temperature sensor that can be specified.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#592,$,$,$,.READWRITE.);
#592= IFCPROPERTYENUMERATION('PEnum_TemperatureSensorType',(IFCLABEL('HIGHLIMIT'),IFCLABEL('LOWLIMIT'),IFCLABEL('OUTSIDETEMPERATURE'),IFCLABEL('OPERATINGTEMPERATURE'),IFCLABEL('ROOMTEMPERATURE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#593= IFCLIBRARYREFERENCE($,$,'\X2\6E295EA630BB30F330B530FC30BF30A430D7\X0\','\X2\660E793A3055308C305F6E295EA630BB30F330B530FC306E30BF30A430D730928B5852253059308B4E0089A73002\X0\','ja-JP',#2);
#594= IFCRELASSOCIATESLIBRARY('0kn2Thlfr6HvyJ9QYFSC9U',$,$,$,(#591),#593);
#595= IFCLIBRARYREFERENCE($,$,'\X2\C628B3C4\X0\ \X2\C13CC11C\X0\ \X2\D0C0C785\X0\','\X2\BA85C2DCB41C\X0\ \X2\C628B3C4\X0\ \X2\C13CC11C\X0\ \X2\C720D615C744\X0\ \X2\C2DDBCC4D558B294\X0\ \X2\BAA9B85D\X0\.','ko-KR',#2);
#596= IFCRELASSOCIATESLIBRARY('3LJXSegqz2H9Mqua20ZsKp',$,$,$,(#591),#595);
#597= IFCSIMPLEPROPERTYTEMPLATE('1smEJT0R120u2ZDMYs73cl',$,'SetPointTemperature','The temperature value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_BOUNDEDVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#598= IFCLIBRARYREFERENCE($,$,'\X2\6E295EA68A2D5B9A5024\X0\','\X2\611F77E53055308C308B6E295EA63002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#599= IFCRELASSOCIATESLIBRARY('33JQWKD41BcwW00s80GyRg',$,$,$,(#597),#598);
#600= IFCLIBRARYREFERENCE($,$,'\X2\C628B3C4\X0\ \X2\C131C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\C628B3C4\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#601= IFCRELASSOCIATESLIBRARY('2fTLz1JPn7bR_C_ixrOrJ1',$,$,$,(#597),#600);
#602= IFCPROPERTYSETTEMPLATE('02s4EWN_164ObixPPc4dlG',$,'Pset_SensorTypeWindSensor','A device that senses or detects wind speed and direction. HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSensor/WINDSENSOR',(#605,#611));
#603= IFCLIBRARYREFERENCE($,$,$,'\X2\98A8901F3092611F77E5307E305F306F691C51FA3059308B30C730D030A430B93002\X0\','ja-JP',#2);
#604= IFCRELASSOCIATESLIBRARY('23WCekXrrEM8rLVfgysgdu',$,$,$,(#602),#603);
#605= IFCSIMPLEPROPERTYTEMPLATE('1IA6nxQYT2dBGpFeiS7sYa',$,'WindSensorType','Enumeration that Identifies the types of wind sensors that can be specified.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#606,$,$,$,.READWRITE.);
#606= IFCPROPERTYENUMERATION('PEnum_WindSensorType',(IFCLABEL('CUP'),IFCLABEL('WINDMILL'),IFCLABEL('HOTWIRE'),IFCLABEL('LASERDOPPLER'),IFCLABEL('SONIC'),IFCLABEL('PLATE'),IFCLABEL('TUBE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#607= IFCLIBRARYREFERENCE($,$,'\X2\98A830BB30F330B530FC30BF30A430D7\X0\','\X2\660E793A3055308C305F98A830BB30F330B530FC306E30BF30A430D730928B5852253059308B4E0089A73002\X0\','ja-JP',#2);
#608= IFCRELASSOCIATESLIBRARY('2qiu0gGO1A2e04Ue3k2x2s',$,$,$,(#605),#607);
#609= IFCLIBRARYREFERENCE($,$,'\X2\BC14B78C\X0\ \X2\C13CC11C\X0\ \X2\D0C0C785\X0\','\X2\BA85C2DCB41C\X0\ \X2\BC14B78C\X0\ \X2\C13CC11C\X0\ \X2\C720D615C744\X0\ \X2\C2DDBCC4D558B294\X0\ \X2\BAA9B85D\X0\.','ko-KR',#2);
#610= IFCRELASSOCIATESLIBRARY('13$liQXAX7gupPeFZ1QbiP',$,$,$,(#605),#609);
#611= IFCSIMPLEPROPERTYTEMPLATE('2ZicLCMU1DLhgRkl_Jc_cx',$,'SetPointSpeed','The wind speed value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.',.P_SINGLEVALUE.,'IfcLinearVelocityMeasure','',$,$,$,$,.READWRITE.);
#612= IFCLIBRARYREFERENCE($,$,'\X2\98A8901F8A2D5B9A5024\X0\','\X2\611F77E53055308C308B98A8901F3002\X0\\X\0A\X2\30BB30C330C830DD30A430F330C8502430927F6E304F305F3081306B3001\X0\IfcPropertyBoundedValue.SetPointValue\X2\30924F7F75283059308B3002\X0\','ja-JP',#2);
#613= IFCRELASSOCIATESLIBRARY('2zpasVYzn08Ame$ktTcUj7',$,$,$,(#611),#612);
#614= IFCLIBRARYREFERENCE($,$,'\X2\D48DC18D\X0\ \X2\C124C815\X0\','\X2\AC10C9C0B418B294\X0\ \X2\BC14B78C\X0\. \X2\C138D2B8\X0\ \X2\D3ECC778D2B8\X0\ \X2\AC12C744\X0\ \X2\B123C73CB824BA74\X0\, IfcPropertyBoundedValue.SetPointValue\X2\B97C\X0\ \X2\C0ACC6A9D558C2EDC2DCC624\X0\.','ko-KR',#2);
#615= IFCRELASSOCIATESLIBRARY('1t7Pi_ldj8WOIl6U3pCqx7',$,$,$,(#611),#614);
#616= IFCPROPERTYSETTEMPLATE('12aLX7oA15mwIStDUK8Hz5',$,'Pset_UnitaryControlElementPHistory','Properties for history and operating schedules of thermostats.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcUnitaryControlElement',(#617,#618,#619,#620));
#617= IFCSIMPLEPROPERTYTEMPLATE('3FLDPmJx12$gQNiEEmBcrR',$,'Temperature','Indicates the current measured temperature.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcThermodynamicTemperatureMeasure',$,$,$,$,.READWRITE.);
#618= IFCSIMPLEPROPERTYTEMPLATE('3e2zuVhv1FtvdH$C6GH8TX',$,'Mode','Indicates operation mode corresponding to Pset_UnitaryControlTypeCommon.Mode.  For example, ''HEAT'', ''COOL'', ''AUTO''.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcIdentifier',$,$,$,$,.READWRITE.);
#619= IFCSIMPLEPROPERTYTEMPLATE('0TFzQxGhf0UPqUtwrqzDna',$,'Fan','Indicates fan operation where True is on, False is off, and Unknown is automatic.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcLogical',$,$,$,$,.READWRITE.);
#620= IFCSIMPLEPROPERTYTEMPLATE('2D$tjdlc185x7ciS7YW4xO',$,'SetPoint','Indicates the temperature setpoint.  For thermostats with setbacks or separate high and low setpoints, then the time series may contain a pair of values at each entry where the first value is the heating setpoint (low) and the second value is the cooling setpoint (high).',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcIdentifier',$,$,$,$,.READWRITE.);
#621= IFCPROPERTYSETTEMPLATE('3LxhzBdL9A9fnWEU8d4lni',$,'Pset_UnitaryControlElementTypeCommon','Unitary control element type common attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcUnitaryControlElement',(#624,#629,#633));
#622= IFCLIBRARYREFERENCE($,$,$,'\X2\53584E00306E30B330F330C830ED30FC30EB89817D20306E5171901A5C5E60273002\X0\','ja-JP',#2);
#623= IFCRELASSOCIATESLIBRARY('3fD$T8hZv9AxRaeXrgpxyG',$,$,$,(#621),#622);
#624= IFCSIMPLEPROPERTYTEMPLATE('20rrUNwtj7Ux9hMA_2$sxC',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#625= IFCLIBRARYREFERENCE($,$,'\X2\53C271678A1853F7\X0\','\X2\3053306E30D730ED30B830A730AF30C8306B304A3051308B53C271678A1853F7\X0\(\X2\4F8BFF1A\X0\A-1)\X2\30025206985E30B330FC30C93067306F306A304F518590E830674F7F75283055308C308B30D730ED30B830A730AF30C830BF30A430D73068305730664F7F75283055308C308B3082306E3002\X0\','ja-JP',#2);
#626= IFCRELASSOCIATESLIBRARY('2yUOyoeo1EYBDcJosWHbSM',$,$,$,(#624),#625);
#627= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\ ID','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0C11C\X0\ \X2\C0ACC6A9C774\X0\ \X2\C720D615C5D0\X0\ \X2\B300D55C\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : ''A-1'') \X2\203B\X0\ \X2\AE30BCF8C774C788B294\X0\ \X2\ACBDC6B0\X0\ \X2\ADF8\X0\ \X2\AE30D638B97C\X0\ \X2\C0ACC6A9\X0\','ko-KR',#2);
#628= IFCRELASSOCIATESLIBRARY('2zk3zCEL12gQKlARXPuAw8',$,$,$,(#624),#627);
#629= IFCSIMPLEPROPERTYTEMPLATE('3qvtvxj6T3Xw9hCVy2Kkml',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#630,$,$,$,.READWRITE.);
#630= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#631= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#632= IFCRELASSOCIATESLIBRARY('0WX6ukQkv1hPundzrJ7vGJ',$,$,$,(#629),#631);
#633= IFCSIMPLEPROPERTYTEMPLATE('03CIm_V$jF_QkvViYJV3TS',$,'Mode','Table mapping operation mode identifiers to descriptive labels, which may be used for interpreting Pset_UnitaryControlElementPHistory.Mode.',.P_TABLEVALUE.,'IfcIdentifier','IfcLabel',$,$,$,$,.READWRITE.);
#634= IFCPROPERTYSETTEMPLATE('0TlaCMilrFKfMn66MYJx02',$,'Pset_UnitaryControlElementTypeIndicatorPanel','Unitary control element type indicator panel attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcUnitaryControlElement/INDICATORPANEL',(#635));
#635= IFCSIMPLEPROPERTYTEMPLATE('1uPn5FUIn5sgkZUaVB64$J',$,'Application','The application of the unitary control element.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#636,$,$,$,.READWRITE.);
#636= IFCPROPERTYENUMERATION('PEnum_UnitaryControlElementApplication',(IFCLABEL('LiftPositionIndicator'),IFCLABEL('\X\0ALiftHallLantern'),IFCLABEL('\X\0ALiftArrivalGong'),IFCLABEL('\X\0ALiftCarDirectionLantern'),IFCLABEL('\X\0ALiftFireSystemsPort'),IFCLABEL('\X\0ALiftVoiceAnnouncer'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#637= IFCPROPERTYSETTEMPLATE('24tzYDHBDC4fqvkfFjpH4$',$,'Pset_UnitaryControlElementTypeThermostat','Unitary control element type thermostat attributes.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcUnitaryControlElement/THERMOSTAT',(#638));
#638= IFCSIMPLEPROPERTYTEMPLATE('346mpFu8r5uP7RXqtHrBBR',$,'TemperatureSetPoint','The temperature setpoint range and default setpoint.',.P_BOUNDEDVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#639= IFCPROPERTYSETTEMPLATE('1kTrg_Nq91xfOg37CNpbXz',$,'Pset_CableSegmentOccurrence','Properties for the occurrence of an electrical cable, core or conductor that conforms to a type as specified by an appropriate type definition within IFC. NOTE: Maximum allowed voltage drop should be derived from the property within Pset_ElectricalCircuit.',.PSET_OCCURRENCEDRIVEN.,'IfcCableSegment',(#640,#641,#642,#643,#644,#646,#647,#648,#649,#651,#652,#653,#654,#655));
#640= IFCSIMPLEPROPERTYTEMPLATE('3$_y1yiNHDVQI$cK5Sbdpn',$,'DesignAmbientTemperature','The highest and lowest local ambient temperature likely to be encountered.',.P_BOUNDEDVALUE.,'IfcThermodynamicTemperatureMeasure','',$,$,$,$,.READWRITE.);
#641= IFCSIMPLEPROPERTYTEMPLATE('0O3qx6Y0LDvfLaQoodeuKe',$,'UserCorrectionFactor','An arbitrary correction factor that may be applied by the user.',.P_SINGLEVALUE.,'IfcReal','',$,$,$,$,.READWRITE.);
#642= IFCSIMPLEPROPERTYTEMPLATE('16n7KB8XL0MffEJyqnIWY8',$,'NumberOfParallelCircuits','Number of parallel circuits.',.P_SINGLEVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#643= IFCSIMPLEPROPERTYTEMPLATE('33Kb0Ij4924hRF2FlG0bsC',$,'InstallationMethod','Method of installation of cable/conductor. Installation methods are typically defined by reference in standards such as IEC 60364-5-52, table 52A-1 or BS7871 Appendix 4 Table 4A1 etc. Selection of the value to be used should be determined from such a standard according to local usage.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#644= IFCSIMPLEPROPERTYTEMPLATE('3bXWjU7IjCYR_hnnOqyS8B',$,'InstallationMethodFlagEnum','Special installation conditions relating to particular types of installation based on IEC60364-5-52:2001 reference installation methods C and D.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#645,$,$,$,.READWRITE.);
#645= IFCPROPERTYENUMERATION('PEnum_InstallationMethodFlagEnum',(IFCLABEL('INDUCT'),IFCLABEL('INSOIL'),IFCLABEL('ONWALL'),IFCLABEL('BELOWCEILING'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#646= IFCSIMPLEPROPERTYTEMPLATE('0zVX3DVCHEyfG27l_lS5ED',$,'DistanceBetweenParallelCircuits','Distance measured between parallel circuits.',.P_SINGLEVALUE.,'IfcLengthMeasure','',$,$,$,$,.READWRITE.);
#647= IFCSIMPLEPROPERTYTEMPLATE('3lm4edBTP6awPIIPNa1vMc',$,'SoilConductivity','Thermal conductivity of soil. Generally, within standards such as IEC 60364-5-52, table 52A-16, the resistivity of soil is required (measured in [SI] units of degK.m /W). This is the reciprocal of the conductivity value and needs to be calculated accordingly.',.P_SINGLEVALUE.,'IfcThermalConductivityMeasure','',$,$,$,$,.READWRITE.);
#648= IFCSIMPLEPROPERTYTEMPLATE('01k0KqpHfEIfUQolMlm0uH',$,'CarrierStackNumber','Number of carrier segments (tray, ladder etc.) that are vertically stacked (vertical is measured as the z-axis of the local coordinate system of the carrier segment).',.P_SINGLEVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#649= IFCSIMPLEPROPERTYTEMPLATE('0ylC$obib4dRdCb5b9nMYA',$,'MountingMethod','The method of mounting cable segment occurrences on a cable carrier occurrence from which the method required can be selected. This is for the purpose of carrying out ''worst case'' cable sizing calculations and may be a conceptual requirement rather than a statement of the physical occurrences of cable and carrier segments.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#650,$,$,$,.READWRITE.);
#650= IFCPROPERTYENUMERATION('PEnum_MountingMethodEnum',(IFCLABEL('PERFORATEDTRAY'),IFCLABEL('LADDER'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#651= IFCSIMPLEPROPERTYTEMPLATE('17xSalWRvDbQSL4gCKlsbq',$,'IsHorizontalCable','Indication of whether the cable occurrences are mounted horizontally (= TRUE) or vertically (= FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#652= IFCSIMPLEPROPERTYTEMPLATE('1FVTJr4xzAHfCOef0GtMS1',$,'IsMountedFlatCable','Indication of whether the cable occurrences are mounted flat (= TRUE) or in a trefoil pattern (= FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#653= IFCSIMPLEPROPERTYTEMPLATE('1yr8lWPHv1TgUmesRdpWJz',$,'CurrentCarryingCapasity','Maximum value of electric current which can be carried continuously by a conductor, a device or an apparatus, under specified conditions without its steady-state temperature exceeding a  specified value. Based on IEC60826-11-13. NOTE: The temperature specified value is maximum Design Ambient Temperature.',.P_SINGLEVALUE.,'IfcElectricCurrentMeasure','',$,$,$,$,.READWRITE.);
#654= IFCSIMPLEPROPERTYTEMPLATE('2hrntQW31Aogg_FIr2esWt',$,'MaximumCableLength','Maximum cable length based on voltagedrop. NOTE: This value may also be specified as a constraint within an IFC model if required but is included within the property set at this stage pending implementation of the required capabilities within software applications.',.P_SINGLEVALUE.,'IfcLengthMeasure','',$,$,$,$,.READWRITE.);
#655= IFCSIMPLEPROPERTYTEMPLATE('2KRFizeUD8WQoXykUo20yb',$,'PowerLoss','Total loss of power across this cable.',.P_SINGLEVALUE.,'IfcElectricCurrentMeasure','',$,$,$,$,.READWRITE.);
#656= IFCPROPERTYSETTEMPLATE('3JiTIvluD0Mw$RNtC1wJXG',$,'Pset_CableSegmentTypeCommon','Properties for the definitions of electrical cable segments.',.PSET_TYPEDRIVENOVERRIDE.,'IfcCableSegment',(#659,#664));
#657= IFCLIBRARYREFERENCE($,$,$,'\X2\96FB6C1730B130FC30D630EB306B95A23059308B60278CEA306730B330A230845C0E96FB5E2F3001\X0\IFC\X2\306B30665B9A7FA93055308C305F30B330A230845C0E96FB5E2F306E60278CEA3002\X0\\X\0A\X2\6CE88A18FF0967005927306E8A315BB996FB57274F4E4E0B306F\X0\Pset_ElectricalCircuit\X2\5185304B30895B9A7FA93055308C308B3082306E30673042308B3002\X0\','ja-JP',#2);
#658= IFCRELASSOCIATESLIBRARY('1tPlLnXArENv2eSIDxfP7q',$,$,$,(#656),#657);
#659= IFCSIMPLEPROPERTYTEMPLATE('04D7ZqbCD5QwxmL2mODJtC',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#660= IFCLIBRARYREFERENCE($,$,'\X2\53C27167\X0\','\X2\5F538A7230D730ED30B830A730AF30C830675B9A7FA93059308B5F625F0F306E53C27167\X0\ID\X2\FF084F8BFF1A\X0\A-1)\X2\3001627F8A8D3055308C305F5206985E306B5B5857283057306A30443068304D306B4F7F75283055308C308B3002\X0\','ja-JP',#2);
#661= IFCRELASSOCIATESLIBRARY('3CoYTd_l54rghuik8BpN3b',$,$,$,(#659),#660);
#662= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\','\X2\D574B2F9D504B85CC81DD2B8C5D0\X0\ \X2\C815C758B3C4B2C8\X0\ \X2\D615C2DDC758\X0\ \X2\CC38C870\X0\ID (\X2\C608\X0\ : A-1) \X2\C2B9C778B41C\X0\ \X2\BD84B958C5D0\X0\ \X2\C874C7ACD558C9C0\X0\ \X2\C54AC744\X0\ \X2\B54C\X0\ \X2\C0ACC6A9B41CB2E4\X0\.','ko-KR',#2);
#663= IFCRELASSOCIATESLIBRARY('3EB7ituFP2K8cdnaoKDn$D',$,$,$,(#659),#662);
#664= IFCSIMPLEPROPERTYTEMPLATE('34Fm3XPDjBOwuGw3zA45_$',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#665,$,$,$,.READWRITE.);
#665= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#666= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#667= IFCRELASSOCIATESLIBRARY('3yV7pgPmH5DxUmml6GH19E',$,$,$,(#664),#666);
#668= IFCPROPERTYSETTEMPLATE('246ZGcarHCFAJXVeOP15xo',$,'Pset_CommunicationsAppliancePHistory','Captures realtime information for communications devices, such as for server farm energy usage.  HISTORY: Added in IFC4.',.PSET_PERFORMANCEDRIVEN.,'IfcCommunicationsAppliance',(#669));
#669= IFCSIMPLEPROPERTYTEMPLATE('3HyaiIHGvEz89UvO8Ou5Kf',$,'PowerState','Indicates the power state of the device where True is on and False is off.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcBoolean',$,$,$,$,.READWRITE.);
#670= IFCPROPERTYSETTEMPLATE('0RCmtSeEj7hPWXF8wPtx$F',$,'Pset_CommunicationsApplianceTypeCommon','Common properties for communications appliances.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcCommunicationsAppliance',(#673,#678));
#671= IFCLIBRARYREFERENCE($,$,$,'\X2\901A4FE16A5F5668306E5171901A30D730ED30D130C630A33002\X0\\X\0AIFC4\X2\306B30668FFD52A03002\X0\','ja-JP',#2);
#672= IFCRELASSOCIATESLIBRARY('2BltC$LnHDJAVCHX0jtXAQ',$,$,$,(#670),#671);
#673= IFCSIMPLEPROPERTYTEMPLATE('3CL_EvXcf5VAglXet$HDHS',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#674= IFCLIBRARYREFERENCE($,$,'\X2\53C27167\X0\','\X2\5F538A7230D730ED30B830A730AF30C830675B9A7FA93059308B5F625F0F306E53C27167\X0\ID\X2\FF084F8BFF1A\X0\A-1)\X2\3001627F8A8D3055308C305F5206985E306B5B5857283057306A30443068304D306B4F7F75283055308C308B3002\X0\','ja-JP',#2);
#675= IFCRELASSOCIATESLIBRARY('3hM69S4o1FMuXf2E8pLYSV',$,$,$,(#673),#674);
#676= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\','\X2\D574B2F9\X0\ \X2\D504B85CC81DD2B8C5D0\X0\ \X2\C815C758B41C\X0\ \X2\D615C2DDC758\X0\ \X2\CC38C870\X0\ ID (\X2\C608\X0\ : A-1) \X2\C2B9C778B41C\X0\ \X2\BD84B958C5D0\X0\ \X2\C874C7ACD558C9C0\X0\ \X2\C54AC744\X0\ \X2\B54C\X0\ \X2\C0ACC6A9B41CB2E4\X0\.','ko-KR',#2);
#677= IFCRELASSOCIATESLIBRARY('0e3Xd1Ehf32vZksO5ZM13c',$,$,$,(#673),#676);
#678= IFCSIMPLEPROPERTYTEMPLATE('1fkk4M5U98MRDadmsb3Fds',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#679,$,$,$,.READWRITE.);
#679= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#680= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#681= IFCRELASSOCIATESLIBRARY('0iWszW9pLBQwanLKHAtRMG',$,$,$,(#678),#680);
#682= IFCPROPERTYSETTEMPLATE('3smBkHUVz41gdFVVyfLt62',$,'Pset_SwitchingDeviceTypeCommon','A switching device is a device designed to make or break the current in one or more electric circuits.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice',(#685,#690,#694,#699,#705,#710,#715,#720));
#683= IFCLIBRARYREFERENCE($,$,$,'IEC 441-14-01\X2\306E5B9A7FA9\X0\: \X\0A\X2\520763DB88C57F6E306F3001\X0\1\X2\30644EE54E0A306E96FB6C1756DE8DEF306796FB6D413092906E65AD3059308B30883046306B8A2D8A083055308C305F88C57F6E306730593002\X0\','ja-JP',#2);
#684= IFCRELASSOCIATESLIBRARY('2X6jF3PPvE6wfns9QG$EjL',$,$,$,(#682),#683);
#685= IFCSIMPLEPROPERTYTEMPLATE('1nnoqOGRfB5gNjmdWQKS1e',$,'Reference','Reference ID for this specified type in this project (e.g. type ''A-1''), provided, if there is no classification reference to a recognized classification system used.',.P_SINGLEVALUE.,'IfcIdentifier','',$,$,$,$,.READWRITE.);
#686= IFCLIBRARYREFERENCE($,$,'\X2\53C27167\X0\','\X2\3053306E30D730ED30B830A730AF30C8\X0\ (\X2\4F8BFF0E\X0\ ''A-1''\X2\300030BF30A430D7306A3069\X0\)\X2\306763075B9A3055308C305F53C27167\X0\ID\X2\30028A8D30813089308C305F5206985E4F537CFB306E5206985E53C27167304C5B5857283057306A304458345408306B906975283055308C308B3002\X0\','ja-JP',#2);
#687= IFCRELASSOCIATESLIBRARY('0vbnT77gL8sPQgeSnt7Sej',$,$,$,(#685),#686);
#688= IFCLIBRARYREFERENCE($,$,'\X2\CC38C870\X0\','\X2\C774\X0\ \X2\D504B85CC81DD2B8\X0\ (\X2\C608\X0\ : ''A-1''\X2\C720D615\X0\ \X2\B4F1\X0\) \X2\C9C0C815B41C\X0\ \X2\CC38C870\X0\ ID. \X2\C778C815\X0\ \X2\BD84B958\X0\ \X2\CCB4ACC4C758\X0\ \X2\BD84B958\X0\ \X2\CC38C870AC00C5C6B294\X0\ \X2\ACBDC6B0C5D0\X0\ \X2\C801C6A9B41CB2E4\X0\.','ko-KR',#2);
#689= IFCRELASSOCIATESLIBRARY('3KY4TEKNbApB5nRren2Z2j',$,$,$,(#685),#688);
#690= IFCSIMPLEPROPERTYTEMPLATE('0VGiv0oWj1OfO4llAKIG5k',$,'Status','Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished,  "Temporary" - element will exists only temporary (like a temporary support structure).',.P_ENUMERATEDVALUE.,'IfcLabel',$,#691,$,$,$,.READWRITE.);
#691= IFCPROPERTYENUMERATION('PEnum_Status',(IFCLABEL('NEW'),IFCLABEL('EXISTING'),IFCLABEL('DEMOLISH'),IFCLABEL('TEMPORARY'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#692= IFCLIBRARYREFERENCE($,$,'\X2\72B6614B\X0\','\X2\89817D20FF084E3B306B30EA30CE30D930FC30B730E730F3307E305F306F65394FEE30D730ED30B830A730AF30C8306B304A30443066FF09306E72B6614B3002\X0\ \X2\72B6614B306F3001300C65B0898F\X0\(New)\X2\300DFF0D65B03057304F8FFD52A03055308C308B89817D203002300C65E25B58300DFF0D89817D20306F5B58572830573001304B30646B8B308A3082306E3002300C783458CA300DFF0D89817D20306F5B5857283057305F304C30015EC368C43055308C308B3082306E3002300C4E0066427684300DFF0D4E0066427684306B5B5857283059308B89817D20FF084E0066427684306B30B530DD30FC30C8305730663044308B69CB9020306E30883046306A3082306EFF093002\X0\','ja-JP',#2);
#693= IFCRELASSOCIATESLIBRARY('2RK2B5Vu131Q9Y6tCOV00I',$,$,$,(#690),#692);
#694= IFCSIMPLEPROPERTYTEMPLATE('3mtqJH47f0qAlCn2plt9IQ',$,'NumberOfGangs','Number of gangs/buttons on this switch.',.P_SINGLEVALUE.,'IfcInteger','',$,$,$,$,.READWRITE.);
#695= IFCLIBRARYREFERENCE($,$,'\X2\30DC30BF30F36570\X0\','\X2\30B930A430C330C1306E30DC30BF30F36570\X0\','ja-JP',#2);
#696= IFCRELASSOCIATESLIBRARY('2fucDv9p92RedQGsdGsasR',$,$,$,(#694),#695);
#697= IFCLIBRARYREFERENCE($,$,'\X2\BC84D2BC\X0\ \X2\C218\X0\','\X2\C2A4C704CE58\X0\ \X2\BC84D2BC\X0\ \X2\C218\X0\','ko-KR',#2);
#698= IFCRELASSOCIATESLIBRARY('2syQ1wi$T2tO4TsD8PTgzg',$,$,$,(#694),#697);
#699= IFCSIMPLEPROPERTYTEMPLATE('1mUKphBNfFDwttf90Q$NF2',$,'SwitchFunction','Indicates types of switches which differs in functionality.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#700,$,$,$,.READWRITE.);
#700= IFCPROPERTYENUMERATION('PEnum_SwitchFunctionType',(IFCLABEL('ONOFFSWITCH'),IFCLABEL('INTERMEDIATESWITCH'),IFCLABEL('DOUBLETHROWSWITCH'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#701= IFCLIBRARYREFERENCE($,$,'\X2\30B930A430C330C130BF30A430D7\X0\','\X2\6A5F80FD30543068306B7570306A308B30B930A430C330C1306E30BF30A430D73092793A3059\X0\','ja-JP',#2);
#702= IFCRELASSOCIATESLIBRARY('1bLGP_HG91MPix5XjiiGvD',$,$,$,(#699),#701);
#703= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\C720D615\X0\','\X2\AE30B2A5B9C8B2E4\X0\ \X2\B2E4B978\X0\ \X2\C2A4C704CE58\X0\ \X2\D0C0C785C744\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#704= IFCRELASSOCIATESLIBRARY('1vuTUBdJbDzQGT68NCfDtS',$,$,$,(#699),#703);
#705= IFCSIMPLEPROPERTYTEMPLATE('1Cr$y3Yab48fCngUBExUvO',$,'HasLock','Indication of whether a switching device has a key operated lock (=TRUE) or not (= FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#706= IFCLIBRARYREFERENCE($,$,'\X2\30ED30C330AF306E53EF5426\X0\','\X2\30B930A430C330C188C57F6E304C30AD30FC64CD4F5C306730ED30C330AF3059308B58345408306FFF08\X0\TRUE)\X2\3001305D30463067306A304458345408306FFF08\X0\FALSE)\X2\3092886830593002\X0\','ja-JP',#2);
#707= IFCRELASSOCIATESLIBRARY('3OUtU$n4H8p9kEKNonjWZu',$,$,$,(#705),#706);
#708= IFCLIBRARYREFERENCE($,$,'\X2\C7A0AE08C5ECBD80\X0\','\X2\C2A4C704CE58\X0\ \X2\C7A5CE58AC00\X0\ \X2\D0A4\X0\ \X2\C870C791C73CB85C\X0\ \X2\C7A0AE00\X0\ \X2\ACBDC6B0\X0\ (TRUE), \X2\ADF8B807C9C0\X0\ \X2\C54AC740\X0\ \X2\ACBDC6B0\X0\ (FALSE)\X2\C744\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#709= IFCRELASSOCIATESLIBRARY('3JvNdzkdD3feedxSFANzrz',$,$,$,(#705),#708);
#710= IFCSIMPLEPROPERTYTEMPLATE('3D$Dxx4d1DA9yKjE_rk3xa',$,'IsIlluminated','An indication of whether there is an illuminated indicator to show that the switch is on (=TRUE) or not (= FALSE).',.P_SINGLEVALUE.,'IfcBoolean','',$,$,$,$,.READWRITE.);
#711= IFCLIBRARYREFERENCE($,$,'\X2\81EA7167578B\X0\','\X2\30A430EB30DF30CD30FC30B730E730F3578BFF0881EA7167578BFF098868793A6A5F306730B930A430C330C1306E30AA30F3FF08\X0\TRUE\X2\FF09308430AA30D5FF08\X0\FALSE\X2\FF093092793A30593002\X0\','ja-JP',#2);
#712= IFCRELASSOCIATESLIBRARY('3WzFyXtDXDbAOgZn0KHxbq',$,$,$,(#710),#711);
#713= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\C870BA85D45CC2DCAE30\X0\','\X2\C77CB8E8BBF8\X0\ \X2\B124C774C158\X0\ \X2\D615\X0\ (\X2\C790C870\X0\ \X2\D615\X0\) \X2\D45CC2DCAE30\X0\ \X2\C2A4C704CE58B97C\X0\ \X2\CF1CAC70B098\X0\ (TRUE) \X2\B610B294\X0\ \X2\C624D504\X0\ (FALSE)\X2\B97C\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#714= IFCRELASSOCIATESLIBRARY('1TUxVZyrPAkwOEiVUmWUIp',$,$,$,(#710),#713);
#715= IFCSIMPLEPROPERTYTEMPLATE('2sD1CepaP2$Qptn_A6yfu9',$,'Legend','A text inscribed or applied to the switch as a legend to indicate purpose or function.',.P_SINGLEVALUE.,'IfcLabel','',$,$,$,$,.READWRITE.);
#716= IFCLIBRARYREFERENCE($,$,'\X2\51E14F8B\X0\','\X2\76EE7684307E305F306F6A5F80FD3092793A305951E14F8B306A3069300130B930A430C330C1306B906975283055308C308B30C630AD30B930C83002\X0\','ja-JP',#2);
#717= IFCRELASSOCIATESLIBRARY('3KBTv0OlfClP2bT4aZisHb',$,$,$,(#715),#716);
#718= IFCLIBRARYREFERENCE($,$,'\X2\BC94B840\X0\','\X2\BAA9C801C774B098\X0\ \X2\AE30B2A5C744\X0\ \X2\B098D0C0B0B4B294\X0\ \X2\BC94B840C640\X0\ \X2\AC19C740\X0\ \X2\C2A4C704CE58C5D0\X0\ \X2\C801C6A9B418B294\X0\ \X2\D14DC2A4D2B8C785B2C8B2E4\X0\.','ko-KR',#2);
#719= IFCRELASSOCIATESLIBRARY('1ikghSa_PAUgtyO00Ehh_x',$,$,$,(#715),#718);
#720= IFCSIMPLEPROPERTYTEMPLATE('0Ht5Fd_t54Bhh7no0L4JNq',$,'SetPoint','Indicates the setpoint and label.  For toggle switches, there are two positions, 0 for off and 1 for on.  For dimmer switches, the values may indicate the fully-off and full-on positions, where missing integer values in between are interpolated.   For selector switches, the range indicates the available positions.  \X\0AAn IfcTable may be attached (using IfcMetric and IfcPropertyConstraintRelationship) containing columns of the specified header names and types:\X\0A''Position'' (IfcInteger): The discrete setpoint level.\X\0A''Sink'' (IfcLabel): The Name of the switched input port (IfcDistributionPort with FlowDirection=SINK).\X\0A''Source'' (IfcLabel): The Name of the switched output port (IfcDistributionPort with FlowDirection=SOURCE).\X\0A''Ratio'' (IfcNormalizedRatioMeasure): The ratio of power at the setpoint where 0.0 is off and 1.0 is fully on.',.P_TABLEVALUE.,'IfcInteger','IfcLabel',$,$,$,$,.READWRITE.);
#721= IFCLIBRARYREFERENCE($,$,'\X2\8A2D5B9A30DD30A430F330C8\X0\','\X2\8A2D5B9A30DD30A430F330C830687BC456F23092793A3059300230C830B030EB30B930A430C330C1306F\X0\2\X2\3064306E30DD30B830B730E730F3304C3042308BFF1A\X0\0 \X2\306F\X0\ \X2\30AA30D5\X0\(OFF)\X2\3001\X0\1 \X2\306F\X0\ \X2\30AA30F3\X0\(ON)\X2\300230C730A330DE30FC30B930A430C330C1306F300151689589\X0\(fully-off) \X2\307E305F306F30005168958B\X0\(fully-on) \X2\306E4ED6306B3001305D306E9593306753D65F9753EF80FD306A5024309230AA30D730B730E730F33067793A305930029078629E578B30B930A430C330C1306F9078629E53EF80FD306A30DD30B830B730E730F3306E7BC456F23092793A30593002\X0\','ja-JP',#2);
#722= IFCRELASSOCIATESLIBRARY('3AdZnnU2z1WALNinH_0E35',$,$,$,(#720),#721);
#723= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\D3ECD2B8\X0\ \X2\C2F1D06C\X0\','\X2\C785B825\X0\ \X2\D3ECD2B8\X0\ \X2\C774B984\X0\ (IfcDistributionPort \X2\BC0F\X0\ FlowDirection = SINK), Maps SetPoint \X2\C704CE58\X0\. \X2\D68CB85CAC00\X0\ \X2\C5B4B5A4\X0\ \X2\ACBDB85CB97C\X0\ \X2\CD94C801D560C9C0B97C\X0\ \X2\B098D0C0B0B8B2E4\X0\.','ko-KR',#2);
#724= IFCRELASSOCIATESLIBRARY('0cHh_jpwXChw4PvgVjMkdj',$,$,$,(#720),#723);
#725= IFCPROPERTYSETTEMPLATE('1s84UbSH5B4AziPPtf7h$V',$,'Pset_SwitchingDeviceTypeContactor','An electrical device used to control the flow of power in a circuit on or off.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/CONTACTOR',(#728));
#726= IFCLIBRARYREFERENCE($,$,$,'\X2\96FB529B6A5F5668306E8D7752D530FB505C6B62306E305F3081306B300196FB529B56DE8DEF3092958B95893059308B96FB529B6A5F56683002\X0\','ja-JP',#2);
#727= IFCRELASSOCIATESLIBRARY('3Fz_31Fvj6Owhk56Ho2Qfe',$,$,$,(#725),#726);
#728= IFCSIMPLEPROPERTYTEMPLATE('3zo8024FfBQfpoyCwaQz0A',$,'ContactorType','A list of the available types of contactor from which that required may be selected where:\X\0A\X\0ACapacitorSwitching: for switching 3 phase single or multi-step capacitor banks.\X\0ALowCurrent: requires the use of low resistance contacts.\X\0AMagneticLatching: enables the contactor to remain in the on position when the coil is no longer energized.\X\0AMechanicalLatching: requires that the contactor is mechanically retained in the on position.\X\0AModular: are totally enclosed and self contained.\X\0AReversing: has a double set of contactors that are prewired.\X\0AStandard: is a generic device that controls the flow of power in a circuit on or off.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#729,$,$,$,.READWRITE.);
#729= IFCPROPERTYENUMERATION('PEnum_ContactorType',(IFCLABEL('CAPACITORSWITCHING'),IFCLABEL('LOWCURRENT'),IFCLABEL('MAGNETICLATCHING'),IFCLABEL('MECHANICALLATCHING'),IFCLABEL('MODULAR'),IFCLABEL('REVERSING'),IFCLABEL('STANDARD'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#730= IFCLIBRARYREFERENCE($,$,'\X2\63A589E6566830BF30A430D7\X0\','\X2\4EE54E0B3088308A9078629E304C5FC589813068306A308B300163A589E65668306E4E0089A730EA30B930C8FF1A\X0\\X\0A\X\0A\X2\30B330F330C730F330B530B930A430C330C1FF1A\X0\3\X2\3064306E30B730F330B030EB30D530A730FC30BA307E305F306F89076570306E30B330F330C730F330B530D030F330AF30675207308A66FF3048308B3002\X0\\X\0A\X2\4F4E6D41FF1A4F4E304462B5629763A589E6306E4F7F7528304C5FC58981\X0\\X\0A\X2\30DE30B030CD30C330C85F0FFF1A30B330A430EB306E30A830CD30EB30AE30FC304C7121304F306A3063305F6642306B520766FF3092\X0\ON\X2\30DD30B830B730E730F3306B30573066670952B9306B3059308B\X0\\X\0AMechanicalLatching\X2\FF1A520766FF5668304C\X0\ON\X2\30DD30B830B730E730F330927DAD63013059308B305F3081306B6A5F68B07684306A4ED57D44307F304C5FC589813002\X0\\X\0A\X2\30E230B830E530FC30EB5F0FFF1A958993963055308C30663044308B81EA50CD578B520766FF56683002\X0\\X\0A\X2\30EA30D030FC30B9FF1A\X0\2\X2\3064306E520766FF5668309230EF30A430E430FC306763A57D9A3057305F3082306E3002\X0\\X\0A\X2\6A196E96FF1A56DE8DEF306796FB529B6F6E6D41309230AA30F3307E305F306F30AA30D5306730B330F330C830ED30FC30EB3059308B4E00822C7684306A88C57F6E3002\X0\','ja-JP',#2);
#731= IFCRELASSOCIATESLIBRARY('0Sb6JPVDf5VRSK6VYxxZSr',$,$,$,(#728),#730);
#732= IFCLIBRARYREFERENCE($,$,'\X2\C811CD09AE30\X0\ \X2\C720D615\X0\','\X2\B2E4C74CC5D0C11C\X0\ \X2\C120D0DDC774\X0\ \X2\D544C694D558B2E4\X0\, \X2\C811CD09AE30\X0\  \X2\BAA9B85D\X0\ : \X2\CF58B374C11C\X0\ \X2\C2A4C704CE58\X0\ : 3 \X2\AC1CC758\X0\ \X2\B2E8C77C\X0\ \X2\C704C0C1\X0\ \X2\C774C0C1C758\X0\ \X2\CEE4D328C2DCD130\X0\ \X2\BC45D06CB97C\X0\ \X2\C804D658D569B2C8B2E4\X0\. \X2\B0AEC740C5EC\X0\ : \X2\B0AEC740\X0\ \X2\C800D56D\X0\ \X2\C811CD09\X0\ \X2\C0ACC6A9D574C57C\X0\ \X2\B9C8ADF8B124D2F1\X0\ : \X2\CF54C77CC758\X0\ \X2\C5D0B108C9C0AC00\X0\ \X2\BD84C2E4B41C\X0\ \X2\B54C\X0\ \X2\C804D658C744\X0\ ON \X2\C704CE58B85CD558C5EC\X0\ \X2\C0ACC6A9\X0\ MechanicalLatching : \X2\D310C744\X0\ ON \X2\C704CE58B97C\X0\ \X2\C720C9C0D558AE30\X0\ \X2\C704D574\X0\ \X2\AE30ACC4C801C778\X0\ \X2\AD6CC870AC00\X0\ \X2\D544C694D569B2C8B2E4\X0\. \X2\BAA8B4C8D615\X0\ : \X2\D3D0C1C4B418C5B4C788B294\X0\ \X2\C790C2E0\X0\ \X2\B3D9D615\X0\ \X2\D310\X0\. \X2\B9ACBC84C2A4\X0\ : \X2\B450\X0\ \X2\D310C744\X0\ \X2\C640C774C5B4B85C\X0\ \X2\C5F0ACB0D55C\X0\ \X2\AC83\X0\. \X2\D45CC900\X0\ : \X2\D68CB85CC5D0C11C\X0\ \X2\C804B825\X0\ \X2\C870B958B97C\X0\ \X2\CF1CC9C0AC70B098\X0\ \X2\AEBCC9C0C9C0\X0\ \X2\CEE8D2B8B864D558B294\X0\ \X2\C77CBC18C801C778\X0\ \X2\C7A5CE58\X0\','ko-KR',#2);
#733= IFCRELASSOCIATESLIBRARY('2Ogxhra9v7r9IC8I_BZlaq',$,$,$,(#728),#732);
#734= IFCPROPERTYSETTEMPLATE('0nR8G4lwzCKhDmWuSlQbEd',$,'Pset_SwitchingDeviceTypeDimmerSwitch','A dimmer switch is a switch that adjusts electrical power through a variable position level action.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/DIMMERSWITCH',(#737));
#735= IFCLIBRARYREFERENCE($,$,$,'\X2\540430EC30D930EB306E52D54F5C306796FB529B30928ABF65743059308B30C730A330DE30FC30B930A430C330C13002\X0\\X\0A\X2\5C656B74FF1A\X0\IFC2\X2\FF58FF1430788FFD52A03002\X0\','ja-JP',#2);
#736= IFCRELASSOCIATESLIBRARY('1L0fsRRen8pOxAkstVAw2T',$,$,$,(#734),#735);
#737= IFCSIMPLEPROPERTYTEMPLATE('2lBCoEiWb0hhoPpWhy_u6g',$,'DimmerType','A list of the available types of dimmer switch from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#738,$,$,$,.READWRITE.);
#738= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceDimmerSwitchType',(IFCLABEL('ROCKER'),IFCLABEL('SELECTOR'),IFCLABEL('TWIST'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#739= IFCLIBRARYREFERENCE($,$,'\X2\30C730A330DE30FC30BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B300130C730A330DE30FC30B930A430C330C1306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#740= IFCRELASSOCIATESLIBRARY('10wMn1w599au_BExwOqMG1',$,$,$,(#737),#739);
#741= IFCLIBRARYREFERENCE($,$,'\X2\C870AD11AE30\X0\ \X2\C720D615\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\C870AD11AE30\X0\ \X2\C2A4C704CE58\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#742= IFCRELASSOCIATESLIBRARY('1QgSlOOgD0huCyfi4jDiH7',$,$,$,(#737),#741);
#743= IFCPROPERTYSETTEMPLATE('2uSmr8l9938uBS4xYjMoLD',$,'Pset_SwitchingDeviceTypeEmergencyStop','An emergency stop device acts to remove as quickly as possible any danger that may have arisen unexpectedly.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/EMERGENCYSTOP',(#746));
#744= IFCLIBRARYREFERENCE($,$,$,'IEC 826-08-03\X2\306E5B9A7FA9\X0\: \X\0A\X2\7DCA6025505C6B6230B930A430C330C1306F4E88671F305B305A305730668D773053308B3055307E3056307E306A5371967A309253EF80FD306A9650308A8FC5901F306B53D6308A9664304F30883046306B52D54F5C3059308B88C57F6E30673042308B3002\X0\','ja-JP',#2);
#745= IFCRELASSOCIATESLIBRARY('1c1ROq_1rEy8e9b6Usr52_',$,$,$,(#743),#744);
#746= IFCSIMPLEPROPERTYTEMPLATE('0Qy48h4Gf58PbM20tYzuFS',$,'SwitchOperation','Indicates operation of emergency stop switch.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#747,$,$,$,.READWRITE.);
#747= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceEmergencyStopType',(IFCLABEL('MUSHROOM'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#748= IFCLIBRARYREFERENCE($,$,'\X2\30B930A430C330C164CD4F5C\X0\','\X2\7DCA6025505C6B6230B930A430C330C1306E64CD4F5C3092793A30593002\X0\','ja-JP',#2);
#749= IFCRELASSOCIATESLIBRARY('1K_ENN9mn5KhEeiX3FYJEy',$,$,$,(#746),#748);
#750= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\C870C791\X0\','\X2\BE44C0C1\X0\ \X2\C815C9C0\X0\ \X2\C2A4C704CE58C758\X0\ \X2\C870C791C744\X0\ \X2\BCF4C5ECC900B2E4\X0\.','ko-KR',#2);
#751= IFCRELASSOCIATESLIBRARY('0WKsMz$KH1I9fzRwe5OqGp',$,$,$,(#746),#750);
#752= IFCPROPERTYSETTEMPLATE('3wbT7luQX9x8tZlnQCAdA$',$,'Pset_SwitchingDeviceTypeKeypad','A keypad is a switch supporting multiple functions.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/KEYPAD',(#755));
#753= IFCLIBRARYREFERENCE($,$,$,'\X2\30AD30FC30D130C330C9306F89076570306E6A5F80FD309230B530DD30FC30C83059308B30B930A430C330C13002\X0\\X\0A\X2\5C656B74FF1A\X0\ IFC4\X2\306B8FFD52A03002\X0\','ja-JP',#2);
#754= IFCRELASSOCIATESLIBRARY('00zz81JafAguQcgRQOsrB3',$,$,$,(#752),#753);
#755= IFCSIMPLEPROPERTYTEMPLATE('1Tx8X0Yoz62e1gA9$ZyaAJ',$,'KeypadType','A list of the available types of keypad switch from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#756,$,$,$,.READWRITE.);
#756= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceKeypadType',(IFCLABEL('BUTTONS'),IFCLABEL('TOUCHSCREEN'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#757= IFCLIBRARYREFERENCE($,$,'\X2\30AD30FC30D130C330C930BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B300130AD30FC30D130C330C930B930A430C330C1306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#758= IFCRELASSOCIATESLIBRARY('1XepHq8H91me26$_RHtOEh',$,$,$,(#755),#757);
#759= IFCLIBRARYREFERENCE($,$,'\X2\D0A4D328B4DC\X0\ \X2\C720D615\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\D0A4D328B4DC\X0\ \X2\C2A4C704CE58\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#760= IFCRELASSOCIATESLIBRARY('2_zrdYdgbABeRb_m9rOdfc',$,$,$,(#755),#759);
#761= IFCPROPERTYSETTEMPLATE('2RpkqK74f9IRrr4zaOMGH8',$,'Pset_SwitchingDeviceTypeMomentarySwitch','A momentary switch is a switch that does not hold state.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/MOMENTARYSWITCH',(#764));
#762= IFCLIBRARYREFERENCE($,$,$,'\X2\77AC664230B930A430C330C1FF0830E230FC30E130F330BF30EA30B930A430C330C1FF09306F72B6614B30924FDD63013057306A304430BF30A430D7306E30B930A430C330C13002\X0\\X\0A\X2\5C656B74FF1A\X0\ IFC4\X2\306B8FFD52A03002\X0\','ja-JP',#2);
#763= IFCRELASSOCIATESLIBRARY('2Yto40IJLDgvGCaHYVzRVt',$,$,$,(#761),#762);
#764= IFCSIMPLEPROPERTYTEMPLATE('16wHv2DG52GAn246Eg5YE0',$,'MomentaryType','A list of the available types of momentary switch from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#765,$,$,$,.READWRITE.);
#765= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceMomentarySwitchType',(IFCLABEL('BUTTON'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#766= IFCLIBRARYREFERENCE($,$,'\X2\77AC664230B930A430C330C130BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B300181EA52D55FA95E3030B930A430C330C1306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#767= IFCRELASSOCIATESLIBRARY('1ZBaN9bGP1swHE4jTHdFot',$,$,$,(#764),#766);
#768= IFCLIBRARYREFERENCE($,$,'\X2\C21CAC04C2A4C704CE58\X0\ \X2\C720D615\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\C790B3D9\X0\ \X2\BCF5ADC0\X0\ \X2\C2A4C704CE58\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#769= IFCRELASSOCIATESLIBRARY('19mpK_gpvBY8AlJx0GHHo8',$,$,$,(#764),#768);
#770= IFCPROPERTYSETTEMPLATE('2p2uRJQH97U8ap$hLsjZSr',$,'Pset_SwitchingDeviceTypePHistory','Indicates switch positions or levels over time, such as for energy management or surveillance.',.PSET_PERFORMANCEDRIVEN.,'IfcSwitchingDevice',(#771));
#771= IFCSIMPLEPROPERTYTEMPLATE('1m9cqnaob0BelXGkuR$jdB',$,'SetPoint','Indicates the switch position over time according to Pset_SwitchingDeviceTypeCommon.SetPoint.',.P_REFERENCEVALUE.,'IfcTimeSeries','IfcInteger',$,$,$,$,.READWRITE.);
#772= IFCPROPERTYSETTEMPLATE('2s_wRdy3f2OBHaRABsnvr6',$,'Pset_SwitchingDeviceTypeSelectorSwitch','A selector switch is a switch that adjusts electrical power through a multi-position action.  HISTORY: Added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/SELECTORSWITCH',(#775,#781,#787));
#773= IFCLIBRARYREFERENCE($,$,$,'\X2\520766FF304830B930A430C330C1306F89076570306E30DD30B830B730E730F3306B5408308F305B308B30533068306796FB529B30928ABF65743059308B30B930A430C330C130673042308B3002\X0\\X\0A\X2\5C656B74FF1A\X0\ IFC4\X2\306B8FFD52A03002\X0\','ja-JP',#2);
#774= IFCRELASSOCIATESLIBRARY('13lBRLkzn4Px8cECbmAudq',$,$,$,(#772),#773);
#775= IFCSIMPLEPROPERTYTEMPLATE('1NQf0w5mT7tx4INQw80wDj',$,'SelectorType','A list of the available types of selector switch from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#776,$,$,$,.READWRITE.);
#776= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceDimmerSwitchType',(IFCLABEL('BUTTONS'),IFCLABEL('SLIDE'),IFCLABEL('TWIST'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#777= IFCLIBRARYREFERENCE($,$,'\X2\30BB30EC30AF30BF30FCFF0830B930A430C330C1FF0930BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B3001520766FF304830B930A430C330C1306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#778= IFCRELASSOCIATESLIBRARY('3Kc3xI0on4fx4KY3THqOIl',$,$,$,(#775),#777);
#779= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\D0C0C785\X0\','\X2\C804D658C2A4C704CE58\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#780= IFCRELASSOCIATESLIBRARY('3zrAa$Mz55POXUYi03P1wY',$,$,$,(#775),#779);
#781= IFCSIMPLEPROPERTYTEMPLATE('3DFG$hXDXFtB1BMg_0OJop',$,'SwitchUsage','A list of the available usages for selector switches from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#782,$,$,$,.READWRITE.);
#782= IFCPROPERTYENUMERATION('PEnum_SwitchUsage',(IFCLABEL('EMERGENCY'),IFCLABEL('GUARD'),IFCLABEL('LIMIT'),IFCLABEL('START'),IFCLABEL('STOP'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#783= IFCLIBRARYREFERENCE($,$,'\X2\30B930A430C330C1306E4F7F75286CD5\X0\','\X2\9078629E304C5FC589813068306A308B3001520766FF304830B930A430C330C1306E4F7F75286CD5306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#784= IFCRELASSOCIATESLIBRARY('1X$YAuOVDDKANIA9r4xiIv',$,$,$,(#781),#783);
#785= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\C0ACC6A9\X0\','\X2\C804D658C2A4C704CE58\X0\ \X2\C0ACC6A9\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#786= IFCRELASSOCIATESLIBRARY('3GPSOloIH2MOTI86BRT9w4',$,$,$,(#781),#785);
#787= IFCSIMPLEPROPERTYTEMPLATE('3ZJaRVLir2seoOuRaaF0qN',$,'SwitchActivation','A list of the available activations for selector switches from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#788,$,$,$,.READWRITE.);
#788= IFCPROPERTYENUMERATION('PEnum_SwitchActivation',(IFCLABEL('ACTUATOR'),IFCLABEL('FOOT'),IFCLABEL('HAND'),IFCLABEL('PROXIMITY'),IFCLABEL('SOUND'),IFCLABEL('TWOHAND'),IFCLABEL('WIRE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#789= IFCLIBRARYREFERENCE($,$,'\X2\8D7752D565B95F0F\X0\','\X2\9078629E304C5FC589813068306A308B3001520766FF304830B930A430C330C1306E8D7752D565B95F0F306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#790= IFCRELASSOCIATESLIBRARY('2ZnSdKglX3HxNKVxgy2kYZ',$,$,$,(#787),#789);
#791= IFCLIBRARYREFERENCE($,$,'\X2\AE30B3D9\X0\ \X2\BC29C2DD\X0\','\X2\C2A4C704CE58\X0\ \X2\BD80D305BC29C2DDC758\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#792= IFCRELASSOCIATESLIBRARY('1bs36p_vPAte2CtLAMaQyP',$,$,$,(#787),#791);
#793= IFCPROPERTYSETTEMPLATE('1SsZHek9L4zBGun3dtm1EP',$,'Pset_SwitchingDeviceTypeStarter','A starter is a switch which in the closed position controls the application of power to an electrical device.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/STARTER',(#796));
#794= IFCLIBRARYREFERENCE($,$,$,'\X2\30B930BF30FC30BF30FC30B930A430C330C1306F95893058305F72B6614B306E4F4D7F6E304B3089300196FB6C1788C57F6E306B5BFE305796FB529B306E52297528309252365FA13059308B88C57F6E3002\X0\','ja-JP',#2);
#795= IFCRELASSOCIATESLIBRARY('3k6JsxaQPB2AzY3U_SBcBH',$,$,$,(#793),#794);
#796= IFCSIMPLEPROPERTYTEMPLATE('05sPG$BnD9s8IlP_zeoC9H',$,'StarterType','A list of the available types of starter from which that required may be selected where:\X\0A\X\0AAutoTransformer: A starter for an induction motor which uses for starting one or more reduced voltages derived from an auto transformer. (IEC 441-14-45)\X\0AManual: A starter in which the force for closing the main contacts is provided exclusively by manual energy. (IEC 441-14-39)\X\0ADirectOnLine: A starter which connects the line voltage across the motor terminals in one step. (IEC 441-14-40)\X\0AFrequency: A starter in which the frequency of the power supply is progressively increased until the normal operation frequency is attained.\X\0AnStep: A starter in which there are (n-1) intermediate accelerating positions between the off and full on positions. (IEC 441-14-41)\X\0ARheostatic: A starter using one or several resistors for obtaining, during starting, stated motor torque characteristics and for limiting the current. (IEC 441-14-425)\X\0AStarDelta: A starter for a 3 phase induction motor such that in the starting position the stator windings are connected in star and in the final running position they are connected in delta. (IEC 441-14-44)',.P_ENUMERATEDVALUE.,'IfcLabel',$,#797,$,$,$,.READWRITE.);
#797= IFCPROPERTYENUMERATION('PEnum_StarterType',(IFCLABEL('AUTOTRANSFORMER'),IFCLABEL('MANUAL'),IFCLABEL('DIRECTONLINE'),IFCLABEL('FREQUENCY'),IFCLABEL('NSTEP'),IFCLABEL('RHEOSTATIC'),IFCLABEL('STARDELTA'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#798= IFCLIBRARYREFERENCE($,$,'\X2\59CB52D530BF30A430D7\X0\','\X2\4EE54E0B3088308A9078629E304C5FC589813068306A308B300159CB52D5306E4E0089A730EA30B930C8FF1A\X0\\X\0A\X\0A\X2\81EA52D5FF1A\X0\ \X2\81EA52D530C830E930F330B9304B30895F15304D51FA3055308C305FFF1130644EE54E0A306E4F4E4E0B3057305F96FB5727306730B930BF30FC30C83059308B305F3081306B4F7F75283059308B8A985C0E96FB52D56A5F7528306E30B930BF30FC30BF30FC\X0\ (IEC 441-14-45)\X\0A\X2\624B52D5FF1A\X0\ \X2\30E130A430F3306E30B330F330BF30AF30C8304B30895F3752367684306B520696E23055308C305F30683053308D306B3042308A3001624B52D5306B3088308A30A830CD30EB30AE30FC304C4F9B7D663055308C308B\X0\ (IEC 441-14-39)\X\0A\X2\3058304B5165308C\X0\: \X2\30EF30F330B930C630C330D7306730E230FC30BF30FC30FB30BF30FC30DF30CA30EB9593306E7DDA959396FB572730923064306A305030B930BF30FC30BF30FC\X0\ (IEC 441-14-40)\X\0A\X2\632F52D5FF1A96FB6E90306E632F52D56570304C901A5E38306E64CD4F5C632F52D5307E30676B217B2C306B5897592730573066884C304F30B930BF30FC30BF30FC\X0\\X\0AnStep: \X2\30AA30D5FF08\X0\OFF)\X2\306830AA30F3FF08\X0\ON\X2\FF09306E959330673001FF08\X0\n-1\X2\FF09306E4E2D9593306E52A0901F5EA67684306A4F4D7F6E30673042308B30B930BF30FC30BF30FC3002\X0\ (IEC 441-14-41)\X\0A\X2\62B56297FF1A30E230FC30BF306E30C830EB30AF72796027306E53D65F973001958B59CB3001305D305730665B895B9A3059308B9593306B300196FB6D413092523696503059308B305F3081306B\X0\ 1 \X2\3064307E305F306F3044304F3064304B306E62B562973092522975283057305F30B930BF30FC30BF30FC\X0\ (IEC 441-14-425) \X\0A\X2\30B930BF30FC30C730EB30BFFF1A958B59CB4F4D7F6E3067306F56FA5B9A5C0F5DFB7DDAFF0830B930BF30FC30BF30FC30EF30A430F330C730A330F330B0FF09304C661F72B6306763A57D9A3055308C3001305D306E5F8C300167007D42306E5B9F884C72B6614B3067306F30C730EB30BF72B6306B63A57D9A3055308C308B306830443046\X0\3\X2\76F88A985C0E30E230FC30BF30FC7528306E30B930BF30FC30BF30FC3002FF08\X0\IEC 441-14-44\X2\FF09\X0\','ja-JP',#2);
#799= IFCRELASSOCIATESLIBRARY('370b4VJRHCu9h4dHL74Uh4',$,$,$,(#796),#798);
#800= IFCLIBRARYREFERENCE($,$,'\X2\C2DCC791\X0\ \X2\C720D615\X0\','\X2\C544B798C5D0C11C\X0\ \X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\C2DCB3D9\X0\ \X2\BAA9B85D\X0\ \X2\BAA9B85D\X0\ : \X2\C790B3D9\X0\ : \X2\C790B3D9\X0\ \X2\D2B8B79CC2A4C5D0C11C\X0\ \X2\AC00C838C628\X0\ \X2\D558B098\X0\ \X2\C774C0C1C758\X0\ \X2\C800D558\X0\ \X2\C804C555C73CB85C\X0\ \X2\C2DCC791D558B294\X0\ \X2\B370\X0\ \X2\C0ACC6A9D558B294\X0\ \X2\C720B3C4\X0\ \X2\C804B3D9AE30C758\X0\ \X2\C2A4D0C0D130\X0\ (IEC 441-14-45) \X2\C218B3D9\X0\ : \X2\AE30BCF8\X0\ \X2\C5F0B77DCC98C5D0C11C\X0\ \X2\AC15C81CB85C\X0\ \X2\ACA9B9ACB41C\X0\ \X2\AC70B9ACC5D0\X0\ \X2\C788C73CBA70\X0\, \X2\C218B3D9C73CB85C\X0\ \X2\C5D0B108C9C0AC00\X0\ \X2\ACF5AE09B418B294\X0\ (IEC 441-14-39) \X2\AE00C790\X0\ \X2\D558B098\X0\ \X2\C785B825\X0\ : \X2\D55C\X0\ \X2\BC88C5D0\X0\ \X2\BAA8D130\X0\ \X2\D130BBF8B110\X0\ \X2\C0ACC774C758\X0\ \X2\C120AC04\X0\ \X2\C804C555C744\X0\ \X2\C5F0ACB0\X0\ \X2\C2A4D0C0D130\X0\ (IEC 441-14-40) \X2\C9C4B3D9\X0\ : \X2\C804C6D0C758\X0\ \X2\C9C4B3D9C218AC00\X0\ \X2\C815C0C1\X0\ \X2\C791B3D9\X0\ \X2\C9C4B3D9AE4CC9C0\X0\ \X2\C810CC28\X0\ \X2\C99DB300\X0\ \X2\D574AC00B294\X0\ \X2\C2A4D0C0D130\X0\ nStep : \X2\AEBCC9D0\X0\ (OFF)\X2\ACFC\X0\ \X2\CF1CC9D0\X0\ (ON) \X2\C0ACC774C5D0C11C\X0\ (n-1) \X2\C0ACC774C758\X0\ \X2\AC00C18DB3C4C801C778\X0\ \X2\C704CE58C774B2E4\X0\ \X2\C2A4D0C0D130\X0\. (IEC 441-14-41) \X2\C800D56D\X0\ : \X2\BAA8D130C758\X0\ \X2\D1A0D06C\X0\ \X2\D2B9C131\X0\ \X2\AC00C838C624AE30\X0\ \X2\C2DCC791\X0\, \X2\ADF8B9ACACE0\X0\ \X2\C548C815\X0\ \X2\C0ACC774C5D0\X0\ \X2\C804B958B97C\X0\ \X2\C81CD55CD558AE30\X0\ \X2\C704D574\X0\ \X2\D558B098\X0\ \X2\B610B294\X0\ \X2\BA87\X0\ \X2\AC00C9C0\X0\ \X2\C800D56DC744\X0\ \X2\C774C6A9D55C\X0\ \X2\C2A4D0C0D130\X0\ (IEC 441-14-425) \X2\C2A4D0C0\X0\ \X2\B378D0C0\X0\ : \X2\C2DCC791\X0\ \X2\C704CE58B294\X0\ \X2\ACE0C815\X0\ \X2\5C0F5DFB\X0\ \X2\C120\X0\ (\X2\CD08BCF4\X0\ \X2\C640C778\X0\)\X2\C774\X0\ \X2\C18CD589C131C5D0\X0\ \X2\C5F0ACB0B41C\X0\ \X2\D6C4\X0\, \X2\CD5CC885\X0\ \X2\C0C1D0DCC5D0C11CB294\X0\ \X2\B378D0C0\X0\ \X2\BAA8C591C73CB85C\X0\ \X2\C5F0ACB0B41CB2E4\X0\ 3 \X2\C0C1\X0\ \X2\C720B3C4\X0\ \X2\BAA8D130C758\X0\ \X2\C2A4D0C0D130\X0\. (IEC 441-14-44)','ko-KR',#2);
#801= IFCRELASSOCIATESLIBRARY('1CEZaYbnb2ZRu4vxIxVsoq',$,$,$,(#796),#800);
#802= IFCPROPERTYSETTEMPLATE('3QgLIEbEr46eQHCHrruGlO',$,'Pset_SwitchingDeviceTypeSwitchDisconnector','A switch disconnector is a switch which in the open position satisfies the isolating requirements specified for a disconnector.\X\0A\X\0AHistory: Property ''HasVisualIndication'' changed to ''IsIlluminated'' to conform with property name for toggle switch',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/SWITCHDISCONNECTOR',(#805,#811));
#803= IFCLIBRARYREFERENCE($,$,$,'IEC 441-14-12\X2\306E5B9A7FA9FF1A\X0\\X\0A\X2\9AD85727958B95895668306F958B95895668306E305F3081306B5B647ACB3057305F72B6614B30673042308B5FC5898167614EF630926E80305F30593001958B3044305F4F4D7F6E306B3042308B30B930A430C330C13002\X0\\X\0A\X\0A\X2\5C656B74FF1A\X0\\X\0A\X2\5C5E6027\X0\ ''HasVisualIndication'' \X2\3092\X0\ \X2\30C830B030EB30B930A430C330C1306E30D730ED30D130C630A3540D306B5BFE5FDC3059308B308830463001\X0\''IsIlluminated'' \X2\3078590966F43002\X0\','ja-JP',#2);
#804= IFCRELASSOCIATESLIBRARY('18cOvpnnD3ugIsq5Kuny9c',$,$,$,(#802),#803);
#805= IFCSIMPLEPROPERTYTEMPLATE('00davUmHH93vzHXVLlRozQ',$,'SwitchDisconnectorType','A list of the available types of switch disconnector from which that required may be selected where:\X\0A\X\0ACenterBreak: A disconnector in which both contacts of each pole are movable and engage at a point substantially midway between their supports. (IEC 441-14-08)\X\0ADividedSupport: A disconnector in which the fixed and moving contacts of each pole are not supported by a common base or frame. (IEC 441-14-06)\X\0ADoubleBreak: A disconnector that opens a circuit at two points. (IEC 441-14-09)\X\0AEarthingSwitch: A disconnector in which the fixed and moving contacts of each pole are not supported by a common base or frame. (IEC 441-14-07)\X\0AIsolator: A disconnector which in the open position satisfies isolating requirements. (IEC 441-14-12)',.P_ENUMERATEDVALUE.,'IfcLabel',$,#806,$,$,$,.READWRITE.);
#806= IFCPROPERTYENUMERATION('PEnum_SwitchDisconnectorType',(IFCLABEL('CENTERBREAK'),IFCLABEL('DIVIDEDSUPPORT'),IFCLABEL('DOUBLEBREAK'),IFCLABEL('EARTHINGSWITCH'),IFCLABEL('ISOLATOR'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#807= IFCLIBRARYREFERENCE($,$,'\X2\9AD85727906E65AD6A5F30BF30A430D7\X0\','\X2\4EE54E0B3088308A9078629E304C5FC589813068306A308B300130B930A430C330C165AD8DEF6A5F306E4E0089A730EA30B930C8FF1A\X0\\X\0A\X\0A\X2\30BB30F330BF30FC30D630EC30A430AFFF1A\X0\ \X2\54046975306E4E2165B9306E63A570B9306F53EF52D55F0F306730015B9F8CEA7684306B4E2D95934ED88FD130924FDD63013059308B65AD8DEF56683002\X0\ (IEC 441-14-08)\X\0ADividedSupport\X2\FF1A\X0\ \X2\54046975306E56FA5B9A5074306879FB52D5507463A570B9304C30015171901A306E30D930FC30B9307E305F306F30D530EC30FC30E03067306F30B530DD30FC30C83055308C306A304465AD8DEF56683002\X0\(IEC 441-14-06)\X\0A\X2\4E8C70B95207308A65AD8DEF5668FF1A\X0\ 2\X2\70B9306756DE8DEF3092958B304F65AD8DEF5668\X0\ (IEC 441-14-09)\X\0A\X2\63A55730958B95895668\X0\ \X2\FF1A\X0\ \X2\54046975306E56FA5B9A5074306879FB52D5507463A570B9304C30015171901A306E30D930FC30B9307E305F306F30D530EC30FC30E03067306F30B530DD30FC30C83055308C306A304465AD8DEF56683002\X0\(IEC 441-14-07)\X\0A\X2\65AD8DEF5668FF1A\X0\ \X2\89E3653E4F4D7F6E306E520696E289814EF630926E80305F3059300165AD8DEF56683002\X0\(IEC 441-14-12)','ja-JP',#2);
#808= IFCRELASSOCIATESLIBRARY('1bD8kAtAr5UhNHptblhoXy',$,$,$,(#805),#807);
#809= IFCLIBRARYREFERENCE($,$,'\X2\ACE0C555CC28B2E8AE30\X0\ \X2\C720D615\X0\','\X2\C544B798C5D0C11C\X0\ \X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\C2A4C704CE58\X0\ \X2\B2E8B85C\X0\ \X2\AE30C758\X0\ \X2\BAA9B85D\X0\ \X2\BAA9B85D\X0\ : \X2\C13CD130\X0\ \X2\BE0CB808C774D06C\X0\ : \X2\AC01\X0\ \X2\AD6DC758\X0\ \X2\B450\X0\ \X2\C811C810C740\X0\ \X2\AC00B3D9\X0\ \X2\C2DDC5D0C11C\X0\ \X2\C2E4C9C8C801C73CB85C\X0\ \X2\C911AC04\X0\ \X2\BD80ADFCC744\X0\ \X2\C720C9C0\X0\ \X2\B2E8B85CAE30\X0\. (IEC 441-14-08) DividedSupport : \X2\AC01\X0\ \X2\AD6DC758\X0\ \X2\ACE0C815\X0\ \X2\CE21ACFC\X0\ \X2\200B200BC774B3D9\X0\ \X2\CE21C758\X0\ \X2\C811C810C774\X0\ \X2\ACF5D1B5\X0\ \X2\AE30BC18\X0\ \X2\B610B294\X0\ \X2\D504B808C784C774\X0\ \X2\C9C0C6D0B418C9C0\X0\ \X2\C54AB294\X0\ \X2\B2E8B85CAE30\X0\. (IEC 441-14-06) \X2\B450AC00C9C0\X0\ \X2\B044ACE0\X0\ \X2\B2E8B85CAE30\X0\ : 2 \X2\C810\X0\ \X2\D68CB85CB97C\X0\ \X2\C5F4\X0\ \X2\B2E8B85CAE30\X0\ (IEC 441-14-09) \X2\C811C9C0\X0\ \X2\AC1CD3D0AE30\X0\ : \X2\AC01\X0\ \X2\AD6DC758\X0\ \X2\ACE0C815\X0\ \X2\CE21ACFC\X0\ \X2\200B200BC774B3D9\X0\ \X2\CE21C758\X0\ \X2\C811C810C774\X0\ \X2\ACF5D1B5\X0\ \X2\AE30BC18\X0\ \X2\B610B294\X0\ \X2\D504B808C784C774\X0\ \X2\C9C0C6D0B418C9C0\X0\ \X2\C54AB294\X0\ \X2\B2E8B85CAE30\X0\. (IEC 441-14-07) \X2\B2E8B85CAE30\X0\ : \X2\D574C81C\X0\ \X2\C704CE58\X0\ \X2\ACA9B9AC\X0\ \X2\C694AD6C\X0\ \X2\C0ACD56DC744\X0\ \X2\CDA9C871\X0\ \X2\B2E8B85CAE30\X0\. (IEC 441-14-12)','ko-KR',#2);
#810= IFCRELASSOCIATESLIBRARY('1DEo$iSZv2dR4GkT0gyqzr',$,$,$,(#805),#809);
#811= IFCSIMPLEPROPERTYTEMPLATE('37cuk8q1XCmg7QLefuUmJr',$,'LoadDisconnectionType','A list of the available types of load disconnection from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#812,$,$,$,.READWRITE.);
#812= IFCPROPERTYENUMERATION('PEnum_LoadDisconnectionType',(IFCLABEL('OFFLOAD'),IFCLABEL('ONLOAD'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#813= IFCLIBRARYREFERENCE($,$,'\X2\520765AD30BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B30018CA08377958B9589566830BF30A430D7306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#814= IFCRELASSOCIATESLIBRARY('3K5DuSE_9BvflWORfXRlpn',$,$,$,(#811),#813);
#815= IFCPROPERTYSETTEMPLATE('0ASWtSMUr2g9$YAXHPG5JA',$,'Pset_SwitchingDeviceTypeToggleSwitch','A toggle switch is a switch that enables or isolates electrical power through a two position on/off action.  HISTORY: SetPoint added in IFC4.',.PSET_TYPEDRIVENOVERRIDE.,'IfcSwitchingDevice/TOGGLESWITCH',(#818,#824,#830));
#816= IFCLIBRARYREFERENCE($,$,$,'\X2\30C830B030EB30B930A430C330C13068306F\X0\ON\X2\3001\X0\OFF\X2\306EFF123064306E30DD30B830B730E730F3306E52D54F5C3067300196FB529B309263A57D9A3057305F308A906E65AD3057305F308A3059308B30B930A430C330C130673042308B3002\X0\ \X\0A\X2\5C656B74FF1A\X0\ IFC4 \X2\306B\X0\ SetPoint \X2\30928FFD52A03002\X0\','ja-JP',#2);
#817= IFCRELASSOCIATESLIBRARY('3vauiK1pX7BQ$5qbwhucCQ',$,$,$,(#815),#816);
#818= IFCSIMPLEPROPERTYTEMPLATE('1pWuX2V_L4uhwPYT4DAEl4',$,'ToggleSwitchType','A list of the available types of toggle switch from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#819,$,$,$,.READWRITE.);
#819= IFCPROPERTYENUMERATION('PEnum_SwitchingDeviceToggleSwitchType',(IFCLABEL('BREAKGLASS'),IFCLABEL('CHANGEOVER'),IFCLABEL('KEYOPERATED'),IFCLABEL('MANUALPULL'),IFCLABEL('PUSHBUTTON'),IFCLABEL('PULLCORD'),IFCLABEL('ROCKER'),IFCLABEL('SELECTOR'),IFCLABEL('TWIST'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#820= IFCLIBRARYREFERENCE($,$,'\X2\30EC30D030FC30B930A430C330C130BF30A430D7\X0\','\X2\9078629E304C5FC589813068306A308B300130C830B030EB30B930A430C330C1306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#821= IFCRELASSOCIATESLIBRARY('33naaj4tf3twd6wYinov2i',$,$,$,(#818),#820);
#822= IFCLIBRARYREFERENCE($,$,'\X2\B808BC84C2A4C704CE58\X0\ \X2\C720D615\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\D1A0AE00\X0\ \X2\C2A4C704CE58\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#823= IFCRELASSOCIATESLIBRARY('0GxkUwhPL9AfpLdcY8BUtx',$,$,$,(#818),#822);
#824= IFCSIMPLEPROPERTYTEMPLATE('0rj3IYP8b86vb$bBQN8jWb',$,'SwitchUsage','A list of the available usages for toggle switches from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#825,$,$,$,.READWRITE.);
#825= IFCPROPERTYENUMERATION('PEnum_SwitchUsage',(IFCLABEL('EMERGENCY'),IFCLABEL('GUARD'),IFCLABEL('LIMIT'),IFCLABEL('START'),IFCLABEL('STOP'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#826= IFCLIBRARYREFERENCE($,$,'\X2\30B930A430C330C1306E4F7F75286CD5\X0\','\X2\9078629E304C5FC589813068306A308B300130C830B030EB30B930A430C330C1306E4F7F75286CD5306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#827= IFCRELASSOCIATESLIBRARY('0M2Alfd1rEl8UKv1pmIwSB',$,$,$,(#824),#826);
#828= IFCLIBRARYREFERENCE($,$,'\X2\C2A4C704CE58\X0\ \X2\C0ACC6A9\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\D1A0AE00\X0\ \X2\C2A4C704CE58\X0\ \X2\C0ACC6A9BAA9B85D\X0\','ko-KR',#2);
#829= IFCRELASSOCIATESLIBRARY('0lmKxOpBH1R8XFjQjcoyYi',$,$,$,(#824),#828);
#830= IFCSIMPLEPROPERTYTEMPLATE('0m1rhLra57auzzdkR96o9F',$,'SwitchActivation','A list of the available activations for toggle switches from which that required may be selected.',.P_ENUMERATEDVALUE.,'IfcLabel',$,#831,$,$,$,.READWRITE.);
#831= IFCPROPERTYENUMERATION('PEnum_SwitchActivation',(IFCLABEL('ACTUATOR'),IFCLABEL('FOOT'),IFCLABEL('HAND'),IFCLABEL('PROXIMITY'),IFCLABEL('SOUND'),IFCLABEL('TWOHAND'),IFCLABEL('WIRE'),IFCLABEL('OTHER'),IFCLABEL('NOTKNOWN'),IFCLABEL('UNSET')),$);
#832= IFCLIBRARYREFERENCE($,$,'\X2\8D7752D565B95F0F\X0\','\X2\9078629E304C5FC589813068306A308B300130C830B030EB30B930A430C330C1306E8D7752D565B95F0F306E4E0089A730EA30B930C83002\X0\','ja-JP',#2);
#833= IFCRELASSOCIATESLIBRARY('0WE2C6KPP84f2rO57EUnml',$,$,$,(#830),#832);
#834= IFCLIBRARYREFERENCE($,$,'\X2\AE30B3D9\X0\ \X2\BC29C2DD\X0\','\X2\C120D0DDC774\X0\ \X2\D544C694D55C\X0\ \X2\D1A0AE00\X0\ \X2\C2A4C704CE58\X0\ \X2\BD80D305\X0\ \X2\BC29C2DDC758\X0\ \X2\BAA9B85D\X0\','ko-KR',#2);
#835= IFCRELASSOCIATESLIBRARY('0UbKGMgl15iPRXZpUkCi7a',$,$,$,(#830),#834);
ENDSEC;

END-ISO-10303-21;
