#### 7.1.4.41 Pset_SensorTypeTemperatureSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / TEMPERATURESENSOR

| A device that senses or detects temperature. HISTORY: TemperatureSensorSensorSetPoint changed to SetPointTemperature. Range, accuracy and time constant deleted.
| 温度を感知または検出するデバイス。

buildingSMART Data Dictionary

PSD-XML

- TemperatureSensorType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_TemperatureSensorType: HIGHLIMIT, LOWLIMIT, OUTSIDETEMPERATURE, OPERATINGTEMPERATURE, ROOMTEMPERATURE, OTHER, NOTKNOWN, UNSET

  | TemperatureSensorType: Enumeration that Identifies the types of temperature sensor that can be specified.
  | 温度センサータイプ: 明示された温度センサーのタイプを識別する一覧。
  | 온도 센서 타입: 명시된 온도 센서 유형을 식별하는 목록.

- SetPointTemperature
  P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

  | SetPointTemperature: The temperature value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
  | 温度設定値: 感知される温度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。
  | 온도 성정: 감지되는 온도. 세트 포인트 값을 넣으려면, IfcPropertyBoundedValue.SetPointValue를 사용하십시오.

Link to this page