#### 7.2.4.10 Pset_SwitchingDeviceTypeMomentarySwitch

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / MOMENTARYSWITCH

| A momentary switch is a switch that does not hold state. HISTORY: Added in IFC4.
| 瞬時スイッチ（モーメンタリスイッチ）は状態を保持しないタイプのスイッチ。 履歴： IFC4に追加。

buildingSMART Data Dictionary

PSD-XML

- MomentaryType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_SwitchingDeviceMomentarySwitchType: BUTTON, OTHER, NOTKNOWN, UNSET

  | MomentaryType: A list of the available types of momentary switch from which that required may be selected.
  | 瞬時スイッチタイプ: 選択が必要となる、自動復帰スイッチの一覧リスト。
  | 순간스위치 유형: 선택이 필요한 자동 복귀 스위치 목록

Link to this page