#### 7.2.4.6 Pset_SwitchingDeviceTypeContactor

PSET_TYPEDRIVENOVERRIDE / IfcSwitchingDevice / CONTACTOR

| An electrical device used to control the flow of power in a circuit on or off.
| 電力機器の起動・停止のために、電力回路を開閉する電力機器。

buildingSMART Data Dictionary

PSD-XML

- ContactorType
  P_ENUMERATEDVALUE / IfcLabel / PEnum_ContactorType: CAPACITORSWITCHING, LOWCURRENT, MAGNETICLATCHING, MECHANICALLATCHING, MODULAR, REVERSING, STANDARD, OTHER, NOTKNOWN, UNSET

  | ContactorType: A list of the available types of contactor from which that required may be selected where: CapacitorSwitching: for switching 3 phase single or multi-step capacitor banks. LowCurrent: requires the use of low resistance contacts. MagneticLatching: enables the contactor to remain in the on position when the coil is no longer energized. MechanicalLatching: requires that the contactor is mechanically retained in the on position. Modular: are totally enclosed and self contained. Reversing: has a double set of contactors that are prewired. Standard: is a generic device that controls the flow of power in a circuit on or off.
  | 接触器タイプ: 以下より選択が必要となる、接触器の一覧リスト： コンデンサスイッチ：3つのシングルフェーズまたは複数のコンデンサバンクで切り替える。 低流：低い抵抗接触の使用が必要 マグネット式：コイルのエネルギーが無くなった時に切替をONポジションにして有効にする MechanicalLatching：切替器がONポジションを維持するために機械的な仕組みが必要。 モジュール式：閉鎖されている自働型切替器。 リバース：2つの切替器をワイヤーで接続したもの。 標準：回路で電力潮流をオンまたはオフでコントロールする一般的な装置。
  | 접촉기 유형: 다음에서 선택이 필요하다, 접촉기 목록 : 콘덴서 스위치 : 3 개의 단일 위상 이상의 커패시터 뱅크를 전환합니다. 낮은여 : 낮은 저항 접촉 사용해야 마그네틱 : 코일의 에너지가 분실된 때 전환을 ON 위치로하여 사용 MechanicalLatching : 판을 ON 위치를 유지하기 위해 기계적인 구조가 필요합니다. 모듈형 : 폐쇄되어있는 자신 동형 판. 리버스 : 두 판을 와이어로 연결한 것. 표준 : 회로에서 전력 조류를 켜지거나 꺼지지 컨트롤하는 일반적인 장치

Link to this page