#### 7.1.4.28 Pset_SensorTypeHeatSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / HEATSENSOR

| A device that senses or detects heat. HISTORY: In IFC4, incorporates Fire Sensor. HeatSensorSetPoint changed to SetPointTemperature
| 熱を感知または検出するデバイス。

buildingSMART Data Dictionary

PSD-XML

- CoverageArea
  P_SINGLEVALUE / IfcAreaMeasure

  | CoverageArea: The area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).
  | 測定範囲: センサでカバーされている範囲。(通常、センターがセンサの位置にある円として測定される)
  | 측정 범위: 센서 커버하는 범위. (일반적으로 센터 센서의 위치에있는 원형으로 측정되는)

- SetPointTemperature
  P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

  | SetPointTemperature: The temperature value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
  | 温度設定値: 感知される温度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。
  | 온도 설정: 감지되는 온도. 세트 포인트 값을 넣으려면, IfcPropertyBoundedValue.SetPointValue를 사용하십시오.

- RateOfTemperatureRise
  P_SINGLEVALUE / IfcTemperatureRateOfChangeMeasure

  | RateOfTemperatureRise: The rate of temperature rise that is to be sensed as being hazardous.
  | 温度上昇率: 危険であるとして感じられることになっている温度上昇率。
  | 온도 상승률: 위험 것으로 느껴지게하는 온도 상승률.

Link to this page