

**INSTALLATION INSTRUCTIONS**

**Bottom Rail for Hi-Point 1095TS, 3895TS, 995TS, 4095TS, & 4595TS**

**Hardware included: 8-32 x ¾ cap screws (2), Hex key for 8-32**

**Note: Our Picatinny bottom rails mount directly to the bottom cut-out/channeled area of the plastic fore-end and install using the existing factory screws. If you no longer have your factory screws, we have included screws for you. It is easier to identify certain parts during the installation if you have the Hi-Point Owner’s Manual open to the pages showing the gun assembly diagrams. If you no longer have the original manual, it can be downloaded and/or viewed directly on the Hi-Point website. It is important that you save all original parts in case you wish to restore back to factory style. Before starting the installation, please fully read these instructions to be sure that you have a good understanding of the installation procedures. If you are still unsure about installation procedure, call us at 973-786-4004.**

**1. Always begin any installation by first removing the clip/magazine, then making sure that the chamber is empty, and your gun is completely unloaded.**

**2. On the bottom mount area of the plastic stock fore-end of the gun, you are going to replace the factory plastic rail with your new LongShot rail using the two existing factory screws. If you no longer have your factory screws, we have included screws for you.**

**3. Firmly push the new rail into place with its back side channeled rib pressed into the slotted mounting area.**

**4. Reinstall the two mounting screws and tighten. Take care not to overtighten.**

**5. Make sure that your new rail is fully pressed into the plastic groove and is properly seated onto the stock.**