

Installation of **Aluminum 3.850” Picatinny Top, Side & Bottom Rails**

for **Chiappa LITTLE BADGER**

Always, always, always…read the instruction in full BEFORE starting the installation so as to be sure that you have a good understanding of the assembly process.

**Hardware Included:** 3mm x 6mm screws ( x3 per rail purchase), 5/64 Hex Key

NOTE: Although it is not necessary, it is easier to ID certain parts during the installation if you have the Original Owners Manual open to the pages showing the gun assembly diagrams.

TO INSTALL:

1. **ALWAYS** CHECK THE CHAMBER AND BEGIN ANY INSTALLATION WITH THE GUN COMPLETELY UNLOADED!
2. USING THE SUPPLIED HEX KEY OR OTHER PROPER SPLINED BIT, UNSCREW THE 3 SCREWS THAT SECURE THE PLASTIC RAIL TO THE GUN AND REMOVE RAIL.
3. POSITION NEW ALUMINUM RAIL SO THE SCREW HOLES LINE UP PROPERLY, INSERT THE 3 SUPPLIED SCREWS LOOSELY AND MAKE SURE THAT ALL SCREWS ARE THREADED INTO ALL HOLES BEFORE TIGHTENING, AND THEN TIGHTEN EACH TO SECURE. **NOTE:** DO NOT OVERTIGHTEN OR DAMAGE TO THREADED HOLES COULD OCCUR.
4. THAT’S IT, YOU’RE DONE. WE SUGGEST THAT YOU SAVE ALL REMOVED PARTS IN CASE YOU WISH TO RETURN GUN TO ORIGINAL FACTORY SET UP.

Got questions?.. or are uncertain of the installation process, please call us at 973-786-4004 and we can guide you over the phone.